	Activity to be Assessed
	Assessment Number

	CONCRETE FLOOR SLAB INSTALLATION
	002

	Persons undertaking or affected by the activity

	

	
	X
	Employees
	X
	Contractor
	X
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	COLLAPSE OF FORMWORK 
	2
	3
	6

	2
	MANUAL HANDLING OF SHUTTERS, REINFORCEMENT BARS ETC. 
	3
	3
	9

	3
	DUST FROM SCABBLING OPERATIONS
	3
	4
	12

	4
	CEMENT BURNS FROM WET CONCRETE
	3
	3
	9

	5
	OPERATIVES FALLING DURING ERECTION OF FORMWORK
	3
	4
	12

	6
	ARM AND BACK STRAIN
	3
	3
	9

	Existing Control Measures / Additional Control Measures Required

	1
	FOREMAN TO CHECK FALSEWORK PRIOR TO WORK COMMENCING TO ENSURE IT IS ERECTED IN A PROPER MANNER AND THAT CLAMPS ARE FITTED CORRECTLY.

	2
	TOOLBOX TALKS AND MANUAL HANDLING TRAINING TO ENSURE OPERATIVES ARE COMPETENT WITH SAFE LIFTING TECHNIQUES

	3
	KEEP AREAS OF WORK CLEAR OF MATERIALS, TOOLS AND THE LIKE

	4
	APPROPRIATE PPE TO BE WORN BY ALL OPERATIVES WORKING IN OR CLOSE TO WORKS.

	5
	

	6
	

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	COLLAPSE OF FORMWORK 
	1
	3
	3

	2
	MANUAL HANDLING OF SHUTTERS, REINFORCEMENT BARS ETC. 
	2
	3
	6

	3
	DUST FROM SCABBLING OPERATIONS
	1
	4
	4

	4
	CEMENT BURNS FROM WET CONCRETE
	2
	3
	5

	5
	OPERATIVES FALLING DURING ERECTION OF FORMWORK
	1
	4
	4

	6
	ARM AND BACK STRAIN
	2
	3
	19

	Name  OWEN TOWEL
Position  MD
	Signed
OWEN TOWEL

	   Date of Completion: 
06/04/2020

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury

	Reviewed by:
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk



METHOD STATEMENT:
1. Prior to work commencing, the excavation will be inspected to ensure ground conditions are suitable.
2. Prior to work commencing a pre-assessment of the formwork is to be undertaken by the Site Manager to ensure erected in a proper manner 
3. All excavations are to be isolated from unauthorised personnel (where necessary) both during working hours and at night time by appropriate barrier & covering
4. Ensure all operatives are wearing the correct PPE to protect them from cement burns, dust etc. 
5. Concrete to be delivered to the site by adhering to the traffic management plan
6. Operatives must not access any area of excavation which is not ‘battered back’ or supported.
7. Undertake an accurate drawing of completed works for inclusion in the Client Health and Safety file.
8. Steel reinforcement to be fixed into position by trained and competent operatives
9. Concrete to be poured into excavation via pump, ensuring that all connections are tight.
10. Tamp finish. 

