show running-config
Building configuration...

Current configuration : 3234 bytes
version 12.2(37)SE1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
hostname DLS1
enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1

ip dhcp excluded-address 172.16.10.251 172.16.10.254
ip dhcp pool dls1
network 172.16.10.0 255.255.255.0
default-router 172.16.10.1
dns-server 8.8.8.8
clock timezone UTC 0
spanning-tree mode pvst
spanning-tree vlan 1,12,434,800,1010,1111,3456 priority 24576
spanning-tree vlan 123,234 priority 28672

interface Loopback0
ip address 1.1.1.1 255.255.255.255
!
interface Port-channel1
switchport trunk encapsulation dot1q
switchport mode trunk

interface Port-channel12

interface FastEthernet0/1
shutdown

interface FastEthernet0/2
shutdown

interface FastEthernet0/3
shutdown

interface FastEthernet0/4
shutdown

interface FastEthernet0/5
switchport access vlan 1111
switchport mode access
switchport nonegotiate
shutdown

interface FastEthernet0/6
switchport access vlan 3456
switchport mode access
switchport nonegotiate
shutdown
interface FastEthernet0/7
switchport trunk native vlan 800
switchport trunk encapsulation dot1q
switchport mode trunk
channel-group 1 mode active

interface FastEthernet0/8
switchport trunk native vlan 800
switchport trunk encapsulation dot1q
switchport mode trunk
channel-group 1 mode active

interface FastEthernet0/9
switchport trunk native vlan 800
switchport trunk encapsulation dot1q
switchport mode trunk

interface FastEthernet0/10
switchport trunk native vlan 800
switchport trunk encapsulation dot1q
switchport mode trunk

interface FastEthernet0/11
switchport trunk encapsulation dot1q
switchport mode trunk
channel-group 12 mode passive

interface FastEthernet0/12
switchport trunk encapsulation dot1q
switchport mode trunk
channel-group 12 mode passive
shutdown

interface FastEthernet0/13
shutdown

interface FastEthernet0/14
shutdown

interface FastEthernet0/15
switchport access vlan 1111
switchport mode access
switchport nonegotiate
shutdown

interface FastEthernet0/16
shutdown
!
interface FastEthernet0/17
shutdown
!
interface FastEthernet0/18
shutdown
!
interface FastEthernet0/19
shutdown
!
interface FastEthernet0/20
shutdown
interface FastEthernet0/21
shutdown
!
interface FastEthernet0/22
shutdown
!
interface FastEthernet0/23
shutdown
!
interface FastEthernet0/24
shutdown
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
no ip address
shutdown
!
interface Vlan12
mac-address 00d0.d3d3.3101
ip address 172.16.10.2 255.255.255.0
!
interface Vlan123
mac-address 00d0.d3d3.3102
ip address 172.16.123.1 255.255.255.0
!
interface Vlan234
mac-address 00d0.d3d3.3103
ip address 172.16.234.1 255.255.255.0
!
interface Vlan1010
mac-address 00d0.d3d3.3104
ip address 172.10.123.1 255.255.255.0
!
interface Vlan1111
mac-address 00d0.d3d3.3105
ip address 172.16.11.1 255.255.255.0
!
interface Vlan3456
mac-address 00d0.d3d3.3106
ip address 172.10.56.1 255.255.255.0
!
ip classless
!
ip flow-export version 9

line con 0
!
line aux 0
!
line vty 0 4
interface FastEthernet0/21
shutdown
!
interface FastEthernet0/22
shutdown
!
interface FastEthernet0/23
shutdown
!
interface FastEthernet0/24
shutdown
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
no ip address
shutdown
!
interface Vlan12
mac-address 00d0.d3d3.3101
ip address 172.16.10.2 255.255.255.0
!
interface Vlan123
mac-address 00d0.d3d3.3102
ip address 172.16.123.1 255.255.255.0
!
interface Vlan234
mac-address 00d0.d3d3.3103
ip address 172.16.234.1 255.255.255.0
!
interface Vlan1010
mac-address 00d0.d3d3.3104
ip address 172.10.123.1 255.255.255.0
!
interface Vlan1111
mac-address 00d0.d3d3.3105
ip address 172.16.11.1 255.255.255.0
!
interface Vlan3456
mac-address 00d0.d3d3.3106
ip address 172.10.56.1 255.255.255.0
!
ip classless
!
ip flow-export version 9

line con 0
!
line aux 0
!
line vty 0 4

















Show IP Interface Brief
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Show VLAN Brief
[image: Table

Description automatically generated]





	













Show VTP Status
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Show etherchannel summary
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Show spanning-tree Summary
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Show standby brief
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DLS1#sh vep status

VTP Version capable S1ee2
VTP version running 2

VTP Domain Name Saac

VTP Pruning Mode Disabled

VTP Traps Generation Dizanled
Devics 10 © 0001 e487.2000

Configuravion last modified by 0.0.0.0 ac 3-1-53 01:0€:17
Local updater ID is 172.16.10.2 on inverface V112 (lowest numbered VIAN interface found)

Feavuze VLAN :

VTP Operaving Mode Server
Maximm VIANS supported locally : 1005

Number of exisving VLANS 12

Configuravion Revision D
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DLS1#show etherchannel summary
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DLS1$Sh spanning-tree summary
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DLS1#sh standby brief
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