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Lab - Building an Ethernet Crossover Cable

Lab – Understanding Ethernet Cable Standards 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection: 
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
A Short Report on Cat 5 & 6 Ethernet Cable Standards
Abstract
This small report will contain information on both variations of CAT 5 & 6 cables and their broadband and data transmission capability, and cable design. Included are CAT5, CAT5e, CAT6, and CAT6a cables.
Category 5 Cable (CAT5)
Category 5 cables are primarily used when transmitting data through Ethernet networks, performing at a maximum of 100 Megahertz (MHz) and 10 – 100 Megabits per second (Mbps) as the standard. CAT5 uses a pair of unshielded twisted pairs (UTP) as its design, however the cable in question is now largely obsolete. [1]
Category 5e Cable (CAT5e)
The ‘Enhanced’ Category 5 Cables are improved for the use of Gigabit Ethernet to now support a higher data transmission rate of 1,000Mbps / 1Gbps, as well as a higher bandwidth capacity at 350Mhz while retaining its 100Mhz standard. On top of these improvements, the design also has reduced crosstalk (Disturbance/Interference to neighbouring wires due to electromagnetic signals on poorly insulated cabling) for both Far-End (FEXT) and Near-End (NEXT). These cables are commonly used nowadays. [1]
Category 6 Cable (CAT6)
[bookmark: _GoBack]Category 6 Cables boast even larger performance than the two previous iterations, now capable of a standard Bandwidth of 250MHz up to a maximum of 550MHz. It still however has the same Transmission specs as CAT5e cables at 1Gbps but can possibly achieve 10Gbps at distances of up to 55 meters. [2] Unlike both CAT5 cables, Category 6 are sometimes now somewhat shielded to further prevent crosstalk from occurring. The design to achieve this makes use of either a foil over the twisted wires or a braid screen. CAT6 cables are also required to be backwards compatible with previous generations back to CAT3 and will downgrade its performance to the appropriate CAT jack (CAT6 in a CAT5 jack will perform at CAT5 capability). [1]
Category 6a (CAT6a)
‘Augmented’ Category 6 cables have greatly improved on its predecessor in several ways. It is now much more shielded than before, removing an incredible amount of crosstalk interference. However, as a result it is now less flexible and denser than the CAT6. The CAT6a can now transmit data at a rate of 10Gbps as standard at 100 meters to accommodate for larger organizations, and a standard bandwidth of 500MHz up to 550MHz. A draft was published by the IEEE (Institute of Electrical and Electronics Engineers) back in October 2004 calling for these specifications in the future. [1]
[image: ]
(Fig. 1: Table of CAT Cable performance and protection) [2]
Conclusion
As time goes on, Ethernet cables continue to improve for an also improving computing system. CAT 7 is the most recent edition and also a price to reflect its amazing quality, its performance shows how demanding networking and the internet has become with work within organizations. With CAT 8 on the horizon time will tell how effective it will be transmitting data and its ability to nullify crosstalk.
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Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
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[image: RJ-45 Jack]
Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-
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Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.



Reflection
Which part of making cables did you find the most difficult?
Making sure the correct colours go in the right order and the exposed trim go all the through to be pierced is the most difficult as the cables tend to twirl back into one another, and it’s hard to gauge if the exposed wire is sufficient enough.
Why do you have to learn how to make a cable if you can easily buy pre-made cables?
Premade cables come in short bundles, so learning to make an extremely long one or incredibly short one is beneficial for whatever situation.
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