R1
R1#sh run
Building configuration...

Current configuration : 1433 bytes
!
! Last configuration change at 13:19:35 UTC Thu Dec 12 2019
!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
multilink bundle-name authenticated
!
cts logging verbose
!
!
license udi pid CISCO1941/K9 sn FCZ2125B0FA
!
!
!
redundancy
!
!
!
!
!
!
interface Embedded-Service-Engine0/0
 no ip address
 shutdown
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
!
interface GigabitEthernet0/0.10
 encapsulation dot1Q 10
 ip address 192.168.10.1 255.255.255.0
!
interface GigabitEthernet0/0.20
 encapsulation dot1Q 20
 ip address 192.168.20.1 255.255.255.0
!
interface GigabitEthernet0/0.30
 encapsulation dot1Q 30
 ip address 192.168.30.1 255.255.255.0
!
interface GigabitEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface Serial0/0/0
 bandwidth 512
 ip address 1.1.1.2 255.255.255.252
!
interface Serial0/0/1
 no ip address
 shutdown
 clock rate 2000000
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
control-plane
!
!
!
line con 0
line aux 0
line 2
 no activation-character
 no exec
 transport preferred none
 transport output pad telnet rlogin lapb-ta mop udptn v120 ssh
 stopbits 1
line vty 0 4
 login
 transport input none
!
scheduler allocate 20000 1000
!
End
R1#SH IP INT BRIEF
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES unset  administratively down down
GigabitEthernet0/0         unassigned      YES unset  up                    up
GigabitEthernet0/0.10      192.168.10.1    YES manual up                    up
GigabitEthernet0/0.20      192.168.20.1    YES manual up                    up
GigabitEthernet0/0.30      192.168.30.1    YES manual up                    up
GigabitEthernet0/1         unassigned      YES unset  administratively down down
Serial0/0/0                1.1.1.2         YES manual up                    up
Serial0/0/1                unassigned      YES unset  administratively down down

R1#sh ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route, H - NHRP, l - LISP
       a - application route
       + - replicated route, % - next hop override

Gateway of last resort is not set

      1.0.0.0/8 is variably subnetted, 2 subnets, 2 masks
C        1.1.1.0/30 is directly connected, Serial0/0/0
L        1.1.1.2/32 is directly connected, Serial0/0/0
      192.168.10.0/24 is variably subnetted, 2 subnets, 2 masks
C        192.168.10.0/24 is directly connected, GigabitEthernet0/0.10
L        192.168.10.1/32 is directly connected, GigabitEthernet0/0.10
      192.168.20.0/24 is variably subnetted, 2 subnets, 2 masks
C        192.168.20.0/24 is directly connected, GigabitEthernet0/0.20
L        192.168.20.1/32 is directly connected, GigabitEthernet0/0.20
      192.168.30.0/24 is variably subnetted, 2 subnets, 2 masks
C        192.168.30.0/24 is directly connected, GigabitEthernet0/0.30
L        192.168.30.1/32 is directly connected, GigabitEthernet0/0.30

R1#sh vtp status
VTP Version                     : 2
Configuration Revision          : 0
Maximum VLANs supported locally : 20
Number of existing VLANs        : 5
VTP Operating Mode              : Server
VTP Domain Name                 :
VTP Pruning Mode                : Disabled
VTP V2 Mode                     : Disabled
VTP Traps Generation            : Disabled
MD5 digest                      : 0xBF 0x86 0x94 0x45 0xFC 0xDF 0xB5 0x70
Configuration last modified by 0.0.0.0 at 0-0-00 00:00:00
Local updater ID is 192.168.10.1 on interface Gi0/0.10 (first interface found)
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