Router

R1>en
Password:
R1#show run
Building configuration...


Current configuration : 3537 bytes
!
! Last configuration change at 21:20:17 UTC Mon Aug 5 2013
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$5lXR$6gs7R2sQd262AqhQ9rF90.
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-4076402168
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-4076402168
 revocation-check none
 rsakeypair TP-self-signed-4076402168
!
!
crypto pki certificate chain TP-self-signed-4076402168
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 34303736 34303231 3638301E 170D3133 30383035 32303537
  31395A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D34 30373634
  30323136 38308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100B39B 8A0C82CE A280E202 8463C4C1 1A6CD2EC 46734924 4FD5AC1E
  CC49386B 7143ACD1 0B4420FA 41B4EDE6 2BB77B3C 92A798BD A148AADC E30B60FE
  5D9E1CF4 05C4CE48 96E22123 8D407A16 23B915A2 C06BB358 C0B2FF6F 5B0AFA37
  E6491010 3D8775D2 6F18F0DC 0EF2EDC8 3F45C7FF 11D5443A 325B7C47 63E3C736
  9EAB0771 50743787 5C8AD302 7072478F 36ECFCBE 1D016962 6C4F66EB 7E79071E
  B47B9C62 EA800187 E99E637A 345398F5 8895C2E8 9A1A34B3 6B1428EB 7BFFC438
  FA4A980D 6816A440 F355254E 824C169B 89379E65 224DFC36 85E469C7 E37AA26C
  5C5B4FA7 01A33B6A 21D4A457 9176EA99 5CA44697 7B51700C ABF6CF3B B49CF427
  2B6A5AC4 71810203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 1472EAA8 68F7FA33 B7FF2247 B051068E 3628F0E2
  E1301D06 03551D0E 04160414 72EAA868 F7FA33B7 FF2247B0 51068E36 28F0E2E1
  300D0609 2A864886 F70D0101 05050003 82010100 86F6F5E6 8E5E3A33 DF3F4F69
  13967FCC 96CB2324 C423BA6F DB4D4458 AE46F7A7 4CF6857C 90F4CE92 4D910613
  F984AD8C 52B6EADE 57A7B871 AE97BD55 9B28CB7C 624117C5 813E1E93 A38469AC
  9129FE8B 17882797 25342EC2 BB7DA9A6 0702CF3F 53C01A24 BC45A189 2D1E831E
  5A52CD4D 0CA735AA E39A81F3 8D0520A7 A2B8BD15 D3EED15A F043BCAD 31467017
  8F66EB95 AE108FFC 850EF4C5 B0ACBA6F 395711C9 321A1759 C084B892 B2F6E72D
  C5F3995B B8077F68 F366D3F0 AC1F302B 82C02AC5 E1298EC4 ED1143A5 84A7980A
  A6F78A3D 35D04968 03AEFCC6 91DF871E 11F036B2 E0513338 E98BC5C1 124D03A0
  3A22F3D7 CF718AAA F02AFF1A 19239B09 C866AB97
        quit
!
license udi pid ISR4221/K9 sn FGL2235928J
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 ip address 172.16.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 172.16.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^Cotd# # "No unauthorized access " #
No unauthorized access ^C
!
line con 0
 transport input none
 stopbits 1
line vty 0 4
 password 7 14141B180F0B
 login
line vty 5 15
 password 7 14141B180F0B
 login
!
!
!
!
!
!
End



Switch 

*Mar  1 03:56:26.100: %SYS-5-CONFIG_I: Configured from console by consoleo run
Building configuration...

Current configuration : 1375 bytes
!
! Last configuration change at 03:56:26 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip http server
ip http secure-server
!
no vstack
banner motd ^Cotd# # " BANNER " #
banner ^C
!
line con 0
line vty 5 15
!
end
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