Rebar spacing
Longitudinal bars: the maximum distance of the following: 
· Maximum nominal diameter
· Maximum aggregate size plus 5 mm
· 20 mm

Minimum vertical distance between groups: the maximum distance of the following:
· Maximum nominal diameter
· 20 mm

Maximum distance between longitudinal bars without any link: 150 mm
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Jail construction: Maximum distance between bars: 250 mm

EXERCISE
Calculate the following rebar distribution (nominal cover 35mm):
1.- A column of 400x400mm with 4Ø20 at each side. Links Ø8
2.- A column of 600x400mm with 3Ø25+4Ø16 at the long side, and 2Ø25+2Ø16 at the small side.
[bookmark: _GoBack]3.- A beam of 400x500mm with 5Ø20 at the bottom and 3Ø12 at the top.
4.- A beam of 400x500mm with 10Ø20 at the bottom and 5Ø16 at the top.
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