Name of the IOS image that the router is running?
Cisco IOS Software, C2900 Software (C2900-UNIVERSALK9-M), Version 15.1(4)M4, RELEASE SOFTWARE (fc2)
Non-volatile random-access memory (NVRAM) does the router have?
255K bytes of non-volatile configuration memory.

How much Flash memory does the router have?
249856K bytes of ATA System CompactFlash 0 (Read/Write)

What is the boot process for the router on the next reload?
	
	Current
	Type
	Next reboot

	ipbase
	ipbasek9
	ipbasek9
	ipbasek9

	security
	Disable
	None
	None

	uc
	Disable
	None
	None

	data
	Disable
	None
	none



How are passwords presented in the output?
Passwords are encrypted so they come in random numbers and letters. 
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What code is used in the routing table to indicate a directly connected
network? 
C code is used to show a directly connected network. 

How many route entries are coded with a C code in the routing table?
2 
What command changed the status of the Gigabit Ethernet ports from
administratively down to up?
No shutdown
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