Assessment 2

1.  
a. Answer – A
b. Answer – B
c. Answer – A
2. 
a. Answer – 26.5
b. Answer – B
c. Answer – D
d. Answer – B
e. Answer – B
f. Answer – A

Fault Response
[bookmark: _GoBack]High resistance on winding 3


1. Answer – A (PWM)
2. Answer – D (Converting DC into AC)
3. Answer – B (Clocking rate of the microprocessor)
4. Answer -  A (A more positive output voltage)
5. Answer – C (EPROM)
6. Answer -  B (Damage to the power supply)
