R1
R1#sh run
Building configuration...

Current configuration : 1004 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
service password-encryption
security passwords min-length 10
!
hostname R1
!
!
!
enable secret 5 $1$mERr$2kSZR9DN2ofxLllbGij.S1
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15241FFJ-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
ip address 192.168.99.0 255.255.0.0
clock rate 2000000
shutdown
!
interface Serial0/3/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router rip
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
password 7 0822455D0A16061E010803
login
!
line aux 0
!
line vty 0 4
login
!
!
!
End

R2
R2#sh run
Building configuration...

Current configuration : 1008 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
service password-encryption
security passwords min-length 10
!
hostname R2
!
!
!
enable secret 5 $1$mERr$2kSZR9DN2ofxLllbGij.S1
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX152420Z1-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
ip address 192.168.99.0 255.255.0.0
shutdown
!
interface Serial0/3/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^Cuthorized Users Only!
^C
!
!
!
!
!
line con 0
password 7 0822455D0A16061E010803
login
!
line aux 0
!
line vty 0 4
login
!
!
!
End



R3
R3#sh run
Building configuration...

Current configuration : 991 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
service password-encryption
security passwords min-length 10
!
hostname R3
!
!
!
enable secret 5 $1$mERr$2kSZR9DN2ofxLllbGij.S1
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX152444D1-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
ip address 192.168.99.4 255.255.0.0
shutdown
!
interface Serial0/3/1
ip address 172.16.1.0 255.255.0.0
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
password 7 0822455D0A16061E010803
login
!
line aux 0
!
line vty 0 4
login
!
!
!
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