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Switch:
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 153.99.11.10 255.255.255.0
!
ip http server
ip http secure-server
!
no vstack
!
line con 0
line vty 5 15
!
end

IvelinS1#show
IvelinS1#show ru
IvelinS1#show running-config
Building configuration...

Current configuration : 1319 bytes
!
! Last configuration change at 23:12:51 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname IvelinS1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 153.99.11.10 255.255.255.0
!
ip http server
ip http secure-server
!
no vstack
!
line con 0
line vty 5 15
!
end

IvelinS1#

IvelinS1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  153.99.11.10    YES manual up                    down
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  down                  down
FastEthernet0/6        unassigned      YES unset  down                  down
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
IvelinS1#



Router:


ivelinR1>enable
Password:
ivelinR1#show runn
ivelinR1#show running-config
Building configuration...


Current configuration : 3349 bytes
!
! Last configuration change at 13:24:00 UTC Tue Jan 14 2020
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname ivelinR1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$IrbD$gMBCn8H01GpF4przSNYe.1
!
no aaa new-model
!
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1227001095
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1227001095
 revocation-check none
 rsakeypair TP-self-signed-1227001095
!
!
crypto pki certificate chain TP-self-signed-1227001095
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31323237 30303130 3935301E 170D3230 30313134 30383534
  32395A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 32323730
  30313039 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 01008BD4 D7134725 AF62106A D4A1E0ED A5192074 433BC2A8 13A68A1D
  2014D056 D9A1CE8E A37BDE16 8A24D241 633E63C8 10C55FCC 07930205 F4DEEE96
  90BABA8E 46EDE316 1A9EC380 53ED876A 81A86346 4301BE2C B9E48817 C5B9C9B4
  A986364E 353C4FF6 214EE5FC 0269D2D6 2399C9FB 2A6D6100 727C4B81 41439AFD
  EA60B41C D263D1B5 6ACBC2E7 56DF7D5B 3D4EF153 BD554666 F6C307D6 E02EFCF3
  8A633DBB 4940AA2E 65AEFDE8 D38EA360 E4E17F46 FC56351B FCE9D2DF 527BE498
  CCFA8FA4 AEA8FDC2 4F094F48 DAD932C6 A93A6758 447E9C34 C32D64C2 CE024F19
  EA8A5388 5C53F1C7 8E2B0BE1 B0B606F6 441CDFC7 22194B57 3C04AE10 402C9DC1
  8A3EC85E 0B230203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14557B30 A0B5F91A 4CD8B25A 793A0FC2 1CCA3E6F
  BA301D06 03551D0E 04160414 557B30A0 B5F91A4C D8B25A79 3A0FC21C CA3E6FBA
  300D0609 2A864886 F70D0101 05050003 82010100 505F220E C725D5AF B2D0E675
  30B4E404 94A99704 E6BDD1C1 EC3BBF7F 981BB4F5 0668942C BCE62AC4 9642D4AB
  F7E94387 47CA28F3 6BFD7084 87916950 3CADC3FA 5972542B 85809303 C4CA4885
  10DEE418 86F4F86F 9B72934E F6FF39C0 41D29C74 73C845BD EC4D9848 3FFBB89D
  FB3267AE C28CDEEB 45597FA5 898EB0C3 F5C8C7D1 B5C69D60 38E2C05F 2CD2B124
  02ED8E0A 14AF386A 5FCBB201 8A78E57E E55E1E7A F488C28C CC8E1BE1 B7D54A95
  8328A8D5 483320D6 EC5F880A 4672E781 21D3A8EF 1EB3ECA3 AB2B3081 5CCBC1C9
  69C58F2E AA8BB33A 0E11545A D34A8B2D 648B946E 0BBC2EC9 A97691B2 AB64B912
  1B29DE3D 237F9C58 AF70D133 C1AC70FE 6D178A38
        quit
!
license udi pid ISR4221/K9 sn FGL224190DV
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 153.99.10.1 255.255.255.0
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
!
line con 0
 transport input none
 stopbits 1
line vty 0 4
 login
!
!
!
!
!
!
end

ivelinR1#
ivelinR1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   153.99.10.1     YES manual administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
ivelinR1#
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‘ommand Prompt

C: \Users\Admin>ipconfig /all

[@Biindous 1P Configuration

Host Name . .
Primary Dns Suffix
Node Type . . . .

TP Routing Enabled.
WINS Proxy Enabled.

Ethernet adapter Ethernet

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. oy
Autoconfiguration Enabled .
Link-local IPv6 Address .
TPva Address.

Subnet Mask

Default Gateway .

DHCPYV6 TATD .

DHCPV6 Client DUTD.

DNS Servers .

NetBIOS over Tcpip.

c: \users\admin>

English (United Kingdor)

Exam - Word

Intel(R) Ethernet Connection (2) 1219-LM
C-9D-92-BF-B9-88

No

Yes

e80: :40b6: afc:547b: 61ef%4(Preferred)
153.99.10.254(Preferred)

255.255.255.6

153.99.16.1

161490066
60-61-60-61-25-60-2E - 6E-0C-9D-92-BF -89-88
Fece:0:0: FFFF::1%1

fece:0:0: FFFF::2%1

fece:0:0: FFFF::3%1

Enabled
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‘ommand Prompt

C: \Users\Admin>ipconfig/all
indows TP Configuration

Host Name . .
Primary Dns Suffix
Node Type . . . .

TP Routing Enabled.
WINS Proxy Enabled.

Ethernet adapter Ethernet

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. oy
Autoconfiguration Enabled .
Link-local IPv6 Address .
TPva Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD .

DHCPV6 Client DUTD.

DNS Servers .

NetBIOS over Tcpip.

C:\Users\Admin>

m

LN265
Hybrid

No

Intel(R) Ethernet Connection (2) 1219-LM
C-9D-92-8F-88-8D

No

Yes

e80: :81b3: CC56:5b22: F684%7 (Preferred)
153.99.11.254(Preferred)

255.255.255.6

153.99.11.1

161490066
60-61-60-61-25-66-28-62-6C-9D-92-BF -B8-BD
Fece:0:0: FFFF::1%1

fece:0:0: FFFF::2%1

fece:0:0: FFFF::3%1

Enabled
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Command Prompt

. [S-inc statistics for 153.99.16.
 Format Painter Packets: Sent = 4, Received = 4, @ (6% loss),

Clipboara 5
& c: \Users\Admin>ping 153.99.11.254

pinging 153.99.11.254 with 32 bytes of data
Reply from 153.99.11.254: bytes=32 time<ims
Reply from 153.99.11.254;

Reply from 153.99.11.254: bytes=32 time<ims
Reply from 153.99.11.254: bytes=32 time<ims

ping statistics for 153.99.11.254
Packets: Sent - 4, Received = 4, Lost = @ (e% loss),
Approximate round trip times in milli-seconds
Minimum = ems, Maximum = @ms, Average = ems
[c: \Users\Adnin>ping 153.99.11.254

pinging 153.99.11.254 with 32 bytes of data

Reply from 153.99.11.254: bytes=32 time<ims
Reply from 153.99.11.254: bytes=32 time<ims
Reply from 153.99.11.254: bytes=32 time<ims
Reply from 153.99.11.254: bytes=32 time<ims

ping statistics for 153.99.11.254
Packets: Sent = 4, Received = 4, Lost = @ (6% loss),
Approximate round trip times in milli-seconds
Minimum = ems, Maximum = @ms, Average = ems

c: \users\admin>
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