Sarah Rule
1810755 – 1810755@student.uwtsd.ac.uk
Lab 3: Design and Configure and IPv4 Network
Part 1 – Fill the Tables with appropriate information/details. 

	Subnet as per the Requirement

	Specification 
	Network: A
	Network: B
	Network: C

	Network Address
	192.168.100.0
	192.168.100.96
	192.168.100.64

	Subnet Mask
	255.255.255.192
	255.255.255.252
	255.255.255.224

	No. of asked hosts/subnets
	50
	2
	20

	No. of usable hosts/subnets
	62
	2
	30

	First Usable Host (FUH)
	192.168.100.1
	192.168.100.97
	192.168.100.65

	Last Usable Host (LUH) 
	192.168.100.62
	192.168.100.98
	192.168.100.94

	Broadcast Address
	192.168.100.63
	192.168.100.99
	192.168.100.95


 

	Addressing Table

	Device
	Requirement
	IP Address
	Subnet Mask
	Gateway

	PC 1
	1st Usable Host Network: A
	192.168.100.1
	255.255.255.192
	192.168.100.62

	Laptop 1
	2nd Usable Host Network: A
	192.168.100.2
	255.255.255.192
	192.168.100.62

	PC 2
	1st Usable Host Network: B
	192.168.100.97
	255.255.255.252
	192.168.100.99

	PC 3
	1st Usable Host Network: C
	192.168.100.65
	255.255.255.224
	192.168.100.95

	Laptop 0
	2nd Usable Host Network: C
	192.168.100.66
	255.255.255.224
	192.168.100.95

	RAI G0/0/0
	Last Usable Host Network: A
	192.168.100.62
	255.255.255.192
	N/A

	RIBC G0/0/1
	Last Usable Host Network: B
	192.168.100.98
	255.255.255.252
	N/A

	RIBC G0/0/0
	Last Usable Host Network: C
	192.168.100.94
	255.255.255.224
	N/A




Packet Tracer Question: 
Check the Switches with appropriate command to find Old VLan Database is deleted
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Subnet as per the Requirement  

Specification   Network: A  Network: B  Network: C  

Network Address  192.168.100.0  192.168.100.96  192.168.100.64  

Subnet Mask  255.255.255.192  255.255.255.252  255.255.255.224  

No. of asked  hosts/subnets  50  2  20  

No. of usable  hosts/subnets  62  2  30  

First Usable Host (FUH)  192.168.100.1  192.168.100.97  192.168.100.65  

Last Usable Host (LUH)   192.168.100.62  192.168.100.98  192.168.100.94  

Broadcast Address  192.168.100.63  192.168.100.99  192.168.100.95  

     

Addressing Table  

Device  Requirement  IP Address  Subnet Mask  Gateway  

PC 1  1 st   Usable Host  Network: A  192.168.100.1  255.255.255.192  192.168.100.62  

Laptop 1  2 nd   Usable Host  Network: A  192.168.100.2  255.255.255.192  192.168.100.62  

PC 2  1 st   Usable Host  Network: B  192.168.100.97  255.255.255.252  192.168.100.99  

PC 3  1 st   Usable Host  Network: C  192.168.100.65  255.255.255.224  192.168.100.95  

Laptop 0  2 nd   Usable Host  Network: C  192.168.100.66  255.255.255.224  192.168.100.95  

RAI G0/0/0  Last Usable Host  Network: A  192.168.100.62  255.255.255.192  N/A  

RIBC G0/0/1  Last Usable Host  Network: B  192.168.100.98  255.255.255.252  N/A  

RIBC G0/0/0  Last Usable Host  Network: C  192.168.100.94  255.255.255.224  N/A  

    Packet  Tracer Ques tion :    Check the S witches with appropriate command to  find  Old VL an Database is deleted   Show Flash   

