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	Unique Identifier for the
	
	
	

	
	
	
	
	
	

	Manufacturer OUI
	
	Interface
	
	Vendor Name
	

	
	
	
	
	
	

	60-E3-27-C1-2B-12
	60:E3:27 
	
	Tp-Link Technologies Co.,Ltd.
	

	
	
	
	
	
	

	FC-AA-14-AC-C3-1F
	
	FC:AA
	
	:14 Giga-Byte Technology Co.,Ltd.
	

	
	
	
	
	
	



[image: ] I’m using ethernet connection. I couldn’t do step 12 and 13 because I don’t have wireless connection.
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Due to the fact I don’t have wi-fi I did not do step 12-25. 
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image7.png
Time. Source Destination
2034.773.792790  Giga-Byt_acic3:1f  ARRISGro_2c:f7:ds
2037..774.689177  AmazonTe 0c:17:61  Broadcast
2033 775.102145  SamsungE_cl:6f:47  Broadcast
2045..777.149262  SamsungE_cl:6f:47  Broadcast
2045 777158410 AmazonTe 0c:17:61  Broadcast
2049.. 775.168961  AmazonTe 0c:17:61  Broadcast
2052.779.169101  AmazonTe 0c:17:61  Broadcast
2052. 779176316 SamsungE_cl:6f:47  Broadcast
2057.. 780719006 AmazonTe 0c:17:61  Broadcast
2059.. 781.197180  SamsungE_cl:6f:47  Broadcast
2060.. 751.699045  AmazonTe 0c:17:61  Broadcast
2064.. 752.698633  AmazonTe 0c:17:61  Broadcast
2065.. 783.225516  SamsungE_cl:6f:47  Broadcast
2069.. 784.619073  AmazonTe 0c:17:61  Broadcast
2071 785.237207  SamsungE_cl:6f:47  Broadcast
2072.. 785.557504  AmazonTe 0c:17:61  Broadcast

Length Info
42 192.165.0.11 is at fc:aa £
60 Who has 192.168.0.1? Tell 192.165.0.43
60 Who has 192.165.0.1? Tell 192.165.0.37
60 Who has 192.165.0.1? Tell 192.165.0.37
60 Who has 192.165.0.1? Tell 192.165.0.43
60 kho has 192.165.0.1? Tell 192.165.0.43
60 kho has 192.165.0.1? Tell 192.165.0.43
60 kho has 192.165.0.1? Tell 192.165.0.37
60 Who has 192.165.0.1? Tell 192.165.0.43
60 kho has 192.165.0.1? Tell 192.168.0.37
60 Who has 192.165.0.1? Tell 192.165.0.43
60 kho has 192.165.0.1? Tell 192.165.0.43
60 Who has 192.165.0.1? Tell 192.165.0.37
60 Who has 192.165.0.1? Tell 192.165.0.43
60 Who has 192.165.0.1? Tell 192.165.0.37
60 Who has 192.165.0.1? Tell 192.165.0.43

EEEEEEEEEEEEEEEE%

> Frame 205743: 60 bytes on wire (480 bits), 60 bytes captured (480 bits) on interface \Device\NPF_{40FOE7E4-ODBD-4D3C-8284-03D3AE14248F}, id 6
~ Ethernet II, Src: AmazonTe_6c:17:61 (14: 61), Dst: Broadcast (f: FF1FF)
> Destination: Broadcast (FF:ff:ff:ff:ffiff)
> Source: AmazonTe_@c:17:61 (14:91:38:0c:17:61)
Type: ARP (ex2306)
Padding: 0000000000000000000000000000577dd574
> Address Resolution Protocol (request)

oo FF FF £F £f £f £f 14 91 38 0c 17 61 08 06 00 0L
0010 05 0 06 04 00 01 14 91 38 Oc 17 61 c@ a5 00 2b
2020 00 00 00 00 00 00 co a5 00 01

P00 00 00 00 00 00 00 00
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Pinging 192.168.0.11 with 32 bytes of data:
Reply from 192.168.0.11: bytes=32 time<ims
Reply from 192.168.0.11: bytes=32 time<ims
Reply from 192.168.0.11: bytes=32 time<ims
Reply from 192.168.0.11: bytes=32 time<ims

ping statistics for 192.168.6.11
Packets: Sent = 4, Received = 4, Lost = @ (8% loss),
Approximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms
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Frame 205743: 60 bytes on wire (480 bits), 60 bytes captured (480 bits) on interface \Device\NPF_{40FQE7E4-9DED-4D3C-5284-03D3AE14248F}, id ©

v Ethernet II, Src: AmazonTe 6 1 (14:91:38; 1), Dst: Broadcast (FF:ff: )
Destination: Broadcast (FFiffiffiffiffiff)
Source: AmazonTe_Bc:17:61 (14:91:38:0c:17:61)
Type: ARP (ex2306)
Padding: 0000000000000000000000000000577dd574

v Address Resolution Protocol (request)
Hardware type: Ethernet (1)
Protocol type: IPv4 (@x800)
Hardware size: 6
Protocol size: 4
Opcode: request (1)
Sender MAC address: AmazonTe_o
Sender Ip address: 192.168.0.43
Target MAC address: 00:00:00_00:
Target IP address: 192.165.0.1

1 (14:91:38:0¢

00 (00:00:00:00:
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pinging 192.168.6.11 with 32 bytes of data:
IReply from 192.168.6.11: bytes=32 time<ims
[Reply from 192.168.6.11: bytes=32 time<ims TTL-128
Reply from 192.168.6.11: bytes=32 time<ims TTL-128
Reply from 192.168.6.11: bytes=32 time<ims TTL-128

ping statistics for 192.168.6.1°
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
pproximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

:\Users\Kristen19995arp -a

nterface: 192.168.6.11 --- 6x9
Internet Address Physical Address Type
192.168.6.1 18-35-d1-2c-7-d8  dynamic
192.168.0.37 84-24-66-C1-6f-47  dynamic
192.168.0.43 14-91-38-6c-17-61  dynamic
192.168.0.44 F6-f0-ad-es-ef-bd  dynamic
192.168.0.255 FE-FE-FE-FE-FF-FF static
224.0.6.7 01-00-50-00-00-67  static
224.0.6.22 01-00-50-00-00-16  static
224.0.6.251 01-00-5-00-00-fb  static
224.0.6.252 01-00-5-00-00-fc static
224.0.1.187 01-00-5e-00-01-bb  static
239.255.255.250 01-00-5e-7f-ff-fa  static
255.255.255.255 FE-FE-FE-FE-FE-FF static

: \Users\Kristen1999>
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eth_addr
if_addr

Example:

> arp -s 157.55.85.212  00-3a-00-62-C6-09

> arp -a

Displays current ARP entries by interrogating the current
protocol data. If inet_addr is specified, the Ip and Physical
addresses for only the specified computer are displayed. If
more than one network interface uses ARP, entries for each ARP
table are displayed.

same as -a.

Displays current ARP entries in verbose mode. All invalid
entries and entries on the loop-back interface will be shown.
Specifies an internet address.

Displays the ARP entries for the network interface specified
by if_addr.

Deletes the host specified by inet_addr. inet_addr may be
wildcarded with * to delete all hosts.

Adds the host and associates the Internet address inet_addr
with the Physical address eth_addr. The Physical address is
given as 6 hexadecimal bytes separated by hyphens. The entry
is permanent.

Specifies a physical address.

If present, this specifies the Internet address of the
interface whose address translation table should be modified.
If not present, the first applicable interface will be used.

. Adds a static entry.
. Displays the arp table.
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Wireless LAN adapter Local Area Connection* 4:

Media State . . . : Media disconnected
Connection-specific DS Suffix .

Description . . . . . ... ... :Microsoft Wi-Fi Direct Virtual Adapter #3
Physical Address. 22-E3-27-C1-28-12

DHCP Enabled. St Yes

Autoconfiguration Enabled . . . . : Yes

Ethernet adapter Ethernet:

Connection-specific DNS Suffix

Realtek PCIe GBE Family Controller

Description . e
Physical Address. . . . . ... . : FC-AA-14-AC-C3-1F

DHCP Enabled. . Yes

Autoconfiguration Enabled . .t Yes

Link-local IPv6 Address . . . . . : fe89::386f:d75d:bebe:19c5%9(Preferred)
1Pv4 Address. R 192.168.6.11(Preferred)

Subnet Mask . © ... ... .:255.255.255.8

Lease Obtained. . . . . . ... .: @9 October 2620 €8:39:35

Lease Expires . 19 October 2620 €8:39:35

Default Gateway . . . . . . ... : 192.168.6.1

DHCP Server . . . . . ... ...:192.168.6.1

DHCPV6 TAID . . 167553556

DHCPV6 Client DUID. . . . . . . . : 06-01-86-01-1D-F2-B2-6D-FC-AA-14-AC-C3-1F
DNS Servers . . . . . . .. ...: 194.168.4.100

194.168.8.106
NetBIOS over Tcpip. . . . . . . . : Enabled
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Ethernet adapter Ethernet 2:

Media State .

Description .
Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .

Wireless LAN adapter WiFi:

Media State .

Description .
Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .

Media State .
Connection-specific DS Suffix
Description . e
Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .

Connection-specific DNS Suffix

Connection-specific DNS Suffix

: Media disconnected

TAP-ProtonVPN Windows Adapter VO
06-FF-2€-D9-9D-BA
Yes

: Yes

: Media disconnected

Qualcomm Atheros AR9287 Wireless Network Adapter
60-E3-27-C1-28-12
Yes

: Yes
Wireless LAN adapter Local Area Connection* 3:

: Media disconnected

Microsoft Wi-Fi Direct Virtual Adapter #2
12-£3-27-C1-28-12
ves

: Yes
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Network Connection Details

Network Connection Detals:

1Pv4 Subnet Mask
Lease Obtained
Lease Bxpies

P4 Defaui Gateway
1Pv4 DHCP Server
1Pv4 DNS Servers

1Pv4 WINS Server
NetBIOS over Tepip En.
Linklocal IPV6 Address.
1P6 Defaui Gateway
1PY6 DNS Server

Valve.

Reatek PCle GBE Family Contrller

Yes

19216801
255.255.255.0

09 October 2020 08:39:35
19 October 2020 08:39:35
19216801

19216801
1941684100
1941688100

Yes
080:306(75d bebe:195%9
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ireless LAN adapter Local Area Connection* 4:

Media State .

Connection-specific DNS Suffix

Description .
Physical Address.
DHCP Enabled. .
Autoconfiguration Enabled .

Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Lease Obtained.

Lease Expires .

Default Gateway .

DHCP Server .

DHCPY6 TATD .

DHCPV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

:\Users\Kristen1999>

Media disconnected

Microsoft Wi-Fi Direct Virtual Adapter #3

22-£3-27-C1-28-12
ves
ves

Realtek PCIe GBE Family Controller
FC-AA-14-AC-C3-1F
Yes

Yves

Fego: :386f:d75d: beb
192.168.6.11(Preferred)
255.255.255.6

89 October 2026 08:39:35
19 October 2620 8:39:36
192.168.6.1

192.168.0.1

167553556

00-61-00-01-1D-F2-B2-6D-FC-AA-14-AC-C3-1F

194.168.4.100
194.168.8.100

: Enabled

9¢5%9 (Preferred)
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maoe RBIR o= aaam

B

o, Tme S Destnaton ProocdLength 1o
71645 278230675 SamsungE_c1:6F:47  Broadeast e 0 Uho has 192.165.6.17 Tell 192.168.0.37
1875 278.369541 1 sroadcast ol 60 Uho has 192.165.6.17 Tell 152.165.0.43
22126 279. 342656 1 sroadcast s 60 Uho has 192.165.6.17 Tell 152.165.0.43
22372 280.253869  SamsungE_c1:6147  Broadeast s €0 Uho has 192.16.6.17 Tell 152.165..37
2397 280.342705  AmazonTe_6c:17:61  Broadeast s 60 Uho has 192.16.6.17 Tell 152.165.0.43
72684 251.36259  AmazonTe 6c:17:61  Broadeast s 60 Uho has 192.16.6.17 Tell 152.165.0.43
72003 252.266687  Samsung_c1:6147  Broadeast s €0 Uho has 192.16.6.17 Tell 152.165..37
73013 262343239 AmazonTe 6c17:61  Broadeast s 60 Uho has 192.16.6.17 Tell 152.165.0.43
73475 283.342557  AmazonTe 6c17:61  Broadeast s 60 Uho has 192.16.6.17 Tell 152.165.0.43
75712 264.290767  Samsung_c1:6:47  Broadeast s 60 Uho has 192.168.6.17 Tell 152.165..37
74260 286.314703  SamsungE_c1:6147  Broadeast s 60 Uho has 192.165.6.17 Tell 152.165.0.37
28616 287, 354086 1 sroadcast s 60 Uho has 192.165.6.17 Tell 152.165.0.43
24892 255.334694  SamsungE_c1:6147  Broadeast s €0 Uho has 192.16.6.17 Tell 152.165..37
24003 288.357159 1 sroadcast s 60 Uho has 192.16.6.17 Tell 152.165.0.43
75173 289.35392 Coci17:61  Brosdeast s 60 Uho has 192.16.6.17 Tell 152.165.0.43
75450 290.355726  Samsung_c1:6147  Broadeast s €0 Uho has 192.165.6.17 Tell 152.165.6.37




