Task 2
Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	Home Router
	NIC
	192.168.0.1
	255.255.255.0
	192.168.0.1

	PCOne
	NIC
	192.168.0.11
	255.255.255.0
	192.168.0.1

	PCTwo
	NIC
	192.178.0.12
	255.255.255.0
	192.168.0.1

	Server
	NIC
	192.178.0.13
	255.255.255.0
	192.168.0.1

	Laptop
	WMP300N
	192.178.0.14
	255.255.255.0
	192.168.0.1

	Phone
	Wireless
	192.178.0.10
	255.255.255.0
	192.168.0.1

	Printer
	WMP300N
	192.178.0.15
	255.255.255.0
	192.168.0.1

	SwitchOne
	NIC
	192.168.0.2
	255.255.255.0
	192.168.0.1

	SwitchTwo
	NIC
	192.168.0.3
	255.255.255.0
	192.168.0.1



Physical Topology
[image: Diagram

Description automatically generated][image: Graphical user interface, diagram, application

Description automatically generated]

Logical Topology
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Connection Testing
PCOne to Router
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Server to PCOne
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Laptop To Printer
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PCTwo To Phone
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ICommand Prompt

Packet Tracer BC Command Line 1.0
\>ping 192.168.0.10

Pinging 192.168.0.10 with 32 bytes of data:

92.168.0.10:

Reply from 192
92.168.0.10:
2
2

Reply from
Reply from
Reply from

92.168.0.1
92.168.0.10:
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1

Ping statistics for 192.168.0.10:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-second:
Minimum = 10ms, Maximum = 30ms, Average
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ICommand Prompt

Packet Tracer BC Command Line 1.0
\>ping 192.168.0.1

Pinging 192.168.0.1 with 32 bytes of dat

92.168.0.1: timeclms

Reply from 192
92.168.0.1: time=lms
2
2

Reply from
Reply from
Reply from

92.168.0. time<lms
92.168.0.1: time<lms

1
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Ping statistics for 192.168.0.1:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = Oms, Maximm = lms, Average = Oms
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ICommand Prompt

Packet Tracer SERVER Command Line 1.0
\>ping 192.168.0.11

Pinging 192.168.0.11 with 32 bytes of data:

92.168.0.11: timeclms

Reply from 192
92.168.0.11: time<lms
2
2

Reply from
Reply from
Reply from

92.168.0.1. time<lms
92.168.0.11: time<lms

1
1
1
1

Ping statistics for 192.168.0.11:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = Oms, Maximm = Oms, Average = Oms
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ICommand Prompt

Packet Tracer BC Command Line 1.0
>

C:\>ping 192.168.0.15
Pinging 192.168.0.15 with 32 bytes of data:

Reply from 192.168.0.15:
Reply from 192.168.0.15:
Reply from 192.168.0.1!

Reply from 192.168.0.15:

Ping statistics for 192.168.0.15
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-second:
Minimum = léms, Maximum = 32ms, Average = 22ms
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