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SITE FIRE RISK ASSESSMENT
Swansea Uni Accommodation – SA1
The Fire Safety Risk Assessment is for the construction phase of the new building and/or refurbishment works to comply with the Regulatory Reform (Fire Safety) Order 2005.

This document will require updating as the building works progress and becomes more enclosed and other trades join the construction team.
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1. Site Plan
The Fire Assembly Point is situated external to the site boundaries and beyond the proximity to the Main Entrance in the adjacent hard-standing road entrance parking area zone [marked as per Site Layout Plan key]

1.1       
Welfare and Office Accommodation Area Layout
Refer to Appendix 1 Demarked in blue 
1.2

Construction Site Layout
Refer to Appendix 1 Demarked in red (site carpark) 
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2
Fire Hazards and Controls.
2.1
Welfare and Office Accommodation

The welfare and accommodation area consist of temporary portable cabins.

	Hazard
	Risk rating without control
	Controls
	Risk rating with control

	Electricity. Cabins have power supplied to them and canteen and offices have 240v equipment in them.
	High
	Mains power supply to be installed by an NIC EIC approved contractor and an electrical installation certificate to be issued for the works.

All 240v equipment to be PAT tested every 12 months. Register kept of all equipment.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Covering heaters in the drying room with wet clothes.
	High
	Operatives are to be told not to place clothes directly over heaters or to cover them. Sufficient supply of coat hooks and hangers are to be made available. 
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Smoking
	High
	No smoking in any cabin.

Designated smoking area.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low


2.2
Construction site

	Hazard
	Risk rating without control
	Controls
	Risk rating with control

	Storage of fuels.
PETROL
	High
	Petrol to be stored in 5 litre containers in the flammable store.
No more than 20 litres of petrol to be stored at any one time.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Storage of flammable substances other than fuel.
	High
	Substances which are highly flammable to be stored in the flammable safe with a metal barrier between them and any fuels.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Storage of gases
	High
	LPG gas cages. Segregation of gases, cages minimum 3 metres apart. Signage, no smoking, danger.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Re-fuelling
	High
	Follow procedure from JRR Ltd as  attached in Appendix 1.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Hot works – 
Gas torch, Welding, cutting, grinding, etc.
	High
	· Risk assessment & method statements.
· Hot Works Permits.
· 2 no fire extinguishers at point of work at all tines

· Naked flames to be kept away a minimum of 3m from Gas bottles.

· Exclusion zones are to be set up around the work area where lead welding may take place.


	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Smoking
	High
	No smoking on the construction site. Use designated smoking area.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low


	Arson
	High
	Site is secure. Access to site is controlled by security passes.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low

	Waste – 
Wood, cardboard, packaging etc.

Accidental or deliberate ignition. 
	High
	Waste to be removed to covered skips as soon as possible.
All wood to be stacked neatly for personnel to remove from site for recycling.
	High

	
	Medium
	
	Medium

	
	Low
	
	Low


3.
Persons at Risk
	Company
	No. of personnel on site
	Description of main tasks
	Fire hazards
	Risk rating

	IP Construction
	4
	Overseeing project
	Minor items
	LOW


	IP Construction 
	10
	Overall project
	General works on site 
	Medium 

	
	
	
	
	


4.
Instruction, Training and Protecting from Risk

4.1
Site Induction

The site induction will explain the emergency procedure for the site.  It will ensure that all personnel know where the fire bells are situated, the location of all fire extinguishers and the assembly point.

4.2
Fire Extinguishers

The use of fire extinguishers will be constrained to those personnel who have received the relevant training in basic fire fighting equipment use.  Any such training records will be retained in the Health and Safety file.  
4.3
Site Information

The Site Manager will update all new and existing site operatives and trades of any changes from the Fire Risk Assessment which are inherent to the existing Fire Plan and Emergency procedures i.e. the relocation of fire alarm and emergency equipment and apparatus and change in routes etc. 

5.
Permits

5.1
Hot Works

All hot works will require a Hot Works Permit from the Site Manager.

