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	Device 
	Interface 
	IP Address 
	Subnet Mask
	Default Gateway

	PC0
	NIC
	192.168.1.25
	255.255.255.0
	192.168.1.1

	PC1
	NIC
	192.168.1.30
	255.255.255.0
	192.168.1.1

	PC2
	NIC
	192.168.1.35
	255.255.255.0
	192.168.1.1

	PC3
	NIC
	192.168.1.40
	255.255.255.0
	192.168.1.1

	Laptop0
	NIC
	192.168.0.4
	255.255.255.0
	192.168.0.2

	Server0
	NIC
	192.168.1.100
	255.255.255.0
	192.168.1.1

	Switch0
	NIC
	N/A
	N/A
	N/A

	Router0
	NIC
	N/A
	N/A
	N/A

	WirelessRouter0
	NIC
	N/A
	N/A
	N/A
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	Device Names
	Pinged Device
	Was the ping successful?

	192.168.1.25 (PC0)
	192.168.0.4 (Laptop0)
	Yes

	192.168.1.30 (PC1)
	192.168.0.4 (Laptop0)
	Yes

	192.168.1.35 (PC2)
	192.168.0.4 (Laptop0)
	Yes

	192.168.1.40 (PC3)
	192.168.0.4 (Laptop0)
	Yes

	192.168.0.4 (Laptop0)
	192.168.1.25 (PC0)
	Yes

	192.168.1.100 (N14 Main_Server)
	192.168.0.4 (Laptop0)
	Yes




Pinging Laptop0 from PC0[image: ]

















Pinging Laptop0 from PC1[image: ]

















Pinging Laptop0 from PC2
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Pinging Laptop 0 from PC3
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Pinging Laptop0 from PC0
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Pinging Laptop 0 from N14 Main_Server
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The image below shows the logical topology of the network [image: ]
















The image below shows the physical typology of the network [image: ]
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