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Lab - Building an Ethernet Crossover Cable

Lab – Understanding Ethernet Cable Standards 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection: 
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
Lab 3 Report - Ethernet Cables
Jordan Soroko, 1805357, BSc Computing, Computer Architecture & Networks,
Cat 5e and 6 Ethernet cable standards
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Abstract
The objective of this report is to research into and understand ethernet cable standards looking at cat 5e and cat 6.
Introduction
The wiring for the two, will come with four pairs on each end made up of copper. The colours are made up of 4 all green, blue, brown and orange and the second pair having the same colours but also striped in white. They will be put together accordingly next with each colour for example: green & white in slot 1 and following green in slot 2. The slots referred to impose using a standard RJ-45 plug which cat 5e and 6 can use appropriately.
Types of cables
Both cables are the twisted pair type, this is currently one of the most popular styles of cabling still used today even though it is an older method of transferring data. The main reason one would argue as to why it’s still used worldwide is that it is inexpensive to set up connections for a local area network [1]. The reason it’s counterpart fibre optic cabling wouldn’t be used is that the glass fibres with an with a wrapped casing are far more expensive due to the production costs with those materials, even though they provide less EMI interference, higher transmitted data speeds and over longer distances than twisted pair cables with copper. [2]
Twisted Pair Cabling 
Both types can come in either the shielded twisted pair or the opposite unshielded twisted pair.  
The main advantages and disadvantages to bring up are that the STP, with it’s thin layer of added external foil: offer more blockage against electromagnetic interference and allow smoother data flow resulting in higher speed bandwidth, but in turn leave them more fragile and prone to decreased nose cancelation as appose to the standard UTP. [3] UTP is more popular in ethernet cabling as per their affordable price, equipped to deal with noise cancellation better and are “smaller than STP cables, which makes them easier to install”. [3]
Cat 5e and Cat 6
When comparing cat 5e to cat 6 users will find the 5e quality to be lower, not being as best suited towards handling faster transmission speeds in return for its marginally lower cost. [4] 
Category 6 cables will typically have a lower frequency of crosstalk, that is; less interference which doesn’t make signals going through the connection cross over each other from intercepting the wrong signals and becoming confused. [4]
The two are backwards compatible implying that they can work together with previous version categories such as cat 3. [4]
Conclusion
Overall looking at networking standards, a populous could reach the conclusion that cat 6 wiring is the better choice as the bandwidth speed of 250mhz far outweighs the cat 5e more lousy speed of 100mhz even when the prices a not contrasted to a great degree. [4]
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Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
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Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-
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Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
I found that placing the correct wire into each slot according to the diagram was the hardest as it could be easy to mix up a wire into the wrong slot or accidentally leave a space, so the next component was incorrectly placed. Furthermore, it required a greater of test of patience throughout the whole process than previously anticipated by me.
Why do you have to learn how to make a cable if you can easily buy pre-made cables?
I believe it is always a useful piece knowledge knowing how to make ethernet cables not just for your career as that task may come up many times in the I.T field but also at home and for friends you may need to make some. Another advantage of learning to make them manually is that it shortens the length as a longer cable may be an annoyance taking up extra unnecessary space. 
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