



	Site Specific Activity and Control Measures        

                                     (This section must be completed)


	Method
	Conveyed by machine & use of shovels

	
	Location
	General Site area

	
	Duration
	Throughout duration of contract

	
	Control
	Assessment included in RA/MS’s briefing

	Exposure Limits


	0.4 mg/m3 total respirable dust 

5 mg/m3 dust

	Physical Properties
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	Aggregates, cement, quartz (crystalline silica*)

	Hazard
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	Risk of serious damage to eyes

Contact with wet cement or mortar may cause irritation, dermatitis or burns

	
	
	Contact with dry cement powder and sweat or eye fluids may  cause irritation, dermatitis or burns
Possible skin sensitisation from chromates in cement.

Prolonged inhalation (dust) can lead to long term lung damage

	Work Procedures/PPE
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	Wear impervious gloves (BS EN 374 & 388), rubber boots, PVC overalls if working in/on wet concrete

Eye protection (BS EN166 F) if splash or dust likely

Prevent skin contact with wet concrete

Ensure area is well ventilated and dampen down with water during cutting operations. Wear respiratory equipment EN Class FFP3

Restrict public access during mixing, application & until set and during cutting operations.

	First Aid/Fire
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	Ingestion: do not induce vomiting, drink plenty of water in sips, seek medical attention

Eye Contact: irrigate with plenty of water for at least 15 minutes, seek medical attention

Skin Contact: wash with plenty of soap and water immediately, seek medical attention if irritation persists.

Fire: non combustible

	Storage/Disposal
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	Storage: as per manufacturer recommendations

Disposal: designated wash out areas must be impermeable to the surrounding environment.  Allow concrete to solidify before breaking it out and disposing of in accordance with legislative and company requirements

	Environmental
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	Do not allow spillages or wash out to enter mains drains, sewers, boreholes, watercourses etc
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