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!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S1
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
 switchport mode trunk
!
interface FastEthernet0/2
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/3
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/4
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/5
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/6
 switchport access vlan 21
!
interface FastEthernet0/7
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/8
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/9
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/10
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/11
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/12
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/13
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/14
 switchport access vlan 6
!
interface FastEthernet0/15
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/16
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/17
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/18
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/19
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/20
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/21
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/22
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/23
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/24
 switchport access vlan 8
 shutdown
!
interface GigabitEthernet0/1
 switchport mode trunk
!
interface GigabitEthernet0/2
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan5
 mac-address 0030.f27b.ce01
 ip address 192.168.5.1 255.255.255.0
!
interface Vlan6
 mac-address 0030.f27b.ce02
 ip address 192.168.6.1 255.255.255.0
!
interface Vlan7
 mac-address 0030.f27b.ce03
 ip address 192.168.7.1 255.255.255.192
!
interface Vlan8
 mac-address 0030.f27b.ce04
 ip address 192.168.8.1 255.255.255.240
!
interface Vlan9
 mac-address 0030.f27b.ce05
 ip address 192.168.9.1 255.255.255.224
!
ip default-gateway 192.168.1.1
!
!
!
!
line con 0
!
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
end

S2 Running Config
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S2
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
 switchport mode trunk
!
interface FastEthernet0/2
 switchport access vlan 5
 switchport mode access
 shutdown
!
interface FastEthernet0/3
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/4
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/5
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/6
 switchport access vlan 5
!
interface FastEthernet0/7
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/8
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/9
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/10
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/11
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/12
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/13
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/14
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/15
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/16
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/17
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/18
 switchport access vlan 23
!
interface FastEthernet0/19
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/20
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/21
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/22
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/23
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/24
 switchport access vlan 8
 shutdown
!
interface GigabitEthernet0/1
 shutdown
!
interface GigabitEthernet0/2
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan5
 mac-address 00e0.8f60.bd01
 ip address 192.168.5.1 255.255.255.0
!
interface Vlan6
 mac-address 00e0.8f60.bd02
 ip address 192.168.6.1 255.255.255.0
!
interface Vlan7
 mac-address 00e0.8f60.bd03
 ip address 192.168.7.1 255.255.255.192
!
interface Vlan8
 mac-address 00e0.8f60.bd04
 ip address 192.168.8.1 255.255.255.240
!
interface Vlan9
 mac-address 00e0.8f60.bd05
 ip address 192.168.9.1 255.255.255.224
!
ip default-gateway 192.168.1.1
!
!
!
!
line con 0
!
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
end



Branch 1 Running Config
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch1
!
!
!
!
ip dhcp excluded-address 192.168.5.1 192.168.5.10
ip dhcp excluded-address 192.168.6.1 192.168.6.10
ip dhcp excluded-address 192.168.7.1 192.168.7.10
ip dhcp excluded-address 192.168.8.1 192.168.8.10
ip dhcp excluded-address 192.168.9.1 192.168.9.10
!
ip dhcp pool VLAN5
 network 192.168.5.0 255.255.255.0
 default-router 192.168.5.1
 dns-server 209.165.200.25
ip dhcp pool VLAN6
 network 192.168.6.0 255.255.255.0
 default-router 192.168.6.1
 dns-server 209.165.200.25
ip dhcp pool VLAN7
 network 192.168.7.0 255.255.255.0
 default-router 192.168.7.1
 dns-server 209.165.200.25
ip dhcp pool VLAN8
 network 192.168.8.0 255.255.255.0
 default-router 192.168.8.1
 dns-server 209.165.200.25
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524KMMO-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
!
interface GigabitEthernet0/0.1
 encapsulation dot1Q 1 native
 ip address 192.168.1.1 255.255.255.0
!
interface GigabitEthernet0/0.5
 encapsulation dot1Q 5
 ip address 192.168.5.1 255.255.255.0
!
interface GigabitEthernet0/0.6
 encapsulation dot1Q 6
 ip address 192.168.6.1 255.255.255.0
!
interface GigabitEthernet0/0.7
 encapsulation dot1Q 7
 ip address 192.168.7.1 255.255.255.192
!
interface GigabitEthernet0/0.8
 encapsulation dot1Q 8
 ip address 192.168.8.1 255.255.255.240
!
interface GigabitEthernet0/0.9
 encapsulation dot1Q 9
 ip address 192.168.9.1 255.255.255.224
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/0/1
 ip address 10.10.4.1 255.255.255.252
 clock rate 64000
!
interface Serial0/1/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/1/1
 no ip address
 clock rate 2000000
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
router rip
 network 10.0.0.0
 network 192.168.0.0
 network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end

Branch 2 Running Config
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX15245L2Y-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 10.10.10.1 255.255.255.252
!
interface Serial0/0/1
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/1/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/1/1
 no ip address
 clock rate 2000000
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
router rip
 network 10.0.0.0
 network 192.168.0.0
 network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end

HQ Running Config
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname HQ
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524RYF1-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 209.165.200.25 255.255.255.248
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 10.10.10.2 255.255.255.252
 clock rate 2000000
!
interface Serial0/0/1
 ip address 10.10.4.2 255.255.255.252
!
interface Serial0/1/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/1/1
 no ip address
 clock rate 2000000
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
router rip
 network 10.0.0.0
 network 192.168.0.0
 network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end


