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Introduction:-
How to make a Virtual Machine on a Computer and how to make a LAN on the Computer.  
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This is where we started to create a new Virtual Machine.
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 Here we are putting in the amount of Memory for the VM
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Creating a hard disk drive for the VM
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Adjusting the Size (GB) of the Hard drive.
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Making the States for the Mother Board.
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 This is to boot the Operating system. 
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Checking to see if Windows will start up on VB
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Windows checking on updates.
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This we installed the system’s operating program files.
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Logging into server using an admin account as we needed to configure the network.	Comment by John Rees: This clearly hasn’t worked at all.  The screen shots show a failed ping, and the ping is at the APIPA address which is not what we are intending to use.
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Here we tested the ping and sent and received packets between our server and a local DNS suffix  
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Here we installed an active directory domain.
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In this pic we set up the domain name and the new forest root domain.  
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In these screen shots we renamed the computer and set it up on the root domain. 
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Here we set up an dns server.
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This is the location of the active directory domain controller this is where the database files are kept.
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Here we finished setting up the active domain serve.  
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Above are the directory users and computers 
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Basic system information.	Comment by John Rees: OK, but you can’t have done this on the configuration you showed as your static IP addresses.  It simply wouldn’t work.  Clearly the earlier screenshots are not what you actually used.
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Testing out domain.
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We then had to restart the VM 
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Default domain policy.         


[image: ]
Our next step was to add roles
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Here we are configuring the I.P. address for the DNS server.
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Here we are cloning both machines as we need 4 to complete the task 
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Testing the connection between the client and server 
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This screenshot shows that both systems have full internet access 
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Here we set an IP range between 2 and 223 
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We excluded this IP from the address range so it is no longer distributed by the DNS server. 	Comment by John Rees: OK, but the presented material doesn’t demonstrate that your DHCP server is operating properly.
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