Router 1

Show run:	
Current configuration : 1176 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15241537-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 185.95.1.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 185.95.12.1 255.255.255.252
 clock rate 128000
!
interface Serial0/0/1
 ip address 185.95.13.1 255.255.255.252
!
interface Vlan1
 no ip address
 shutdown
!
router ospf 1
 router-id 1.1.1.1
 log-adjacency-changes
 passive-interface GigabitEthernet0/0
 auto-cost reference-bandwidth 1000
 network 185.95.1.0 0.0.0.255 area 0
 network 185.95.13.0 0.0.0.3 area 0
 network 185.95.12.0 0.0.0.3 area 0
 distance 200
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThe use of this router is restricted.^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end

Show ip int brief:
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.1.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/0/0            185.95.12.1     YES manual up                    up 
Serial0/0/1            185.95.13.1     YES manual up                    up 
Vlan1                  unassigned      YES unset  administratively down down

Show ip route:
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 9 subnets, 3 masks
C       185.95.1.0/24 is directly connected, GigabitEthernet0/0
L       185.95.1.1/32 is directly connected, GigabitEthernet0/0
O       185.95.2.0/24 [200/657] via 185.95.12.2, 00:04:15, Serial0/0/0
O       185.95.3.0/24 [200/657] via 185.95.13.2, 00:04:15, Serial0/0/1
C       185.95.12.0/30 is directly connected, Serial0/0/0
L       185.95.12.1/32 is directly connected, Serial0/0/0
C       185.95.13.0/30 is directly connected, Serial0/0/1
L       185.95.13.1/32 is directly connected, Serial0/0/1
O       185.95.23.0/30 [200/1294] via 185.95.13.2, 00:04:15, Serial0/0/1
                       [200/1294] via 185.95.12.2, 00:04:15, Serial0/0/0


Show ip ospf neighbor:
Neighbor ID     Pri   State           Dead Time   Address         Interface
2.2.2.2           0   FULL/  -        00:00:37    185.95.12.2     Serial0/0/0
3.3.3.3           0   FULL/  -        00:00:38    185.95.13.2     Serial0/0/1

Show ip ospf database:
 OSPF Router with ID (1.1.1.1) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
185.95.23.1     185.95.23.1     927         0x80000007 0x00b1d0 4
185.95.23.2     185.95.23.2     778         0x80000008 0x00d7d2 5
2.2.2.2         2.2.2.2         707         0x8000000b 0x00e11a 5
1.1.1.1         1.1.1.1         706         0x8000000b 0x00a471 5
3.3.3.3         3.3.3.3         706         0x8000000c 0x0014de 5

Router 2

Show run:
Building configuration...

Current configuration : 1162 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524A255-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 185.95.2.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 185.95.12.2 255.255.255.252
!
interface Serial0/0/1
 ip address 185.95.23.1 255.255.255.252
 clock rate 128000
!
interface Vlan1
 no ip address
 shutdown
!
router ospf 1
 router-id 2.2.2.2
 log-adjacency-changes
 passive-interface GigabitEthernet0/0
 auto-cost reference-bandwidth 1000
 network 185.95.2.0 0.0.0.255 area 0
 network 185.95.12.0 0.0.0.3 area 0
 network 185.95.23.0 0.0.0.3 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThe use of this device is restricted.^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end

Show ip int brief:
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.2.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/0/0            185.95.12.2     YES manual up                    up 
Serial0/0/1            185.95.23.1     YES manual up                    up 
Vlan1                  unassigned      YES unset  administratively down down

Show ip route:
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 9 subnets, 3 masks
O       185.95.1.0/24 [110/657] via 185.95.12.1, 00:18:19, Serial0/0/0
C       185.95.2.0/24 is directly connected, GigabitEthernet0/0
L       185.95.2.1/32 is directly connected, GigabitEthernet0/0
O       185.95.3.0/24 [110/657] via 185.95.23.2, 00:14:35, Serial0/0/1
C       185.95.12.0/30 is directly connected, Serial0/0/0
L       185.95.12.2/32 is directly connected, Serial0/0/0
O       185.95.13.0/30 [110/1294] via 185.95.12.1, 00:15:45, Serial0/0/0
                       [110/1294] via 185.95.23.2, 00:15:45, Serial0/0/1
C       185.95.23.0/30 is directly connected, Serial0/0/1
L       185.95.23.1/32 is directly connected, Serial0/0/1

Show ip ospf neighbor:
Neighbor ID     Pri   State           Dead Time   Address         Interface
3.3.3.3           0   FULL/  -        00:00:37    185.95.23.2     Serial0/0/1
1.1.1.1           0   FULL/  -        00:00:38    185.95.12.1     Serial0/0/0

Show ip ospf database:
 OSPF Router with ID (2.2.2.2) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
185.95.23.1     185.95.23.1     1246        0x80000007 0x00b1d0 4
185.95.23.2     185.95.23.2     1098        0x80000008 0x00d7d2 5
2.2.2.2         2.2.2.2         1027        0x8000000b 0x00e11a 5
1.1.1.1         1.1.1.1         1026        0x8000000b 0x00a471 5
3.3.3.3         3.3.3.3         1026        0x8000000c 0x0014de 5

Router 3

Show run:
Building configuration...

Current configuration : 1163 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524NXN7-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 185.95.3.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 185.95.13.2 255.255.255.252
 clock rate 2000000
!
interface Serial0/0/1
 ip address 185.95.23.2 255.255.255.252
!
interface Vlan1
 no ip address
 shutdown
!
router ospf 1
 router-id 3.3.3.3
 log-adjacency-changes
 passive-interface GigabitEthernet0/0
 auto-cost reference-bandwidth 1000
 network 185.95.3.0 0.0.0.255 area 0
 network 185.95.23.0 0.0.0.3 area 0
 network 185.95.13.0 0.0.0.3 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThe use of this device is restricted.^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end

Show ip int brief:
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.3.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/0/0            185.95.13.2     YES manual up                    up 
Serial0/0/1            185.95.23.2     YES manual up                    up 
Vlan1                  unassigned      YES unset  administratively down down

Show ip route:
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 9 subnets, 3 masks
O       185.95.1.0/24 [110/657] via 185.95.13.1, 00:20:32, Serial0/0/0
O       185.95.2.0/24 [110/657] via 185.95.23.1, 00:20:32, Serial0/0/1
C       185.95.3.0/24 is directly connected, GigabitEthernet0/0
L       185.95.3.1/32 is directly connected, GigabitEthernet0/0
O       185.95.12.0/30 [110/1294] via 185.95.23.1, 00:20:32, Serial0/0/1
                       [110/1294] via 185.95.13.1, 00:20:32, Serial0/0/0
C       185.95.13.0/30 is directly connected, Serial0/0/0
L       185.95.13.2/32 is directly connected, Serial0/0/0
C       185.95.23.0/30 is directly connected, Serial0/0/1
L       185.95.23.2/32 is directly connected, Serial0/0/1

Show ip ospf neighbor:
Neighbor ID     Pri   State           Dead Time   Address         Interface
1.1.1.1           0   FULL/  -        00:00:31    185.95.13.1     Serial0/0/0
2.2.2.2           0   FULL/  -        00:00:39    185.95.23.1     Serial0/0/1

Show ip ospf database:
OSPF Router with ID (3.3.3.3) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
2.2.2.2         2.2.2.2         1242        0x8000000b 0x00e11a 5
185.95.23.1     185.95.23.1     1461        0x80000007 0x00b1d0 4
185.95.23.2     185.95.23.2     1313        0x80000008 0x00d7d2 5
3.3.3.3         3.3.3.3         1240        0x8000000c 0x0014de 5
1.1.1.1         1.1.1.1         1240        0x8000000b 0x00a471 5

Ping from PC-A to PC-B
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Pinging 185.55.2.3 with 32 byres of data.

Request cimed out.
Reply from 185.55
Reply from 18555
Reply from 185 55

Ping scavistics for 185.55.2.3
Packets: Sent = 3, Received = 3, Lost = 1 (25% loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = lns, Maximm = ims, Average = lms

C:\>ping 185.55.2.3
Pinging 185.55.2.3 with 32 byres of data:

Reply from 185.55 “ime=3ms TTL=12¢
Reply from 18555 “ime=3ms TTL=12¢
Reply from 18555 bytes=32 vime=lms TTL=12¢
Reply from 185 55 bytes=32 vime=lms TTI=12¢

Ping scavistics for 185.55.2.3
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Bpproximate round trip vimes in milli-seconds

Minimm = lns, Maximm = ims, Average = 2ms
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Pinging 185.55.3.3 with 32 bytes of data.

Request cimed out.
Reply from 185.55
Reply from 18555
Reply from 185 55

Ping scavistics for 185.55.3.3
Packets: Sent = 4, Received = 3, Lost = 1 (25% loss),
Bpprosimate round trip vimes in milli-seconds

Minimm = lns, Maximm = lms, Average = lms
C:\>ping 185.55.3.3
Pinging 185.55.3.3 with 32 byres of data:
Trim2e
Trim126

Trim126
Tri-ze

Reply from 185.55
Reply from 18555
Reply from 18555
Reply from 185 55

Ping scavistics for 185.55.3.3
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpproximate round trip vimes in milli-seconds

Minimm = lns, Maximm = ims, Average = 2ms





