[image: A screenshot of a computer

Description automatically generated][image: A screenshot of a computer

Description automatically generated][image: A screenshot of a computer

Description automatically generated]
[image: A screenshot of a computer

Description automatically generated][image: A screenshot of a computer

Description automatically generated][image: A screenshot of a computer

Description automatically generated]

[image: A screenshot of a computer

Description automatically generated][image: A screenshot of a computer

Description automatically generated]
[image: A diagram of a network

Description automatically generated]


Router1(config)# interface GigabitEthernet0/0
Router1(config-if)# ip address 192.168.1.1 255.255.255.0
Router1(config-if)# no shutdown

Router1(config)# interface GigabitEthernet0/1
Router1(config-if)# no shutdown

Router1(config)# wireless ssid MyWLAN
Router1(config-ssid)# authentication open
Router1(config-ssid)# key-management wpa version 2
Router1(config-ssid)# wpa-psk ascii YourSecretKey

RA   Router>enable
RA   Router#configure terminal

image5.png
3

R RA - o X
Physical CL  Attributes ser Draw Desi¢ Layo! Refer Maili Revie View He
GLOBAL Serial3/0 Vigw Be careful—files from the Intemet can contair
Settings you need to edit, it's safer to stay in Protecte«
- - Port Status [Jon Fa0
Algorithm Settings uplex .
RO“TFHG Clock Rate 1200 ~
Static
RIP IP Configuration d
Adrmin_PCA
INTERFACE IPv4 Address 100121 T min §
FastEthernet0/0 ‘Subnet Mask 1255.255.255.252 opology
FastEthernet1/0
Serial2/0 TxRing Limit 10
Serial3/0
FastEthernet4/0
FastEthernet5/0
Page 2 of 12

Addressing Tab

Eguivalent I0S Commands
-

Device Interface | IP Address Sub

Router (confi

AlA G0/0/0.10 | 192.168.1.1 | 255.2




image6.png
ISCO Facket Ira

cer

Bra

R Dl

Physical  Config _Deskiop | Programming _ Attibutes

Desic Layo! Refer Maili Revie Vie

areful—files from the Internet can ¢

Interface Wireless0
IP Configuration

O DHcP
1Pv4 Address

‘Subnet Mask
Default Gateway
DNS Server

1Pv6 Configuration

(®) Automatic
1Pv6 Address

Link Local Address
Default Gateway

DNS Server

(® static

need to edit, it's safer to stay in Pr

172.16.0.252

ation (80 marks)

2552552550

0000

0000

L: (On all devices) (15 mark
me on all devices as per the

O static

kup
ices with IP address shown i

fion (15 marks)

FE80:2D0-BAFF-FE14:74D

RP with AS 12 on RA, RB &

tic summarization. Use the N
.1.1.1onRA,2.2.2.2 0onRB
ces to Passive.

)nfiguration (15 marks)
INs as shown in the table.
rfaces appropriately as Trunk
easible network connectivity.
and SB, configure Rapid PV
ast and BPDU Guard on the |

figuration ( 10 marks)

thannel interfaces as trunk linl
pure a PAgP EtherChannel on

rure an PAgP EtherChannel o




image7.png
= oL a q

RA

i Bt Bl bl

Physical )x ¢

Physical Config _CLI_ Aftributes

10S Command Line Interface

Router con0 is now available

Press RETURN to get started.

Press RETURN to get started!

Router>configure terminal

% Invalid input detected at '' marker.

Router>config terminal

% Invalid input detected at '' marker.

Router>
Router>enable

Router#configure terminal

Enter configuration commands, one per line.
Router (config) ¥hostname RA

RA(config) #no ip domain-lookup

RA (config) #|

End with CNTL/Z.
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it, it's safer to stay in Protected View.
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Routerfhostname RB

% Invalid input detected at '' marker.

Router#RB
Translating "RB"
Router#enable
Router#hostname RB

.domain server (255.255.255.255)

% Invalid input detected at '' marker.

Routerfhost

Router#name rb]

% Invalid input detected at '' marker.

Router#

Router#enable

Router#configure terminal

Enter configuration commands, one per line. End with CNTL/Z.
Router (config) fhostname RB

RE(config) #no ip domain-lookup

RE(config) #interface S0/1/0

% Invalid input detected at '' marker.
RB (config) #network 192.168.1.0 0.0.0.255
% Invalid input detected at '' marker.

RB (config) #no ip domain-lookup

RB (config) #

RB(config) #

RB(config) #interface FastEthernet0/0
RB (config-if)#

RB (config-if) #exit

RB(config) #interface FastEthernet0/0
RB (config-if)#

RB (config-if) #exit

RB(config) #interface FastEthernetl/0
RB (config-if)#

RB (config-if) #exit

RB(config) #interface Serial2/0

RB (config-if)#

% Unknown command or computer name, or unable to find computer address
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Switch(config) #interface FastEthernet4/1
Switch(config-if) #
Switch(config-if)#exit

Switch(config) #interface FastEthernet5/1
Switch(config-if) #
Switch(config-if)#exit

Switch(config) #interface FastEthernet0/1
Switch(config-if) #

switch con0 is now available

Press RETURN to get started.

Switch>enable
switch#config t
Enter configuration commands, one per line.

switch(config) #interface range fa0/1-2

End with CNTL/Z.
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Press RETURN to get started!

Router>configure terminal

% Invalid input detected at '' marker.

Router>config terminal

% Invalid input detected at '' marker.

Router>
Router>enable

Router#configure terminal

Enter configuration commands, one per line. End with CNTL/Z.
Router (config) fhostname RA

RA(config)#no ip domain-lookup

RA(config) #router eigrp 12

RA(config-router) #network 192.168.1.0 0.0.0.255
RA(config-router) #network 192.168.2.0 0.0.0.255
RA(config-router) #network 10.0.0.0 0.0.0.3

RA(config-router) #network 10.0.12.0 0.0.0.3
RA(config-router) #network 10.0.23.0 0.0.0.3
RA(config-router) #no auto-summary

RA(config-router) feigrp router-id 1.1.1.1

RA(config-router) #passive-interface

% Incomplete command.

RA(config-router) #passive-interface default
RA(config-router) #no passive-interface G0/0/0.10
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GLOBAL
Settings
Algorithm Settings
ROUTING
Static
RIP
INTERFACE
FastEthernet1/0
Serial2/0
Serial3/0
FastEthernet4/0
FastEthernet5/0

FastEthemet0/0
Port Status [Jon
Bandwidth 100 Mbps () 10 Mbps [] Auto
Duplex Half Duplex () Full Duplex [] Auto
MAC Address 00E0.8F2C.7598

IP Configuration

1Pv4 Address 192.168.1.1

‘Subnet Mask 255.255.255.0
TxRing Limit 10





