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In this document will be given screen shots and commands which I used to do my part 2 of the test.
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VLAN and STP Configuration
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EtherChannel Configuration
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DHCP Configuration
Below are the commands when I tried to config DHCP Configuration, as follows

enable
configure terminal
Create the RVlan10 DHCP pool:

ip dhcp excluded-address 192.168.1.1 192.168.1.10
ip dhcp pool RVlan10
network 192.168.1.0 255.255.255.0
default-router 192.168.1.1 
dns-server 172.16.0.254
Create the RVlan20 DHCP pool:

ip dhcp excluded-address 192.168.2.1 192.168.2.10
ip dhcp pool RVlan20
network 192.168.2.0 255.255.255.0
default-router 192.168.2.1
dns-server 172.16.0.254
Exit back to privileged EXEC mode:

End




Bellow all my logs from Paket tracer:

Tue Nov 14 10:42:18 2023   RA   Router>enable
Tue Nov 14 10:42:18 2023   RA   Router#configure terminal
Tue Nov 14 10:42:18 2023   RA   Router(config)#router rip
Tue Nov 14 10:42:20 2023   RA   Router(config-router)#end
Tue Nov 14 10:42:20 2023   RA   Router#configure terminal
Tue Nov 14 10:42:20 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:44:28 2023   RA   Router(config-if)#exit
Tue Nov 14 10:44:28 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:44:44 2023   RC   Router>enable
Tue Nov 14 10:44:44 2023   RC   Router#configure terminal
Tue Nov 14 10:44:44 2023   RC   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:45:30 2023   RA   Router(config-if)#exit
Tue Nov 14 10:45:30 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:45:48 2023   RA   Router(config-if)#exit
Tue Nov 14 10:45:48 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:47:05 2023   RA   Router(config-if)#exit
Tue Nov 14 10:47:05 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:47:14 2023   RA   Router(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 10:47:14 2023   RA   Router(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 10:47:37 2023   RB   Router>enable
Tue Nov 14 10:47:37 2023   RB   Router#configure terminal
Tue Nov 14 10:47:37 2023   RB   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:47:43 2023   RB   Router(config-if)#exit
Tue Nov 14 10:47:43 2023   RB   Router(config)#interface GigabitEthernet0/1
Tue Nov 14 10:47:53 2023   RB   Router(config-if)#ip address 10.0.12.2 255.0.0.0
Tue Nov 14 10:47:54 2023   RB   Router(config-if)#ip address 10.0.12.2 255.0.0.0
Tue Nov 14 10:47:57 2023   RB   Router(config-if)#ip address 10.0.12.2 255.255.255.252
Tue Nov 14 10:48:14 2023   RB   Router(config-if)#exit
Tue Nov 14 10:48:33 2023   RB   Router(config)#router rip
Tue Nov 14 10:48:34 2023   RB   Router(config-router)#end
Tue Nov 14 10:48:34 2023   RB   Router#vlan database
Tue Nov 14 10:48:42 2023   RB   Router(vlan)#exit
Tue Nov 14 10:48:42 2023   RB   Router#configure terminal
Tue Nov 14 10:48:42 2023   RB   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:48:47 2023   RB   Router(config-if)#exit
Tue Nov 14 10:48:47 2023   RB   Router(config)#interface GigabitEthernet0/1
Tue Nov 14 10:48:52 2023   RB   Router(config-if)#ip address 172.16.0.1 255.255.255.252
Tue Nov 14 10:48:52 2023   RB   Router(config-if)#ip address 172.16.0.1 255.255.255.252
Tue Nov 14 10:48:57 2023   RB   Router(config-if)#ip address 172.16.0.1 255.255.255.0
Tue Nov 14 10:49:10 2023   RA   Router(config-if)#exit
Tue Nov 14 10:49:10 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:49:14 2023   RA   Router(config-if)#exit
Tue Nov 14 10:49:14 2023   RA   Router(config)#interface GigabitEthernet0/1
Tue Nov 14 10:49:20 2023   RA   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 10:49:20 2023   RA   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 10:49:23 2023   RA   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 10:49:27 2023   RA   Router(config-if)#exit
Tue Nov 14 10:49:49 2023   RC   Router(config-if)#exit
Tue Nov 14 10:50:02 2023   RC   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 10:50:05 2023   RC   Router(config-if)#ip address 172.16.0.2 255.255.0.0
Tue Nov 14 10:50:06 2023   RC   Router(config-if)#ip address 172.16.0.2 255.255.0.0
Tue Nov 14 10:50:43 2023   SM 1   Switch>enable
Tue Nov 14 10:50:43 2023   SM 1   Switch#configure terminal
Tue Nov 14 10:50:49 2023   SM 1   Switch(config)#interface FastEthernet0/1
Tue Nov 14 10:50:50 2023   SM 1   Switch(config-if)#exit
Tue Nov 14 10:50:50 2023   SM 1   Switch(config)#interface FastEthernet0/2
Tue Nov 14 10:50:51 2023   SM 1   Switch(config-if)#exit
Tue Nov 14 10:50:51 2023   SM 1   Switch(config)#interface FastEthernet0/3
Tue Nov 14 10:50:52 2023   SM 1   Switch(config-if)#exit
Tue Nov 14 10:50:52 2023   SM 1   Switch(config)#interface FastEthernet0/4
Tue Nov 14 11:03:51 2023   RA   IR800>interface G0/0/0.10
Tue Nov 14 11:03:51 2023   RA   IR800>ip address 192.168.1.1 255.255.255.0
Tue Nov 14 11:03:51 2023   RA   IR800>interface G0/0/0.20 
Tue Nov 14 11:03:51 2023   RA   IR800>ip address 192.168.2.1 255.255.255.0
Tue Nov 14 11:03:51 2023   RA   IR800>interface S0/2/0
Tue Nov 14 11:03:51 2023   RA   IR800>ip address 10.0.0.1 255.255.255.252
Tue Nov 14 11:03:51 2023   RA   IR800>interface S0/1/0
Tue Nov 14 11:03:51 2023   RA   IR800>ip address 10.0.12.1 255.255.255.252 
Tue Nov 14 11:03:51 2023   RA   IR800>interface S0/1/1
Tue Nov 14 11:03:53 2023   RA   IR800>ip address 10.0.23.1 255.255.255.252
Tue Nov 14 11:04:12 2023   RA   IR800>interface G0/00.10
Tue Nov 14 11:07:59 2023   RA   IR800>enable
Tue Nov 14 11:07:59 2023   RA   IR800#configure terminal
Tue Nov 14 11:07:59 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:08:06 2023   RA   IR800(config-if)#no ip address
Tue Nov 14 11:08:13 2023   RA   IR800(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 11:08:16 2023   RA   IR800(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 11:08:18 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:18 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:08:25 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:25 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:08:27 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:27 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:08:28 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:28 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:08:28 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:28 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:08:29 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:29 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:08:30 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:30 2023   RA   IR800(config)#interface GigabitEthernet3
Tue Nov 14 11:08:31 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:31 2023   RA   IR800(config)#interface GigabitEthernet4
Tue Nov 14 11:08:31 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:31 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:08:32 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:32 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:08:33 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:08:33 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:08:37 2023   RA   IR800(config-if)#ip address  
Tue Nov 14 11:08:39 2023   RA   IR800(config-if)#ip address  
Tue Nov 14 11:08:39 2023   RA   IR800(config-if)#end
Tue Nov 14 11:08:39 2023   RA   IR800#vlan database
Tue Nov 14 11:09:38 2023   RA   IR800(vlan)#enable
Tue Nov 14 11:09:43 2023   RA   IR800(vlan)#enable
Tue Nov 14 11:09:49 2023   RA   IR800(vlan)#configure terminal
Tue Nov 14 11:10:10 2023   RA   IR800(vlan)#exit
Tue Nov 14 11:10:10 2023   RA   IR800#configure terminal
Tue Nov 14 11:10:10 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:10:11 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:10:11 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:19:38 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:19:38 2023   RA   IR800(config)#interface Wlan-GigabitEthernet0
Tue Nov 14 11:19:40 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:19:40 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:19:49 2023   RA   IR800(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 11:19:49 2023   RA   IR800(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 11:19:52 2023   RA   IR800(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 11:19:57 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:19:57 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:19:59 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:19:59 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:20:00 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:00 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:20:03 2023   RA   IR800(config-if)#switchport mode trunk
Tue Nov 14 11:20:04 2023   RA   IR800(config-if)#switchport mode access
Tue Nov 14 11:20:05 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:05 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:20:07 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:07 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:20:08 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:08 2023   RA   IR800(config)#interface GigabitEthernet3
Tue Nov 14 11:20:09 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:09 2023   RA   IR800(config)#interface GigabitEthernet4
Tue Nov 14 11:20:09 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:09 2023   RA   IR800(config)#interface wlan-ap0
Tue Nov 14 11:20:11 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:11 2023   RA   IR800(config)#interface Wlan-GigabitEthernet0
Tue Nov 14 11:20:12 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:12 2023   RA   IR800(config)#interface wlan-ap0
Tue Nov 14 11:20:20 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:20:20 2023   RA   IR800(config)#interface wlan-ap0
Tue Nov 14 11:23:33 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:23:33 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:23:41 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:23:41 2023   RA   IR800(config)#interface GigabitEthernet1
Tue Nov 14 11:23:44 2023   RA   IR800(config-if)#shutdown
Tue Nov 14 11:23:45 2023   RA   IR800(config-if)#no shutdown
Tue Nov 14 11:23:59 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:23:59 2023   RA   IR800(config)#interface GigabitEthernet2
Tue Nov 14 11:24:00 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:24:00 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:24:11 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:24:11 2023   RA   IR800(config)#interface Wlan-GigabitEthernet0
Tue Nov 14 11:24:12 2023   RA   IR800(config-if)#exit
Tue Nov 14 11:24:12 2023   RA   IR800(config)#interface GigabitEthernet0
Tue Nov 14 11:26:24 2023   SM 1   Switch>enable
Tue Nov 14 11:26:24 2023   SM 1   Switch#configure terminal
Tue Nov 14 11:27:59 2023   RA   IR800(config-if)#configure termina;
Tue Nov 14 11:28:06 2023   RA   IR800(config-if)#hostname RA
Tue Nov 14 11:28:49 2023   RA   RA(config)#no ip domain-lookup
Tue Nov 14 11:29:11 2023   RA   RA(config)#interface  G0/0/0.10
Tue Nov 14 11:29:12 2023   RA   RA(config)#interface  G0/0/0.10
Tue Nov 14 11:30:43 2023   RA   RA(config)#interface GigabitEthernet0
Tue Nov 14 11:30:59 2023   RA   RA(config-if)#exit
Tue Nov 14 11:30:59 2023   RA   RA(config)#interface GigabitEthernet1
Tue Nov 14 11:31:00 2023   RA   RA(config-if)#exit
Tue Nov 14 11:31:00 2023   RA   RA(config)#interface GigabitEthernet0
Tue Nov 14 11:31:19 2023   RA   RA(config-if)#end
Tue Nov 14 11:31:30 2023   RA   RA#write
Tue Nov 14 11:35:10 2023   SA   Switch>enable
Tue Nov 14 11:35:10 2023   SA   Switch#configure terminal
Tue Nov 14 11:35:14 2023   SA   Switch(config)#interface FastEthernet0/1
Tue Nov 14 11:35:17 2023   SA   Switch(config-if)#exit
Tue Nov 14 11:35:17 2023   SA   Switch(config)#interface FastEthernet0/2
Tue Nov 14 11:35:18 2023   SA   Switch(config-if)#exit
Tue Nov 14 11:35:18 2023   SA   Switch(config)#interface FastEthernet0/3
Tue Nov 14 11:40:38 2023   RB   Router>enable
Tue Nov 14 11:40:44 2023   RB   Router#configure terminal
Tue Nov 14 11:40:51 2023   RB   Router(config)#conf t
Tue Nov 14 11:41:04 2023   RB   Router(config)#hostname RB
Tue Nov 14 11:42:32 2023   RB   RB(config)#hostname RB
Tue Nov 14 11:42:36 2023   RB   RB(config)#configure 
Tue Nov 14 11:42:38 2023   RB   RB(config)#enable
Tue Nov 14 11:42:40 2023   RB   RB(config)#enable
Tue Nov 14 11:42:52 2023   RB   RB(config)#enable
Tue Nov 14 11:42:55 2023   RB   RB(config)#exit
Tue Nov 14 11:42:58 2023   RB   RB#enable
Tue Nov 14 11:43:05 2023   RB   RB#configure terminal
Tue Nov 14 11:43:21 2023   RB   RB(config)#hostname RB
Tue Nov 14 11:43:35 2023   RB   RB(config)#no ip domain-lookup
Tue Nov 14 11:43:44 2023   RB   RB(config)#interface GigabitEthernet0/0
Tue Nov 14 11:43:55 2023   RB   RB(config-if)#exit
Tue Nov 14 11:43:55 2023   RB   RB(config)#interface GigabitEthernet0/0
Tue Nov 14 11:43:59 2023   RB   RB(config-if)#exit
Tue Nov 14 11:43:59 2023   RB   RB(config)#interface GigabitEthernet0/1
Tue Nov 14 11:44:00 2023   RB   RB(config-if)#exit
Tue Nov 14 11:44:00 2023   RB   RB(config)#interface GigabitEthernet0/0
Tue Nov 14 11:44:02 2023   RB   RB(config-if)#exit
Tue Nov 14 11:44:02 2023   RB   RB(config)#interface GigabitEthernet0/1
Tue Nov 14 11:44:39 2023   RB   RB(config-if)#ip address 10.0.12.2 255.255.255.0
Tue Nov 14 11:44:39 2023   RB   RB(config-if)#ip address 10.0.12.2 255.255.255.0
Tue Nov 14 11:44:42 2023   RB   RB(config-if)#ip address 10.0.12.2 255.255.255.252
Tue Nov 14 11:44:47 2023   RB   RB(config-if)#ip address 10.0.12.2 255.255.255.0
Tue Nov 14 11:44:53 2023   RB   RB(config-if)#ip address 172.16.0.1 255.255.255.0
Tue Nov 14 11:44:54 2023   RB   RB(config-if)#exit
Tue Nov 14 11:44:56 2023   RB   RB(config)#router rip
Tue Nov 14 11:44:56 2023   RB   RB(config-router)#end
Tue Nov 14 11:44:56 2023   RB   RB#configure terminal
Tue Nov 14 11:44:57 2023   RB   RB(config)#end
Tue Nov 14 11:44:57 2023   RB   RB#vlan database
Tue Nov 14 11:44:58 2023   RB   RB(vlan)#exit
Tue Nov 14 11:44:58 2023   RB   RB#configure terminal
Tue Nov 14 11:44:58 2023   RB   RB(config)#interface GigabitEthernet0/0
Tue Nov 14 11:45:01 2023   RB   RB(config-if)#exit
Tue Nov 14 11:45:01 2023   RB   RB(config)#interface GigabitEthernet0/1
Tue Nov 14 11:45:02 2023   RB   RB(config-if)#exit
Tue Nov 14 11:45:02 2023   RB   RB(config)#interface GigabitEthernet0/0
Tue Nov 14 11:45:08 2023   RB   RB(config-if)#exit
Tue Nov 14 11:45:30 2023   RB   RB(config)#router rip
Tue Nov 14 11:45:31 2023   RB   RB(config-router)#end
Tue Nov 14 11:45:31 2023   RB   RB#vlan database
Tue Nov 14 11:45:32 2023   RB   RB(vlan)#exit
Tue Nov 14 11:45:32 2023   RB   RB#configure terminal
Tue Nov 14 11:45:32 2023   RB   RB(config)#interface GigabitEthernet0/0
Tue Nov 14 11:46:12 2023   RC   Router>enable
Tue Nov 14 11:46:15 2023   RC   Router#configure terminal
Tue Nov 14 11:46:27 2023   RC   Router(config)#hostname RC
Tue Nov 14 11:46:41 2023   RC   RC(config)#no ip domain-lookup
Tue Nov 14 11:47:02 2023   RC   RC(config)#interface S0/1/0
Tue Nov 14 11:47:06 2023   RC   RC(config)#exit
Tue Nov 14 11:47:31 2023   RC   RC#configure terminal
Tue Nov 14 11:47:31 2023   RC   RC(config)#interface GigabitEthernet0/0
Tue Nov 14 11:50:02 2023   RA   RA>router eigrp 12
Tue Nov 14 11:50:16 2023   RA   RA>config t
Tue Nov 14 11:50:19 2023   RA   RA>enable
Tue Nov 14 11:50:29 2023   RA   RA#router eigrp 12
Tue Nov 14 11:51:37 2023   RA   RA#configure terminal
Tue Nov 14 11:51:58 2023   RA   RA(config)#router eigrp 12
Tue Nov 14 11:52:26 2023   RA   RA(config-router)#network 192.168.1.0 0.0.0.255
Tue Nov 14 11:52:35 2023   RA   RA(config-router)#network 192.168.2.0 0.0.0.255
Tue Nov 14 11:53:01 2023   RA   RA(config-router)#network 10.0.0.0 0.0.0.3
Tue Nov 14 11:53:11 2023   RA   RA(config-router)#network 10.0.12.0 0.0.0.3
Tue Nov 14 11:53:18 2023   RA   RA(config-router)#network 10.0.23.0 0.0.0.3
Tue Nov 14 11:53:30 2023   RA   RA(config-router)#no auto-summary
Tue Nov 14 11:53:56 2023   RA   RA(config-router)#eigrp router-id 1.1.1.1
Tue Nov 14 11:54:11 2023   RA   RA(config-router)#passive-interface default
Tue Nov 14 11:54:49 2023   RA   RA(config-router)#no passive-interface G0/0/0.10
Tue Nov 14 11:55:17 2023   RA   RA(config-router)#no passive-interface
Tue Nov 14 11:55:58 2023   RA   RA(config-router)#exit
Tue Nov 14 11:56:01 2023   RA   RA(config)#exit
Tue Nov 14 11:56:19 2023   RB   RB>enable
Tue Nov 14 11:56:22 2023   RB   RB#configure terminal
Tue Nov 14 11:56:34 2023   RB   RB(config)#router eigrp 12
Tue Nov 14 11:56:50 2023   RB   RB(config-router)#network 10.0.12.0 0.0.03
Tue Nov 14 11:57:32 2023   RB   RB(config-router)#network 172.16.0.0 0.0.0.255
Tue Nov 14 11:57:44 2023   RB   RB(config-router)#no auto-summary
Tue Nov 14 11:58:03 2023   RB   RB(config-router)#eigrp router-id 2.2.2.2
Tue Nov 14 11:58:20 2023   RB   RB(config-router)#passive-interface default
Tue Nov 14 11:59:06 2023   RC   RC>enable
Tue Nov 14 11:59:11 2023   RC   RC#configure terminal
Tue Nov 14 11:59:48 2023   RC   RC(config)#network 172.16.0.0 0.0.0.255
Tue Nov 14 12:00:10 2023   RC   RC(config)#router eigrp 12
Tue Nov 14 12:00:21 2023   RC   RC(config-router)#network 172.16.0.0 0.0.0.255
Tue Nov 14 12:00:32 2023   RC   RC(config-router)#no auto-summary
Tue Nov 14 12:00:49 2023   RC   RC(config-router)#eigrp router-id 3.3.3.3
Tue Nov 14 12:01:06 2023   RC   RC(config-router)#passive-interface default
Tue Nov 14 12:05:10 2023   RC   RC(config-router)#no passive-interface G0/0/0
Tue Nov 14 12:08:26 2023   SA   Switch>vlan 10
Tue Nov 14 12:08:28 2023   SA   Switch>enable
Tue Nov 14 12:08:31 2023   SA   Switch#vlan 10
Tue Nov 14 12:08:33 2023   SA   Switch#enable
Tue Nov 14 12:08:35 2023   SA   Switch#config terminal
Tue Nov 14 12:10:29 2023   SA   Switch(config)#vlan 1
Tue Nov 14 12:10:37 2023   SA   Switch#config terminal
Tue Nov 14 12:10:42 2023   SA   Switch(config)#vlan 10
Tue Nov 14 12:10:46 2023   SA   Switch(config-vlan)#name Carol
Tue Nov 14 12:11:18 2023   SA   Switch(config-vlan)#interface Fa0/1
Tue Nov 14 12:11:38 2023   SA   Switch(config-if)#switchport mode trunk
Tue Nov 14 12:11:50 2023   SA   Switch(config-if)#interface Fa0/2
Tue Nov 14 12:12:11 2023   SA   Switch(config-if)#switchport mode access
Tue Nov 14 12:12:36 2023   SA   Switch(config-if)#switchport access vlan 10
Tue Nov 14 12:13:28 2023   SA   Switch(config-if)#interface Fa0/3
Tue Nov 14 12:13:32 2023   SA   Switch(config-if)#interface Fa0/3
Tue Nov 14 12:13:50 2023   SA   Switch(config-if)#switchport
Tue Nov 14 12:14:08 2023   SA   Switch(config-if)#switch fastethswitchport
Tue Nov 14 12:14:15 2023   SA   Switch(config-if)#interface Fa0
Tue Nov 14 12:14:22 2023   SA   Switch(config-if)#interface Fa0/1
Tue Nov 14 12:14:27 2023   SA   Switch(config-if)#switchport access vlan 10
Tue Nov 14 12:14:33 2023   SA   Switch(config-if)#switchport mode access
Tue Nov 14 12:14:34 2023   SA   Switch(config-if)#switchport access vlan 10
Tue Nov 14 12:16:07 2023   SA   Switch#config terminal
Tue Nov 14 12:16:13 2023   SA   Switch(config)#vlan 10
Tue Nov 14 12:16:32 2023   SA   Switch(config-vlan)#sparring-tree mode rapid-pvst
Tue Nov 14 12:16:50 2023   SA   Switch(config-vlan)#interface 
Tue Nov 14 12:17:02 2023   SA   Switch(config-vlan)#interface range fa0/4-24
Tue Nov 14 12:17:12 2023   SA   Switch(config-if-range)#shutdown
Tue Nov 14 12:18:32 2023   SB   Switch>enable
Tue Nov 14 12:18:34 2023   SB   Switch#config t
Tue Nov 14 12:18:42 2023   SB   Switch(config)#vlan 20
Tue Nov 14 12:18:46 2023   SB   Switch(config-vlan)#name Carol
Tue Nov 14 12:19:01 2023   SB   Switch(config-vlan)#interface Fa0
Tue Nov 14 12:19:12 2023   SB   Switch(config-vlan)#interface Fa0/1
Tue Nov 14 12:19:22 2023   SB   Switch(config-if)#switchport mode trunk
Tue Nov 14 12:19:33 2023   SB   Switch(config-if)#switchport mode trunk
Tue Nov 14 12:19:48 2023   SB   Switch(config-if)#interface Fa0/2
Tue Nov 14 12:19:56 2023   SB   Switch(config-if)#switchport mode access
Tue Nov 14 12:20:16 2023   SB   Switch(config-if)#switchport access vlan 20
Tue Nov 14 12:20:30 2023   SB   Switch(config-if)#sparring-tree mod
Tue Nov 14 12:20:39 2023   SB   Switch(config-if)#sparring-tree mode rapid-pvst
Tue Nov 14 12:21:06 2023   SB   Switch(config-if)#sparing-tree portfast
Tue Nov 14 12:21:11 2023   SB   Switch(config-if)#sparing-tree portfast
Tue Nov 14 12:21:25 2023   SB   Switch(config-if)#inteface range fa0/4-24
Tue Nov 14 12:25:25 2023   SM 1   Switch>enable
Tue Nov 14 12:25:27 2023   SM 1   Switch#conf t
Tue Nov 14 12:25:39 2023   SM 1   Switch(config)#interface range fa0/1-2
Tue Nov 14 12:25:54 2023   SM 1   Switch(config-if-range)#channel-group 1 mode desirable
Tue Nov 14 12:26:10 2023   SM 1   Switch(config-if-range)#inte
Tue Nov 14 12:26:17 2023   SM 1   Switch(config-if-range)#interface port-channel 1
Tue Nov 14 12:26:31 2023   SM 1   Switch(config-if)#switch mode trunk
Tue Nov 14 12:28:15 2023   SA   Switch(config-if-range)#no shutdown
Tue Nov 14 12:42:46 2023   SM 2   Switch>enable
Tue Nov 14 12:42:48 2023   SM 2   Switch#config t
Tue Nov 14 12:44:44 2023   SM 2   Switch(config)#interface range fa0/1-2
Tue Nov 14 12:48:33 2023   SM 2   Switch(config-if-range)#channel-group 1 mode desirable
Tue Nov 14 12:48:37 2023   SM 2   Switch(config-if-range)#up
Tue Nov 14 12:49:20 2023   SM 2   Switch(config-if-range)#switchport mode trunk
Tue Nov 14 12:52:53 2023   SM 2   Switch#exit
Tue Nov 14 12:55:41 2023   RB   RB>enable
Tue Nov 14 12:55:46 2023   RB   RB#config t
Tue Nov 14 12:55:55 2023   RB   RB(config)#interface g0/0
Tue Nov 14 12:56:14 2023   RB   RB(config-if)#standby 1 172.16.0.3
Tue Nov 14 12:56:32 2023   RB   RB(config-if)#standby 1 172.16.0.3
Tue Nov 14 12:56:42 2023   RB   RB(config-if)#standby 1 priority 110
Tue Nov 14 12:56:45 2023   RB   RB(config-if)#end
Tue Nov 14 12:57:43 2023   RC   RC>enable
Tue Nov 14 12:57:44 2023   RC   RC#config t
Tue Nov 14 12:57:51 2023   RC   RC(config)#interface g0/0
Tue Nov 14 12:58:10 2023   RC   RC(config-if)#standby 1 ip 172.16.03
Tue Nov 14 12:58:13 2023   RC   RC(config-if)#standby 1 ip 172.16.0.3
Tue Nov 14 12:58:17 2023   RC   RC(config-if)#end
Tue Nov 14 13:06:48 2023   RC   RC#exit
Tue Nov 14 13:00:55 2023   RA   RA(config)#interface enable
Tue Nov 14 13:01:14 2023   RA   RA(config-if)#ip dhcp excluded-address 192.168.1.1 192.168.1.10
Tue Nov 14 13:01:32 2023   RA   RA(config-if)#ip dhcp pool RVlan103
Tue Nov 14 13:01:42 2023   RA   RA(config-if)#network 192.168.1.0 255.255.255.0
defaul
Tue Nov 14 13:01:45 2023   RA   RA(config-if)#t-router 192.168.1.1 
Tue Nov 14 13:03:25 2023   RA   RA(config-if)#dns-server 172.16.0.254
Tue Nov 14 13:04:12 2023   RA   RA(config-if)#ip dhcp excluded-address 192.168.2.1 192.168.2.10
Tue Nov 14 13:04:15 2023   RA   RA(config-if)#ip dhcp pool RVlan20
Tue Nov 14 13:04:24 2023   RA   RA(config-if)#network 192.168.2.0 255.255.255.0
Tue Nov 14 13:05:15 2023   RA   RA(config-if)#default-router 192.168.2.1
Tue Nov 14 13:06:14 2023   RA   RA(config-if)#dns-server 172.16.0.254
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Equivalent I0S Commands

TRE00 (cont1g-1T) Foxit
IR800 (config) #interface GigabitEthernet2
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface Wlan-GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetd
1R800 (config-if)#
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Press RETURN to get started.

RA>router eigrp 12

% Invalid input detected at '°' marker.

RA>config ©

% Invalid input detected at '°' marker.

Ra>enable
RAfrouter eigrp 12

% Invalid input detected at '°' marker.

RAfconfigure terminal
Enter configuration commands, one per line. End with CNTL/Z.
RA(config) frouter eigrp 12

RA(config-router) fnetwork 192.168.1.0 0.0.0.255
RA(config-router) fnetwork 192.168.2.0 0.0.0.255
RA(config-router) #network 10.0.0.0 0.0.0.3

RA(config-router) #network 10.0.12.0 0.0.0.3
RA(config-router) #network 10.0.23.0 0.0.0.3
RA(config-router) #no auto-sumary

RA(config-router) #eigrp router-id 1.1.1.1

RA(config-router) fpassive-interface default
RA(config-router) #no passive-interface G0/0/0.10

O Top

Copy.

Paste





image9.png
e
Gigort

Faor P24
Fao.
Fa0
=i PePT

C 2-1921682.024 PC -152.168.1.02¢

JAFEEHREY

“Automatically Choose Connection Type

Physical  Config _CLI_ Attributes

10S Command Line Interface

BB con0 is now available

Press RETURN to get started.

RB>enable
RBfconfigure terminal

Enter configuration commands, one per line. End with CNTL/Z.
RB(config) $router eigrp 12

BB (config-router) $network 10.0.12.0 0.0.03

% Invalid input detected at '°' marker.

RB(config-router) #network 172.16.0.0 0.0.0.255
RB(config-router) #no auto-summary
RB(config-router) feigrp router-id 2.2.2.2

BB (config-router) fpassive-inter

BB (config-router) fpassive-inter

BB (config-router) fpassive-interface default
RB(config-router) #
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RC con0 is now available

Press RETURN to get started.

Press RETURN to get started!

Press RETURN to get started!

RC>enable
RCiconfigure terminal

Enter configuration commands, one per line. End with CNTL/Z.
RC(config) #network 172.16.0.0 0.0.0.255

% Invalid input detected at '°' marker.

RC(contig) frouter eigzp 12
RC(contig-zoutes) fnstwork 172.16.0.0 0.0.0.255
RC(config-router) fno auco-summary
RC(config-router)#eigrp router-id 3.3.3.3
RC(config-router) #passive-interface default

RC (config-routes)} no passive-interface G0/0/0]
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Switcn>vian 10

% Invalid input detected at '°' marker.

Switch>enable
switchfvian 10

% Invalid input detected at '°' marker.

Switchfenable
switchfconfig terminal

Enter configuration commands, one per line. End with CNTL/Z.
Switch(config)#vian 1

Switch(config-vian) $°2

switcn#

£SYS-3-CONFIG_I: Configured from console by console

Switchfconfig terminal
Enter configuration commands, one per line. End with CNTL/Z.

Switch(config) $vian 10

Switch(config-vlan) $name Carol

Switch(config-vlan) finterface Fa0/l

Switch (config-if) switchport mode trunk

Switch(config-if) finterface Fa0/2

Switch(config-if) switchport mode access

Switch(config-if)fswitchport access vian 10

Switch(config-if) $3SPANTREE-2-RECV_PVID_ERR: Received $02.1Q BEDU on non trunk FastEthernet/2
vLANL.

*SPANTREE-2-BLOCK_PVID_LOCAL: Blocking FastEthernet0/2 on VLANOOOL. Inconsistent port type.

interfece Fa0/3
Switch (config-if) #interface Fa0/3

Switch (config-if) fswitchport acc

£CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discovered on FastEthernet0/2 (10), with Switch
FastEthswitchport

% Incomplete command.

Switch(config-if) fswitch fastethswitchport
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SLINK-5-CHANGED: Interface FastEthernec0/S, changed state to down
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SLINK-5-CHANGED: Interface FastEthernet0/22, changed state to down
SLINK-5-CHANGED: Interface FastEthernec0/23, changed state to down
SLINK-5-CHANGED: Interface FastEthernet0/24, changed state to down
Switch(config-if-range)§

SLINK-5-CHANGED: Interface FastEthernet0/4, changed state to up

$LINEPROTO-5-UBDOWN: Line protocol on Interface FastEthernet0/4, changed state to up

4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on FastEtherneto/2 (10), with Switch
|
5 5@ 5 / / Copy Paste
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4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on Fastfthernetd/2 (1), with Switch
FastEtherneto/2 (10).

4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on Fastfthernetd/2 (1), with Switch
FastEtherneto/2 (10).

4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on Fastfthernetd/2 (1), with Switch
FastEtherneto/2 (10).

4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on Fastfthernetd/2 (1), with Switch
FastEtherneto/2 (10).

4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on Fastfthernetd/2 (1), with Switch
FastEtherneto/2 (10).

4CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discoversd on Fastfthernetd/2 (1), with Switch
FastEtherneto/2 (10).

Switch>enable
switchfconfig ©

Enter configuration commands, one per line. End with CNTL/Z.
Switch(config) $vian 20

Switch(config-vlan) $name Carol

Switch(config-vian) $interface Fad

% Invalid input detected at '°' marker.

Switch (config-vlan) finterface Fa0/l
Switch (config-if) #switchport mode trunk

Switch (config-if) $i

£CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discovered on FastEthernet0/2 (1), with Switch
FastEthernet0/2 (10).switchport mode trunk

Switch (config-if) #interface Fa0/2

Switch (config-if) #switchport mode access

Switch (config-if) #switchport access vian 20

Switch (config-if) fsparring-tree mod

£CDP-4-NATIVE_VLAN MISMATCH: Native VLAN mismatch discovered on FastEthernet0/2 (20), with Switch
FastEthernet0/2 (10).
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Press RETURN to get started.

SLINK-3-UPDOWN: Interface FastEthernet0/S, changed state to down
SLINEPROTO-5-UBDOWN: Line protocol on Interface FastEthernec0/S, changed state to down
SLINK-S-CHANGED: Interface GigabitEthernet/l, changed state to up

$LINEPROTO-5-UBDOWN: Line protocol on Interface GigabitEthernet0/1, changed state to up

Switch>enable
switchicont ©

Enter configuration commands, one per line. End with CNTL/Z.
Switch(config) finterface range fa0/1-2
Switch(config-if-range) fchannel-group 1 mode desirable
Switch(config-if-range)§

Creating a port-channel interface Port-channel 1

SLINEPROTO-5-UBDOWN: Line protocol on Interface FastEthernec0/2, changed state to down

SLINEPROTO-5-UEDOWN: Line protocol on Interface FastEthernet0/2, changed state to up
inte

% Invalid input detected at '°' marker.

Switch(config-if-range) finterface port-channel 1
Switch(config-if) #switch mode trunk
Switch(config-if) ¢
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Press RETURN to get started!

vepow: Interssl
SLINK-5-CHANGED: Interface FastEthernet0/l, changed state to up

>To-s-UepowN: Li|

+LINEPROTO-5-UBDOWN: Line protocol on Interface FastEthernet0/1, changed state to up

cHaNGED: Invers

sto-s-uspowy: 14 | SLINK-S-CHANGED: Interface Fastfthernetd/2, changed state to up

ALINEPROTO-5-UEDOWN: Line protocol on Interface FastEthernet0/2, changed state to up
nab1e
nf ©

nfiguracion co
ontig) $incertac
ontig-if-range) | SLINEPROTO-S-UPDOWN: Line protocol on Interface FastEthernet0/3, changed state to up
ontig-it-range)
;& porc-channel]

SLINK-5-CHANGED: Interface FastEthernet0/3, changed state to up

SLINK-3-UPDOWN: Interface FastEthernet0/2, changed state to down
>To-s-uepow: L

SLINEPROTO-5-UBDOWN: Line protocol on Interface FastEthernec0/2, changed state to down
>To-s-UepowN: Ll

SLINK-5-CHANGED: Interface FastEthernet0/2, changed state to up

d 1npuc dececcd

ALINEPROTO-5-UEDOWN: Line protocol on Interface FastEthernet0/2, changed state to up

Switch>enable
switchfconfig ©
Enter configuration commands, one per line. End with CNTL/Z.
Switch(config) finterface range fa0/1-2
Switch(config-if-range) fchannel-group 1 mode desirable
Switch(config-if-range)§

Creating a port-channel interface Port-channel 1
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BB con0 is now available

Press RETURN to get started.

T

88.1.02¢ RB>enable
RBfconfig ©

Enter configuration commands, one per line. End with CNTL/Z.
RB(config) $interface g0/0

RB(config-if)#standby 1 172.16.0.3

% Invalid input detected at '°' marker.
BB (config-if)#standby 1 172.16.0.3

% Invalid input detected at '°' marker.

BB(config-if)#standby 1 priority 110

BB (config-if) fend
=B#
£SYS-3-CONFIG_I: Configured from console by console
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RC con0 is now available

Press RETURN to get started.

RC>enable
RCfconfig ©

Enter configuration commands, one per line. End with CNTL/Z.
RC(config) $interface g0/0

RC(config-if) #standby 1 ip 172.16.03

% Invalid input detected at '°' marker.

RC(config-if) #standby 1 ip 172.16.0.3
RC(config-if) fend
rCE

£SYS-3-CONFIG_I: Configured from console by console

Copy Paste
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TRSUT(centig) FinterTace WIan-aET
The wlan-ap 0 interface is used for managing the embedded AP.

Please use the "service-module wlan-ap 0 session” command to conscle into the embedded AP
1R800 (config-1f)§

Maz 01, O SLINK-3-UPDOWN: Interface GigabitEthernetd, changed state to down
“Mar 01, 00: $LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernetd, changed
state to down

Mar 01, SLINK-S-CHANGED: Interface GigabitEthernet2, changed state to up

Mar 01, *LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet2, changed

state to up
“Mar 01, 00:23:41.2323: SPANTREE-2-RECV_PVID_ERR: Received $02.1Q BEDU on non trunk
GigabitEthernet2 VLANI.

“Mar 01, 00:23:41.232
Inconsistent port type.

SPANTREE-2-BLOCK_PVID_LOCAL: Blocking GigabitEthernet2 on VLANOOOL.

1R800 (config-if) fexit
1R800 (config) finterface GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetl
1R800 (contig-if) #shucdown

IR800 (config-if)#no shutdown

1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernet2
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface Wlan-GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetd
1R800 (config-if) fconfigure termina;

% Invalid input detected at '°' marker.

IR800 (config-if) fnostname RA
RA (confia) #no in domain—lookun
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1R800 (config-if) #shucdown
IR800 (config-if)#no shutdown

1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernet2
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface Wlan-GigabitEthernetd
1R800 (config-if)#

1R800 (config-if) fexit

1R800 (config) finterface GigabitEthernetd
1R800 (config-if) fconfigure termina;

% Invalid input detected at '°' marker.

IR800 (config-if) fnostname RA
RA(config)#no ip domain-lookup
RA(config) #interface G0/0/0.10

% Invalid input detected at '°' marker.

RA(config) $interface G0/0/0.10

% Invalid input detected at '°' marker.

RA(config)#
RA(config) #interface GigabitEthernetd
RA(config-if)#

RA(config-if) fexit

RA(config) #interface GigabitEthernetl
RA(config-if)#

RA(config-if) fexit

RA(config) #interface GigabitEthernetd
RA(config-if) fend

Bt

“Mar 01, 00:32:05.3232: SYS-3-CONFIG 3
Building configuration.

[0K]

Rt

Configured from console by consolewrite
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RBfvien aatabase

% Warning: It is recommended to configure VLAN from config mode,
as VLAN database mode is being deprecated. Please consult user
documentation for configuring VIP/VLAN in config mode.

BB (vian)§
£SYS-3-CONFIG_I: Configured from console by console

BB (vian) fexit

RPPLY completed.

Exiting.

RBfconfigure terminal

Enter configuration commands, one per line. End with CNTL/Z.

RB(config) #interface GigabitEthernec0/0

BB (config-if)#

RB(config-if) fexit

RB(config) $interface GigabitEthernec0/1

BB (config-if)#

RB(config-if) fexit

RB(config) #interface GigabitEthernec0/0

BB (config-if)#

RB(config-if) ¥exit

RB(config) #

RB(config) #

RB(config) #router rip

RB(config-router) #

BB (config-router) fend

RB#vian database

% Warning: It is recommended to configure VLAN from config mode,
as VLAN database mode is being deprecated. Please consult user
documentation for configuring VIP/VLAN in config mode.

BB (vian)§
£SYS-3-CONFIG_I: Configured from console by console

BB (vian) fexit
RPPLY completed.

Exiting.

RBfconfigure terminal

Enter configuration commands, one per line. End with CNTL/Z.
RB(config) #interface GigabitEthernec0/0

BB (config-if)§

e
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Router con0 is now available

Press RETURN to get started.

Press RETURN to get started!

Router>enable
Routerjconfigure terminal

Enter configuration commands, one per line. End with CNTL/Z.
Router (config) #hostname RC

RC(config)#no ip domain-lookup

RC(config) $interface 50/1/0

#Invalid interface type and number

RC(config) fexit

rCE

£SYS-3-CONFIG_I: Configured from console by console

(O Top

Copy.
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