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Foundation Science Coursework Part Two

2.
a) i)
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a) ii)
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a) iii)
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2 b) i)
Gradient = y ÷ x
                 = 0.1 ÷ 0.215
                 = 0.465


b) ii)
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2 d)
i)
A systematic error is a consistent, repeatable error that is due to a measuring instrument or apparatus setup.

d)
ii) 
The friction in the pulleys has to be overcome as each of the loading weights are applied. Friction will therefor decrease the force exerted on the weight W  through the tension in the strings.
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