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Lab - Accessing Network Devices with SSH

Lab - Accessing Network Devices with SSH 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.1.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.11
	255.255.255.0
	192.168.1.1

	PC-A
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.1


Objectives
Part 1: Configure Basic Device Settings
Part 2: Configure Basic Security Measures on the Router and Switch
Part 3: Configure the Router for SSH Access
Part 4: Configure the Switch for SSH Access
Part 5: SSH from the CLI on the Switch
Background / Scenario
In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.
Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands; however, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.
The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.
Note: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.
Note: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.
Required Resources
1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
1 Switch (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
1 PC (Windows 7 or 8 with terminal emulation program, such as Tera Term, and Wireshark installed)
Console cables to configure the Cisco IOS devices via the console ports
Ethernet cables as shown in the topology
Configure Basic Device Settings
In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.
Cable the network as shown in the topology.
Step 1: Initialize and reload the router and switch.
Step 2: Configure the router.
a. Console into the router and enable privileged EXEC mode.
b. Enter configuration mode.
c. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
d. Assign class as the privileged EXEC encrypted password.
e. Assign cisco as the console password and enable login.
f. Assign cisco as the VTY password and enable login.
g. Encrypt the plaintext passwords.
h. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
i. Configure and activate the G0/1 interface on the router using the information contained in the Addressing Table.
j. Save the running configuration to the startup configuration file.
Configure PC-A.
Configure PC-A with an IP address and subnet mask.
Configure a default gateway for PC-A.
Verify network connectivity.
Ping R1 from PC-A. If the ping fails, troubleshoot the connection.



1. Configure Basic Security Measures on the Router
b. Encrypt the clear text passwords.
R1(config)# service password-encryption
b. Strengthen passwords.
An administrator should ensure that passwords meet the standard guidelines for strong passwords. These guidelines could include combining letters, numbers and special characters in the password and setting a minimum length.
Note: Best practice guidelines require the use of strong passwords, such as those shown here, in a production environment. However, the other labs in this course use the cisco and class passwords for ease in performing the labs.
2. Change the privileged EXEC encrypted password to meet guidelines.
R1(config)# enable secret Enablep@55
2. Require that a minimum of 10 characters be used for all passwords.
R1(config)# security passwords min-length 10
b. Secure the console and VTY lines.
3. You can set the router to log out of a connection that has been idle for a specified time. If a network administrator was logged into a networking device and was suddenly called away, this command automatically logs the user out after the specified time. The following commands cause the line to log out after five minutes of inactivity.
R1(config)# line console 0
R1(config-line)# exec-timeout 5 0
R1(config-line)# line vty 0 4
R1(config-line)# exec-timeout 5 0
R1(config-line)# exit
R1(config)#
3. The following command impedes brute force login attempts. The router blocks login attempts for 30 seconds if someone fails two attempts within 120 seconds. This timer is set especially low for the purpose of this lab.
R1(config)# login block-for 30 attempts 2 within 120
What does the 2 within 120 mean in the above command?
2 within 120 is used to to block access if there is 2 failed login attempts within 120 seconds.
What does the block-for 30 mean in the above command?
 	Block-for 30 is used to block access for 30 seconds if there are failed login attempts.
b. Verify that all unused ports are disabled.
Router ports are disabled by default, but it is always prudent to verify that all unused ports are in an administratively down state. This can be quickly checked by issuing the show ip interface brief command. Any unused ports that are not in an administratively down state should be disabled using the shutdown command in interface configuration mode.


R1# show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/0         unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/1         192.168.1.1     YES manual up                    up      
Serial0/0/0                unassigned      YES NVRAM  administratively down down    
Serial0/0/1                unassigned      YES NVRAM  administratively down down    

Configure the Router for SSH Access
Using Telnet to connect to a network device is a security risk because all information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.
Configure device authentication.
The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the crypto key command.
Configure the domain for the device.
R1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
R1(config)# crypto key generate rsa modulus 1024
The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds) 

R1(config)#
*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled
Configure a local database username.
R1(config)# username admin privilege 15 secret adminpass (adminpass)
Note: A privilege level of 15 gives the user administrator rights.
Enable SSH on the VTY lines.
Enable Telnet and SSH on the inbound VTY lines using the transport input command.
R1(config)# line vty 0 4
R1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
R1(config-line)# login local
R1(config-line)# end
R1#
Save the running configuration to the startup configuration file.
R1# copy running-config startup-config
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
Establish an SSH connection to the router.
Start Tera Term from PC-A.
Use Tera Term to telnet to R1.
Does R1 accept the Telnet connection? Explain.
Yes
Use Tera Term, establish an SSH session to R1. Use the username admin and password adminpass. You should be able to establish an SSH session with R1.
Does R1 accept the SSH connection? Yes 
Intentionally mistype the user and password information to see if login access is blocked after two attempts.
What happened after you failed to login the second time?
I was refused by the remote host 
From your console session on the router, issue the show login command to view the login status. In the example below, the show login command was issued within the 30 second login blocking period and shows that the router is in Quiet-Mode. The router will not accept any login attempts for 14 more seconds.
R1# show login
     A default login delay of 1 second is applied.
     No Quiet-Mode access list has been configured.

     Router enabled to watch for login Attacks.
     If more than 2 login failures occur in 120 seconds or less,
     logins will be disabled for 30 seconds.

     Router presently in Quiet-Mode.
     Will remain in Quiet-Mode for 14 seconds.
     Denying logins from all sources.
R1#
After the 30 seconds has expired, SSH to R1 again and login using the SSHadmin username and Admin1p@55 for the password.
After you successfully logged in, what was displayed? 
Unauthorized access is prohibited 
Enter privileged EXEC mode and use Enablep@55 for the password.
If you mistype this password, are you disconnected from your SSH session after two failed attempts within 120 seconds? Explain.
Yes because the router was configured to disconnect you after 2 failes attempts within 120 seconds using the command, R1(config)# login block-for 30 attempts 2 within 120.

Issue the show running-config command at the privileged EXEC prompt to view the security settings you have applied.
Configure the Switch for SSH Access
In Part 3, you will configure the switch in the topology to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.
Configure the basic settings on the switch.
Console into the switch and enable privileged EXEC mode.
Enter configuration mode.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plain text passwords.
Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.
Save the running configuration to the startup configuration file.
Configure the switch for SSH connectivity.
Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.
Configure the device name as listed in the Addressing Table.
Configure the domain for the device.
S1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
S1(config)# crypto key generate rsa modulus 1024
Configure a local database username.
S1(config)# username admin privilege 15 secret adminpass (adminpasss)
Enable Telnet and SSH on the VTY lines.
S1(config)# line vty 0 15
S1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
S1(config-line)# login local
S1(config-line)# end
Establish an SSH connection to the switch.
Start Tera Term from PC-A, and then SSH to the SVI interface on S1.
Are you able to establish an SSH session with the switch?
Yes
SSH From the CLI on the Switch
The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.
View the parameters available for the Cisco IOS SSH client.
Use the question mark (?) to display the parameter options available with the ssh command.
S1# ssh ?
  -c    Select encryption algorithm
  -l    Log in using this user name
  -m    Select HMAC algorithm
  -o    Specify options
  -p    Connect to this port
  -v    Specify SSH Protocol Version
  -vrf  Specify vrf name
  WORD  IP address or hostname of a remote system
SSH to R1 from S1.
You must use the –l admin option when you SSH to R1. This allows you to log in as user admin. When prompted, enter adminpass for the password.
S1# ssh -l admin 192.168.1.1
Password: 
***********************************************
  Warning: Unauthorized Access is Prohibited!
***********************************************

R1#
You can return to S1 without closing the SSH session to R1 by pressing Ctrl+Shift+6. Release the Ctrl+Shift+6 keys and press x. The switch privileged EXEC prompt displays.
R1#
S1#
To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.
S1#
[Resuming connection 1 to 192.168.1.1 ... ]

R1#
To end the SSH session on R1, type exit at the router prompt.
R1# exit

[Connection to 192.168.1.1 closed by foreign host]
S1#

What versions of SSH are supported from the CLI?
Using the ssh -v? command on the command line for switch I found out that the different versions supported are protocol V1 and V2 
How would you provide multiple users, each with their own username, access to a network device?
The username command allows you to add in additional users with their own unique username and password.

Reflection (max 800 words): 
Write a research report comparing various Encryption standards, e.g AES, SHA, DES, RSA.  
[bookmark: _GoBack]Encryption standards
Encryption is when information or data is encoded to prevent unauthorised access it encrypts plaintext into ciphertext which is a scrambled message. The demand for encryption is ever increasing since there is much more reliance on transferring data over networks, this includes online shopping, ending personal emails and also high classified Government information. Different encryption standards are used depending on the sensitivity of the contents, sending a personal message doesn’t need the same level of encryption which highly classified government information needs. 
AES
Advanced Encryption Standard begun in 1997 when NIST worked with cryptographic community. This encryption standard was developed to be used by the US Government but also to be available to the private sector [2]Advanced Encryption Standard (AES) was the encryption standard which was used by the US Government for protecting sensitive but not classified data [3]. This encryption standard was chosen by the US Government in 2001 for its brute protection, speed, maintenance and administration [3]. The protocol is available for hardware/software with both high power and limited power such as key cards, AES uses 128, 192- and 256-bit keys all in blocks of 128 bits. [3].
SHA
SHA-1 was published in 1993 by the National Institute of Standards and Technology, it was designed as a secure hash standard. SHA-1 has 160-bits but is no longer considered safe to use since its collision in 2003, the collision was a result form a team from Google who attempted to break the algorithm. A collision is when two separate files made up of different bits produce the same hash, this stops the computer being able to identify one file from the other which attackers could use [5]. Since 2015 SHA-1 certificates have stopped being issued, SHA-1 certificates now come with a warning which advises you that the connection may not be private [5].
The newest SHA standard is SHA-2 which the SSL industry when through the “SHA-2 Transition”. SHA-2 uses 384-,224- and 512-bits. The 224-bits and 512-bits are not usually used because the 224-bits is not approved for use with publicly trusted certificates and the 512-bits is not supported by all software [5]. 
DES
DES was the encryption standard used by the US Government for protecting classified information until it was replaced with AES, through the 1990s it was the most widely used and trusted encryption algorithm, its trust was lost by many people in 1998 when a computer built by Electronic Frontier Foundation decrypted a DES encoded message in 56 hours  [4]. DES is no longer a strong enough encryption as it only uses 56 bits it would be easy for modern computers to crack. In May 2005 DES was officially withdrawn from government use however, 3DES is still approved until 2030 for sensitive government information [4]. 3DES has three DES algorithms which means that it has a key length of 168 bits, even though this encryption standard is the updated version of DES it is slower as it has a longer key length [4]. 
RSA  
Rivest-Shamir-Adleman (RSA) is an encryption standard which uses public key encryption, it is widely used for used to secure sensitive data particularly when being sent over an insecure network such as the internet [4]. RSA uses Public key encryption which was first created by Clifford Cocks who was a British mathematician, the encryption was kept secret by the GCHQ until 1997. Public key encryption uses two different but mathematically linked keys, one of these keys is public and the second must be kept private [4]. Many protocols such as secure shell, OpenPGP and SSL use RSA for their encryption and digital signature, its also used in browsers to establish secure connections over insecure networks. RSA is still used today as its hard to crack even using modern supercomputers, to decrypt the code you need to multiply the two numbers and determine the original prime numbers which is infeasible [4]. 
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