



	Site Specific Activity and Control Measures        

                                     (This section must be completed)


	Method
	Storage , Mixing & Use by Hand tools

	
	Location
	General Site

	
	Duration
	Various stages during contract duration

	
	Control
	Assessment included in RA/MP’s briefing

	Exposure Limits


	Dust generated during cutting of cement/concrete etc.

0.4mg/m3 respirable crystalline silica – 5mg/m3 dust.

	Physical Properties
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	Mixtures of dusts from cement, sand and aggregates.

	Hazard
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	Skin and eye irritation, possible skin sensitisation to chromates.

Silicosis, allergic dermatitis, skin sensitisation to chromates.

	Work Procedures/PPE
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	Dampen during cutting – Ensure adequate ventilation – wear approved respirator where ventilation and damping inadequate.

Avoid skin and eye contact – wear impervious gloves to BS EN 374, keep skin covered and wear eye protection to BS EN 166 B4

Restrict public access in dusty conditions.

	First Aid/Fire
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	Fire:  Non Combustible

Inhalation:  Remove to fresh air and rest – Seek medical attention if irritation persists.

Ingestion:  Rinse mouth with water.

Eye Contact:  Rinse with clean water – Seek medical attention if irritation persists.

Skin contact:  Wash with plenty of soap and water.                

	Storage/Disposal

[image: image5.wmf]

	N/A.

	Environmental
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	N/A
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