Router R1 Configurations
Unauthorised Access Is Strictly Prohibited
User Access Verification
Password:
R1> en
[bookmark: _GoBack]Password:
R1#show running-config
Building configuration...


Current configuration : 1438 bytes
!
! Last configuration change at 10:42:45 UTC Tue Mar 27 2018
! NVRAM config last updated at 10:43:21 UTC Tue Mar 27 2018
!
version 12.4
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
logging message-counter syslog
enable password 7 14321C0A0E08793B043B2075
!
no aaa new-model
!
dot11 syslog
ip source-route
!
!
ip cef
!
!
no ip domain lookup
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
voice-card 0
!
!
!
!
!
archive
 log config
  hidekeys
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 description PC-B L PORT CONNECTED TO ROUTER GE0/0 PORT
 ip address 172.16.2.1 255.255.255.192
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 description SWITCHPORT FA0/1 CONNECTED TO ROUTER GE0/1 PORT
 ip address 172.16.2.65 255.255.255.240
 duplex auto
 speed auto
!
interface Serial0/0/0
 no ip address
 shutdown
 no fair-queue
 clock rate 2000000
!
interface Serial0/0/1
 no ip address
 shutdown
 clock rate 2000000
!
ip forward-protocol nd
no ip http server
no ip http secure-server
!
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
!
!
!
banner motd ^C
Unauthorised Access Is Strictly Prohibited
Unauthorised Access Is Strictly Prohibited ^C
!
line con 0
 password 7 05080F1C2243
 login
line aux 0
line vty 0 4
 password 7 121A0C041104
 login
!
scheduler allocate 20000 1000
end

R1#show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0         172.16.2.1      YES manual up                    up
GigabitEthernet0/1         172.16.2.65     YES manual up                    up
Serial0/0/0                unassigned      YES unset  administratively down down
Serial0/0/1                unassigned      YES unset  administratively down down
R1#show ip route
Codes: C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2
       i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2
       ia - IS-IS inter area, * - candidate default, U - per-user static route
       o - ODR, P - periodic downloaded static route

Gateway of last resort is not set

     172.16.0.0/16 is variably subnetted, 2 subnets, 2 masks
C       172.16.2.0/26 is directly connected, GigabitEthernet0/0
C       172.16.2.64/28 is directly connected, GigabitEthernet0/1
R1#

