show running-config
DLS2#show running-config
Building configuration...

Current configuration : 3473 bytes
!
version 12.2(37)SE1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname DLS2
!
!
enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
vtp domain SoAC
vtp mode transparent
!
spanning-tree mode pvst
spanning-tree vlan 123,234 priority 24576
spanning-tree vlan 12,434,800,1010,1111,3456 priority 28672
!
!
!
!
!
!
vlan 12
name executives
!
vlan 123
name cubes
!
vlan 234
name guest
!
vlan 434
name parking
!
vlan 567
name accounting
!
vlan 800
 name native
!
vlan 1010
 name voive
!
vlan 1111
 name videonet
!
vlan 3456
 name management
!
interface Loopback0
 ip address 1.1.1.1 255.255.255.255
!
interface Port-channel1
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Port-channel12
!
interface FastEthernet0/1
 shutdown
!
interface FastEthernet0/2
 shutdown
!
interface FastEthernet0/3
 shutdown
!
interface FastEthernet0/4
 shutdown
!
interface FastEthernet0/5
 shutdown
!
interface FastEthernet0/6
 switchport access vlan 1010
 switchport mode access
 switchport nonegotiate
 shutdown
!
interface FastEthernet0/7
 switchport trunk native vlan 800
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface FastEthernet0/8
 switchport trunk native vlan 800
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface FastEthernet0/9
 switchport trunk native vlan 800
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface FastEthernet0/10
 switchport trunk native vlan 800
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface FastEthernet0/11
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 12 mode passive
 shutdown
!
interface FastEthernet0/12
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 12 mode passive
 shutdown
!
interface FastEthernet0/13
 shutdown
!
interface FastEthernet0/14
 shutdown
!
interface FastEthernet0/15
 switchport access vlan 1111
 switchport mode access
 switchport nonegotiate
 shutdown
!
interface FastEthernet0/16
 switchport access vlan 567
 switchport mode access
 switchport nonegotiate
 shutdown
!
interface FastEthernet0/17
 switchport access vlan 567
 switchport mode access
 switchport nonegotiate
 shutdown
!
interface FastEthernet0/18
 switchport access vlan 567
 switchport mode access
 switchport nonegotiate
 shutdown
!
interface FastEthernet0/19
 shutdown
!
interface FastEthernet0/20
 shutdown
!
interface FastEthernet0/21
 shutdown
!
interface FastEthernet0/22
 shutdown
!
interface FastEthernet0/23
 shutdown
!
interface FastEthernet0/24
 shutdown
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan12
 mac-address 000a.f30a.3501
 ip address 172.16.12.1 255.255.255.0
!
interface Vlan123
 mac-address 000a.f30a.3502
 ip address 172.16.123.1 255.255.255.0
!
interface Vlan234
 mac-address 000a.f30a.3503
 ip address 172.16.234.1 255.255.255.0
!
interface Vlan1010
 mac-address 000a.f30a.3504
 ip address 172.16.10.1 255.255.255.0
!
interface Vlan1111
 mac-address 000a.f30a.3505
 ip address 172.16.11.1 255.255.255.0
!
interface Vlan3456
 mac-address 000a.f30a.3506
 ip address 172.16.56.1 255.255.255.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
ntp server 172.16.56.1
!
end
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Show VTP Status
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Show etherchannel
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Show spanning-tree Summary
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Show standby brief
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DLS2§show vlan brief
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DLS28show vep status

VTP Version capable

VTP version running :
VTP Domain Name

VTP Pruning Mode :
VTP Traps Generation

Devics 10 :

Configuration last modified by 0.0.0.0 av 0-0-00 Ol

Feavuze VLAN :

VTP Operaving Mode
Maximm VIANS supporved locally
Number of exisving VLANS
Configuravion Revision

205 aigest

-

L2
2

Saac

Disabled
Dizanled
0000.0¢z0.3¢c0

© Transparent
1008

S
o

o 0xA3 0xE5 0xAC 0xDL 0x95 0xB8 0xE0 0x2F
035 055 0x3¢ OFF 0P OSE Osh Osl




image4.png
DLS2$show etherchannel summary
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DLS2#show spanning-tree summary
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DLS2#show standby brief
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