S-DC1: 
Ipconfig /all
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)ebian GNU/Linux 13 L-CD ttyl

-CD login: 7[ “["[[2

_-CD login: londonlogin

*assword:

_inux L-CD 6.12.48+deb13-amd64 #1 SMP PREEMPT_DYNAMIC Debian 6.12.48-1 (2025-09-20) x86_64

rhe programs included with the Debian GNU/Linux system are free software;
the exact distribution terms for each program are described in the
individual files in susr/share/doc/*/copyright.

ebian GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
ermitted by applicable law.
londonlogin@L-CD:™% ip a
l: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default glen 1eee
link/loopback ©0:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_lft forever preferred_lft forever
ineté - /128 scope host noprefixroute
valid_lft forever preferred_lft forever
enpoes3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 gdisc fg_codel state UF group default glen 1eee
link/ether 08:00:27:27:68:c3 brd ff:ff:ff:ff:ff:ff
altname enx0800272768c3
inet 10.0.2.15/24 brd 10.0.2.255 scope global dynamic noprefixroute enpe@s3
valid_lft 85626sec preferred_lft 74826sec
inete 0o /64 scope global dynamic mngtmpaddr noprefixroute
valid_lft 85623sec preferred_lft 13623sec
ineté oo oo o0 /64 scope link
valid_lft forever preferred_lft forever
3: enpos8: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 gdisc fg_codel state UP group default glen 1006
link/ether 08:00:27:dc:83:e8 brd ff:ff:ff:ff:ff:ff
altname enx080027dc83e8
inet6 ‘oo cialoc oo in o0 /64 scope link
valid_lft forever preferred_lft forever
}: enpos9: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fg_codel state UP group default glen 1000
links/ether 08:00:27:22:a32:34 brd ff:ff:ff:ff:ffoff
altname enx08002722a234
inet 20.0.0.2/30 brd 20.0.0.3 scope global enpess
valid_lft forever preferred_lft forever
ineté - o /64 scope link proto kernel_l11
valid_lft forever preferred_lft forever
enpoes10: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 gdisc fg_codel state UP group default glen 1000
link/ether 08:00:27:07:1c:24 brd ff:ff:ffff:ffoff
altname enx080027071c24
inet 192.168.2.1/24 brd 192.168.2.255 scope global enposie
valid_lft forever preferred_lft forever
inete oo cooooo o ioion oo /64 scope link proto kernel_11
valid_lft forever preferred_lft forever
londonlogin@L-CD: ™% _
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ser preferred_lft for
ineté - /128 scope host noprefixroute
valid_lft forever preferred_lft forever
2: enpos3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 gdisc fg_codel state UP group default glen 1000
links/ether o 0:27:27:68:c3 brd ff:ff:ff:ff:ff:ff
altname enxe800272768c3
inet 10.0.2.15/24 brd 10.0.2.255 scope global dynamic noprefixroute enpes3
valid_lft 85626sec preferred_lft 74826sec
ineteé oo /64 scope global dynamic mngtmpaddr nopref
alid_lft 85623sec preferred_lft 13623sec
ineté oo oo aioi oo /64 scope link
valid_lft forever preferred_lft forever
3: enposs: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 gdisc fg_codel state UP group default glen 1000
link/ether 08:00:27:dc:83:e8 brd ff:ff:ff:ff:ff:ff
altname en
inete ‘oo ctaloco o ioooain o0 /64 scope link
valid_lft forever preferred_lft forever
enpoess BROADCAST,MULTICAST,UP,LOKER_UP> mtu 1508 gdisc fg_codel state UP group default glen 1008
links/ether 00:27:22:a2:34 brd ff:ff:ff:ff:ff:ff
altname enx@B8002722a234
inet 20.0.0.2/30 brd 20.0.0.3 scope global enpos3
valid_lft forever preferred_lft forever
ineté .. . /64 scope link proto kernel_1ll
valid_lft forever preferred_lft forever
enpos10: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 gdisc fg_codel state UP group default glen 1000
link/ether 08:00:27:07:1c:24 brd ff:ff:ff:ff:ff:ff
altname enxe80027071c24
inet 192.168.2.1/24 brd 192.1668.2.255 scope global enpeésie
valid_1ft forever preferred_lft forever
inete . oo /64 scope link proto kernel_l1l
valid_1ft forever preferred_lft forever
londonlogin@L-CD: ™% ping 192.168.1.10
"ING 192.168.1.10 (152.168.1.10) 56(84) bytes of data.
4 hytes from 192.168.1.10: icmp_seg=1 tt1=127 time=3.00 ms
54 bytes from 192.168.1.16: icmp_seq=2 tt1=127 time=0.528 ms
4 hytes from 192.168.1.10: icmp_seq=3 tt1=127 time=0.560 ms
C

-~ 192.168.1.10 ping statistics ---
3 packets transmitted, 3 received, 0% packet loss, time 2022ms
“tt min/savg/max/mdev = ©.528/1.361/2.995/1.155 ms
londonlogin@L-CD: ™% ping 192.168.1.1

*ING 192.168.1.1 (1392.168.1.1) 56(84) bytes of data.

54 bytes from 192.168.1.1: icmp_seg=1 tt1=127 time=3.09 ms

54 hytes from 192.168.1.1: icm 0.342 ms

54 bytes from 192.168.1.1: icmp_: tt time=0.294 ms
C

192.168.1.1 ping statistics ---
ckets transmitted, 3 r
“tt min/avg/max/mdev
londonlogin@L-CD: ™%

o om@m ™ o n =

15:58
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BN Administrator

iindows IP Configuration ~
Host Name . . . . . . . . . . . . : S-DC
Primary Dns Suffix . . . . . . . : swansea.acca
Node Type . . - - = « « - - . . . : Hybrid
IP Routing Enabled. . . . . . . . : No
WINS Proxy Enabled. . . . . . . . : No

DNS Suffix Search List. . . . . . swansea.acca

soac.local
Ethernet adapter Internet:

soac.local

Intel(R) PRO/100@ MT Desktop Adapter
©8-00-27-1A-80-9D

Yes

Yes
£d17:625c:¥037:2:cfd@:7c37:27cc:3d7(Preferred)
fe80: :e147:b674:a231:8284%7 (Preferred)
10.0.2.15(Preferred)

255.255.255.0

29 September 2025 15:37:11

3@ September 2025 15:37:10

fe80::2%7

Connection-specific DNS Suffix -
Description . . . . . . . . . . .
Physical Address. . . . . . . . .
DHCP Enabled. . . . . . .
Autoconfiguration Enabled . . . .
R 1Pve Address. . . . . .
Link-local IPv6 Address . . . . .
IPv4 Address. . . . . . . . . . .
Subnet Mask . . . . . . . . . . .
Lease Obtained. . . . . . . . . .
Lease Expires . . . . . . . . . .
Default Gateway . . . . . . . . .

1©6.©.2.2
DHCP Server . . . . . . « « « .+« . 10.©.2.2
DHCPVv6 IAID . . « e & e = = = = 101187623

DHCPv6 Client DUID. . . . . . . .
DNS Servers . . . . . . . . . . .

©0-01-00-01-30-66-31-06-88-00-27-1A-80-9D

127.0.0.1
NetBIOS over Tcpip. . . . . . . . : Enabled

Fthernet adapter IntSwa:

Connection-specific DNS Suffix .
Description . . . . . . . . . . .
Physical Address. . . . . . . . .
DHCP Enabled. . . . . . .
Autoconfiguration Enabled . . . .
Link-local IPv6 Address . . . . .
IPv4 Address. . . . . . .+« « .« .+
Subnet Mask . . . . . . . . . . .
Default Gateway . . . . . . . . .
DHCPv6 IAID . . 168296487 v

B O m O = oo

Intel(R) PRO/100@ MT Desktop Adapter #2
©8-00-27-7D-19-D1

No

Yes
fe80::ad8d:9a21:a0c7:250c%13(Preferred)
192.168.1.1(Preferred)

255.255.255.0

~ E & 9% 5900005 FA
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NetBIOS over Tcpip. Enabled

Etherneﬁkadapter IntSwa:

Connection-specific DNS Suffix . :
Description . . . . . . . . . .

Physical Address. . . . . . . . .
DHCP Enabled. . . . . . . . . . .
Autoconfiguration Enabled . . . .

Intel(R) PRO/1©0©©@ MT Desktop Adapter #2
e8-e0-27-7D-19-D1
No

Yes
Link-local IPv6 Address . . . . . : fe8@::ad8d:9a21:a@c7:250c%13(Preferred)
IPv4 Address. . . . . .+« « « « .« 192.168.1.1(Preferred)

Subnet Mask . . . . . . . . . . . : 255.255.255.0

Default Gateway . . . . . . . . .

DHCPV6 IAID . . . . . . . . . . . 168296487

DHCPv6 Client DUID. . . . . . . . ©0-01-00-01-30-66-31-06-08-00-27-1A-80-9D

DNS Servers . . . . . .« « « « « = 1
127.0.0.1
NetBIOS over Tcpip. . . . . . . . : Enabled

“thernet adapter External:

Connection-specific DNS Suffix . :
Description . . . . . . . . . .

Physical Address. . . . . . . . .
DHCP Enabled. . . . . . . . . . .
Autoconfiguration Enabled . . . .

Intel(R) PRO/100© MT Desktop Adapter #3
©8-00-27-72-4F-05
No

Yes
Link-local IPv6 Address . . . . . : fe80::53d6:6f1:dd51:786c%15(Preferred)
IPv4 Address. . . . . . . . . . . 20.0.0.1(Preferred)
Subnet Mask . . . . . . . . . . . : 255.255.255.252
Default Gateway . . . . . . . . .
DHCPv6 IAID . . . . . . . . . . . 185073703
DHCPv6 Client DUID. . . . . . . . ©0-01-00-01-30-66-31-06-08-00-27-1A-80-9D

DNS Servers . . . . . . +« +« « +« 1
192.168.1.1
NetBIOS over Tcpip. . . . . . . . : Enabled

\Users\Administrator>ping 192.168.1.10

>inging 192.168.1.10 with 32 bytes of data:
Reply from 192.168.1.10: bytes=32 time<ims
eply from 192.168.1.10: bytes=32 time<ims
Reply from 192.168.1.1 bytes=32 time<ims

>ing statistics for 192.168

10:
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Connection-specific DNS Suffix
Description . . . . . . . . .
Physical Address. . . . . . .

Intel(R) PRO/100@ MT Desktop Adapter #3
©8-00-27-72-4F-05

DHCP Enabled. . . . . . . . . No
Autoconfiguration Enabled . . Yes
Link-local IPv6 Address . . . . . fes80 53d6:6f1:dd51:786c%15(Preferred)

IPv4 Address. . . . . . .+« « « .+

20.0.0.1(Preferred)

Subnet Mask . . . . . . . . . . . : 255.255.255.252
Default Gateway . . . . . . . . .
DHCPv6 IAID . . - - - - . . . : 185073703

DHCPv6 Client DUID. . . . . . . .
DNS Servers . . . . . . . . . . .

©0-01-00-01-30-66-31-06-88-00-27-1A-80-9D

1
192.168.1.1
NetBIOS over Tcpip. . . . . . . . : Enabled

\Users\Administrator>ping 192.168.1.10

inging 192.168.1.10 with 32 bytes of data:

eply from 192.168.1.10: bytes=32 time<ims TTL=128
eply from 192.168.1.10: bytes=32 time<ims TTL=128
eply from 192.168.1.10: bytes=32 time<ims TTL=128

*ing statistics for 192.168.1.10

Packets: Sent - 3, Received - 3, Lost - © (@% loss),
\pproximate round trip times in milli-seconds:

Minimum = ©ms, Maximum = ©ms, Average = ©Oms
“ontrol-C

*C

\Users\Administrator>ping 192.168.2.1

>inging 192.168.2.1 with 32 bytes of data:

eply from 192.168.2.1:
eply from 192.168.2.1
eply from 192.168.2.1:

bytes=32 time<ims
bytes=32 time<ims
bytes=32 time<ims

’ing statistics for 192.168.2.1:

Packets: Sent = 3,

Received = 3, Lost = © (@% loss),

\pproximate round trip times in milli-seconds:
Minimum = ©ms, Maximum = ©ms, Average = ©Oms

“ontrol-C

*C

\Users\Administrator>,

H @ =B © m & T

~

15:52
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