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1 Three-Phase Inverter
1a: a - broader
1b: b – 40
1c: a – Yes
Load current = 26.5mA AC
2 Over-Current Protection
2b: c
2c: d
2d: b
2e: b
2f: a
Single-Phase Synchronous Motor
1: a
2: d
3: b
[bookmark: _GoBack]4: a
5: c
6: b
Fault ‘B’ was inserted into the circuit and it was found that circuit 7 was faulty. When the motor is connected to circuit 7 the voltage is reduced to a minimum. It was found that 7.1 is shorted with 7.6.


