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Safety must always be a priority in the hotel industry. The Fire Protection Systems seek to guarantee the safety of the users and the operability of the installation, which is why it is essential that the maintenance of the facilities is rigorous and carried out by approved companies. The seriousness that can lead to the generation of a fire in an accommodation building, especially in the high tourist season, with the high density of customers, makes it necessary to raise the importance of a consolidated strategy in which preventive policies should prevail, being essential the training and information of all the staff of the establishment.
When a fire breaks out, the lives of people in the hotel depend on passive and active safety systems and protections. There are also factors that affect the safety of people, such as: sleeping guests, lack of knowledge of the facilities and the size of these. 
According to statistics, the most common causes of fire in hotels are but also another more like absence of compartmentalization, flammable flame and gas conductors ,a/c ducts and elevators, existence of gaps and vertical communications, ducts for evacuation of dirty clothes, open stairs.
In the UK, the applicable regulations and standards for fire protection are becoming more rigorous, where fixed fire systems and alarm systems are already requested. There are 2 types of fire protection, passive protection and active protection. Discovery systems similar as fire admonitions should be maintained and tested to insure that they ’re always ready to reply and give guests and staff the stylish chance of dealing with the fire to escaping. Admonitions must be loud enough and call points should be placed constantly throughout the demesne. exigency lighting, firefighting outfit and fire safety signage should all be easily marked, maintained and rightly specified for the hotels.
Passive or structural protection refers to the types of building materials, whether combustible materials treated with fire retardants or non-combustible materials. These passive elements do not act directly on the fire, but can compartmentalize its development, the wall, prevent the fall of a building covering metal structures or allow evacuation. 
Active protection refers to fire-fighting systems that do have a direct action on fire, such as: fire extinguishers, detectors, hoses, sprinklers, hydrants, pumps, etc. 
Hotels must have and comply with the minimum safety and security requirements to reduce risk, which are: fire detection system, fire protection system, escape or evacuation routes.  
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