	[bookmark: _Hlk37337169]Activity to be Assessed
	Assessment Number

	Working at height from a Scaffolding 
	

	Persons undertaking or affected by the activity

	

	
	
	Employees
	
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Falling from height 
	3
	5
	15

	2
	Materials falling
	4
	5
	20

	3
	Plant falling
	3
	5
	15

	4
	Equipment falling
	2
	5
	10

	5
	Trips & Slips
	5
	2
	6

	6
	
	
	
	

	Existing Control Measures / Additional Control Measures Required

	1
	Brick guards

	2
	Handrails

	3
	Safety netting

	4
	Gates on openings

	5
	Clean, muck free boards and ladders

	6
	Harness’ to be worn by all working on scaffolding 

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Falling from height 
	1
	4
	4

	2
	Materials falling
	2
	3
	6

	3
	Plant falling
	2
	3
	6

	4
	Equipment falling
	2
	3
	6

	5
	Trips & Slips
	2
	2
	4

	6
	
	
	
	

	Name  Harri Morgan
Position  Quantity Surveyor 
	Signed
H.Morgan

	   Date of Completion: 
09.04.2020

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury

	Reviewed by:
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk


Risk Assessments
	Activity to be Assessed
	Assessment Number

	Manual handling
	

	Persons undertaking or affected by the activity

	

	
	
	Employees
	
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Weight of item too heavy causing lower back problems
	3
	3
	9

	2
	Fragile materials breaking when lifting causing sharp edges to show
	3
	3
	9

	3
	Size of load obstructing employees vision, causing a slip or trip
	3
	2
	6

	4
	Moving items that include liquid, if spilt could cause a fall
	2
	2
	4

	5
	Moving of hazardous substances could cause harm if contact is made with skin and or eyes
	2
	4
	8

	6
	Carrying materials on stairs could cause loss of balance resulting in a fall
	3
	2
	6

	Existing Control Measures / Additional Control Measures Required

	1
	Ensure that the route to be taken while lifting is clear of obstructions before the task takes place

	2
	Team lifting to be used when loads are too heavy or awkward for one person

	3
	All site staff have received the relevant instructions and training to complete the manual handling tasks 

	4
	Lifting straps to be used where applicable

	5
	Where possible, lighten the load when carrying materials up or down stairs to maximise balance

	6
	When handling items of liquid, ensure the lids are securely fastened to avoid spillage

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Weight of item too heavy causing lower back problems
	2
	3
	6

	2
	Fragile materials breaking when lifting causing sharp edges to show
	2
	3
	6

	3
	Size of load obstructing employees vision, causing a slip or trip
	3
	2
	6

	4
	Moving items that include liquid, if spilt could cause a fall
	1
	2
	2

	5
	Moving of hazardous substances could cause harm if contact is made with skin and or eyes
	1
	3
	3

	6
	Carrying materials on stairs could cause loss of balance resulting in a fall
	2
	2
	4

	Name  Harri Morgan
Position  Quantity Surveyor 
	Signed
H.Morgan

	   Date of Completion: 
14.04.2020

	Activity to be Assessed
	Assessment Number

	Excavation for foundations
	

	Persons undertaking or affected by the activity

	

	
	
	Employees
	
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Collapse of the sides of excavation
	4
	5
	15

	2
	Material falling onto the people working in the excavation
	3
	5
	15

	3
	People and vehicles falling into the excavation
	2
	5
	10

	4
	Undermining of nearby structures causing their collapse into the excavation
	3
	5
	15

	5
	Damage to underground services during the excavation
	2
	4
	8

	6
	Ingress of water causing flooding
	2
	3
	6

	Existing Control Measures / Additional Control Measures Required

	1
	Batter sides of the trench at a safe angle to avoid collapse

	2
	Ensure all stored soil, plant, materials are not close to the excavation.

	3
	Barriers around edge s of the trench 

	4
	Keep all vehicles away from the area of excavation

	5
	Before excavation begins ensure you have reviewed the service plans to locate any underground services.

	6
	Installation of pump to stop the flooding of the excavation. 

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Collapse of the sides of excavation
	2
	4
	10

	2
	Material falling onto the people working in the excavation
	2
	3
	8

	3
	People and vehicles falling into the excavation
	2
	3
	8

	4
	Undermining of nearby structures causing their collapse into the excavation
	2
	3
	4

	5
	Damage to underground services during the excavation
	1
	3
	4

	6
	Ingress of water causing flooding
	1
	2
	3

	Name  Harri Morgan
Position  Quantity Surveyor
	Signed
H.Morgan

	   Date of Completion: 

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5




