Valentin Latinov Miladinov /2024732/
Switching and Routing Exam
21/08/2024

R1#sh run
Building configuration...

Current configuration : 6548 bytes
!
! Last configuration change at 14:48:32 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
ip domain name swre-lab.com
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-4059697185
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-4059697185
 revocation-check none
 rsakeypair TP-self-signed-4059697185
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-4059697185
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 34303539 36393731 3835301E 170D3234 30373330 31353330
  34385A17 0D333430 37333031 35333034 385A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D34 30353936
  39373138 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100A32B FC3D155F 42C26DDA CBEC4540 2BF5F983 B4C95A45 B8756CDC
  01005EDA C4B1BD73 5BD671DB 596699BF E9A7E07E B421C4A8 26E7F3B3 01DA5CFA
  88D5F667 AD59AD64 CBE47E6A 6A7CDFB7 1FEA990A EE00C968 1F57AECF F59B8FCC
  CB1379ED 01B441B7 D4725D3B 2EBFE1BD 19D2AC83 EC4370E7 987638CB AFFF52B8
  9DBB7044 DD6FD9CE 7C4C43CA 1DF5D9B4 161BD4E5 C0320F79 7FE42E9F 65519364
  2F1EFEF4 A3540C26 04FEC25A FE6763F7 1F6E068B 8B3A34CA E8341F7D 64E697DE
  D5BDE1E2 9BB4476C C57D009B 254FDFCE A9F6AA44 4939945F C7072599 35117AA3
  1E01F803 5CD1E33B C7896D0C 7FA112C3 147FBCFB 377DCAC8 AF7E340B B28C6EAB
  5AB76DD6 3D790203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 142872CB F3F5D87B 84ED91A1 2EB284B2 574C2CA7
  AE301D06 03551D0E 04160414 2872CBF3 F5D87B84 ED91A12E B284B257 4C2CA7AE
  300D0609 2A864886 F70D0101 05050003 82010100 44A360D9 D4FA8A2E 72F69247
  F8592EBA 64734E68 6F96F944 B4BA7982 EC904B0D E05452C9 BC9EA930 6C6CB912
  71C3534C DECCDC4B D2FCDFFE FDB23F01 12F3FEDB 6D5B026C 991240EC A29BCD53
  9E1D7D6D 91BF0E07 5CDA88B0 3072F3CA AB38A7B3 04DD1853 5338CB14 6B5A13A6
  82F317DC 42E91C6E 8378B29E C7419BA5 C4A4C882 EE35A75C B5665F2C 52E09B91
  B336CC93 2BBB7B33 3CD075CF 215639FA 26C83EA6 C1BF4769 167D75C0 3C2985CF
  EAA044B6 21B92742 8365651B 0D8D864B 18880FE2 E3B043E2 D6607035 7A45B55E
  40CE8D0F D34BF816 30D776B4 2E4D11B9 12CAD95F BAD14B3A 912713D6 E3836622
  34622961 07F92FA3 E62AC05F 1EC9DA22 B097FA76
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0MX
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
enable secret 9 $9$ox3Gez0Kx82PiU$aFf5JEW2.PQmh9JgA.xG1g/1R3yZlldPMk3V2n/SZq6
!
username cisco privilege 15 secret 9 $9$afc2wqiuNbMgGE$q/UrYoXZajFZe9WeYKuiMONSUoqxOjUkWvb1LGE9tqQ
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.101.1 255.255.255.0
!
interface GigabitEthernet0/0/0
 no ip address
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 negotiation auto
!
interface GigabitEthernet0/0/1.22
 encapsulation dot1Q 22
 ip address 192.168.90.1 255.255.255.0
!
interface GigabitEthernet0/0/1.23
 encapsulation dot1Q 23
 ip address 192.168.100.1 255.255.255.0
!
interface GigabitEthernet0/0/1.24
 encapsulation dot1Q 24
 ip address 192.168.110.1 255.255.255.0
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 password 7 110A1016141D5A5E57
 login
 stopbits 1
line aux 0
line vty 0 4
 password 7 110A1016141D5A5E57
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#sh ip int bri
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES manual down                  down
GigabitEthernet0/0/1   unassigned      YES unset  down                  down
Gi0/0/1.22             192.168.90.1    YES manual down                  down
Gi0/0/1.23             192.168.100.1   YES manual down                  down
Gi0/0/1.24             192.168.110.1   YES manual down                  down
GigabitEthernet0/0/2   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/3   unassigned      YES NVRAM  administratively down down
Serial0/1/0            unassigned      YES NVRAM  administratively down down
Serial0/1/1            unassigned      YES NVRAM  administratively down down
Loopback0              209.165.101.1   YES manual up                    up
R1#
S1#sh run
Building configuration...

Current configuration : 4774 bytes
!
! Last configuration change at 16:59:43 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$jOO8o7jX5k264q$xcpBeoFLNOTPg5PJee6wcObwHw6Vk6FvK2KYBqPhTQU
!
username cisco privilege 15 secret 9 $9$BDPzK2K4pRLWam$TKZzlA16M7nOwq88HO4YTgb7S06AVQuDvze8Adboi0Q
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/2
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/3
 switchport access vlan 25
 switchport trunk native vlan 26
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/4
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/5
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 22
 switchport mode access
 switchport port-security maximum 3
!
interface GigabitEthernet1/0/7
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/8
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/9
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/10
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/11
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/12
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/13
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/14
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/15
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/16
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/17
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 23
 switchport mode access
 switchport port-security maximum 3
!
interface GigabitEthernet1/0/19
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/20
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/21
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/22
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/23
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/24
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/25
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/26
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/27
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface GigabitEthernet1/0/28
 switchport access vlan 25
 switchport mode access
 switchport port-security maximum 3
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan24
 ip address 192.168.110.2 255.255.255.0
!
interface Vlan26
 no ip address
!
ip default-gateway 192.168.110.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 070C285F4D06485744
 login
line vty 0 4
 password 7 070C285F4D06485744
 login
 transport input ssh
line vty 5 15
 password 7 1511021F07257A767B
 login
 transport input ssh
!
end

S1#sh ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
Vlan24                 192.168.110.2   YES manual up                    down
Vlan26                 unassigned      YES unset  up                    down
GigabitEthernet1/0/1   unassigned      YES unset  administratively down down
GigabitEthernet1/0/2   unassigned      YES unset  administratively down down
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
S1#sh vlan bri

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
22   Student                          active    Gi1/0/6
23   Teacher                          active    Gi1/0/18
24   Management                       active
25   Library                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/7
                                                Gi1/0/8, Gi1/0/9, Gi1/0/10
                                                Gi1/0/11, Gi1/0/12, Gi1/0/13
                                                Gi1/0/14, Gi1/0/15, Gi1/0/16
                                                Gi1/0/17, Gi1/0/19, Gi1/0/20
                                                Gi1/0/21, Gi1/0/22, Gi1/0/23
                                                Gi1/0/24, Gi1/0/25, Gi1/0/26
                                                Gi1/0/27, Gi1/0/28
26   Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S1#

User Access Verification

Password:
S2>en
Password:
S2#sh run
Building configuration...

Current configuration : 3712 bytes
!
! Last configuration change at 16:22:19 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$WDGhmzj8aKTYF4$TYSIAWf.hgrSnfVxlGdorltlkJ/qciv3luVktR7uK3g
!
username cisco privilege 15 secret 9 $9$AfiJ.6.cYCnX9y$4PTzreUJFzJH3ChSB0rjpCbkYNMkR5a1u5YJUO.vYfU
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/2
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/3
 switchport access vlan 25
 switchport trunk native vlan 26
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/4
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/5
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 22
 switchport mode access
 switchport port-security maximum 3
!
interface GigabitEthernet1/0/7
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/8
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/9
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/10
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/11
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/12
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/13
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/14
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/15
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/16
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/17
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 23
 switchport mode access
 switchport port-security maximum 3
!
interface GigabitEthernet1/0/19
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/20
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/21
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/22
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/23
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/24
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/25
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/26
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/27
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/28
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 094F471A1A0A464058
 login
line vty 0 4
 password 7 094F471A1A0A464058
 login
 transport input ssh
line vty 5 15
 password 7 060506324F41584B56
 login
 transport input ssh
!
end

S2#sh ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
GigabitEthernet1/0/1   unassigned      YES unset  administratively down down
GigabitEthernet1/0/2   unassigned      YES unset  administratively down down
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
S2#sh vlan bri

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
22   Student                          active    Gi1/0/6
23   Teacher                          active    Gi1/0/18
24   Management                       active
25   Library                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/7
                                                Gi1/0/8, Gi1/0/9, Gi1/0/10
                                                Gi1/0/11, Gi1/0/12, Gi1/0/13
                                                Gi1/0/14, Gi1/0/15, Gi1/0/16
                                                Gi1/0/17, Gi1/0/19, Gi1/0/20
                                                Gi1/0/21, Gi1/0/22, Gi1/0/23
                                                Gi1/0/24, Gi1/0/25, Gi1/0/26
                                                Gi1/0/27, Gi1/0/28
26   Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
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