Advanced networking lab 3
Fill the tables with appropriate information/ details.
	Specification

	Network: A

	Network: B

	Network: C


	Network Address

	192.168.100.0
	192.168.100.96
	192.168.100.64

	Subnet Mask

	255.255.255.192
	255.255.255.252/30
	255.255.255.224/27

	No. of asked hosts/subnet

	
50

	
2

	2
0


	No. of usable hosts/ subnet

	
62
	
2
	
30

	First Usable Host (FUH)

	
192.168.100.1
	
192.168.100.97
	
192.168.100.65

	Last Usable Host (LUH)

	192.168.100.62
	192.168.100.98
	192.168.100.94

	Broadcast Address

	192.168.100.63
	192.168.100.99
	192.168.100.95


















	
Addressing table

	Device
	Requirement
	IP address
	Subnet Mask
	Gateway

	PC1
	1st Usable Host Network: A
	192.168.100.1
	255.255.255.192
	192.168.100.62

	Laptop1
	2nd Usable Host Network: A
	192.168.100.2
	255.255.255.192
	192.168.100.62

	PC2
	1st Usable Host Network: B
	192.168.100.97
	255.255.255.252
	192.168.100.98

	PC3
	1st Usable Host Network: C
	192.168.100.65
	255.255.255.224
	192.168.100.94

	Laptop0
	2nd Usable Host Network: C
	192.168.100.66
	255.255.255.224
	192.168.100.94

	RAI G0/0/0
	Last Usable Host Network: A
	192.168.100.62
	255.255.255.192
	N/A

	RIBC G0/0/1
	Last Usable Host
Network: B
	192.168.100.98
	255.255.255.252
	N/A

	RIBC G0/0/0
	Last Usable Host
Network: C
	192.168.100.94
	255.255.255.224
	N/A



Initialise All the switches 
Delete the old VLAN Database in All switches (S0, S1 &SW2) and reload 
[bookmark: _GoBack]Erase startup-config
Reload Switch
Show Flash 
Delete.vlan.dat
Sh flash – confirm that the file has been deleted
Reload
Check the switches with the appropriate command to find the old vlan database is deleted. 
Sh Vlan (The only vlans should be in the database is 1002 to 1005 as legacy vlans) You are able to create up to 1001 vlans and then the extended vlan database ranges from 1006 to 4094 and then also the native vlan which is 1 

Line console password – ciscocon
Line VTY password – ciscovty 
Username – admin – password: cisco1234
