Basic Command List
Always use cisco or class as password
? 	Help
Tab	autofill 

Three modes of opearation
Router> 		User mode
Router#		Privilege  user exec mode
Router(config)#		global config mode

Would like to enter initial configuration mode[yes/no]: no
If you entered yes to above question press Ctrl+c at any time to exit.
Commands

Router>?						Help
Router>sh? 						List you commands with sh
Router>enable or en					user to privliege exec  mode
Router#show running-config or sh run			to view running config
Router#show startup-config or sh start			to view start config
Router#show flash: 					to view flash memory
Router#copy running-config  startup-config		to copy current config into NVRAM
Router#copy run start					to copy current config into NVRAM
Router#wr						to copy current config into NVRAM
Router#copy startup-config  running-config		to retrieve NVRAM contant
Router#erase startup					to erase NVRAM
Router#reload						to restart the router
Router#show ip route					to view routing table
Router#show ip interface brief				to view interface in brief
Router#show ip interface <int no>			to view interface in detail
Router#show controllers  interface <int no>		to view DCE/DTE interface 
Router#debug  ip <>					to troubleshoot
Router#undebug all or u all				to stop all debugging
Router#configure terminal or conf t			to enter golbal config mode
Router(config)# hostname ####				to set host name
Router(config)# enable password ______		to set clear password
Router(config)# enable secret ______			to set encrypt  password
Router(config)#no ip domain lookup			disable dns lookup
Router(config)# ip routing				enable routing
Router(config)# banner motd				to set Banner
Router(config)#line con 0				to set console password
Router(config-line)#login
Router(config-line)#password cisco
Router(config-line)#exit
Router(config)#line vty  0 4				to set vty line password
Router(config-line)#login
Router(config-line)#password cisco
Router(config-line)#exit
Router(config)#interface Serial 0 or (0/0)		to configure serial interface
Router(config-int)# ip address A.A.A.A M.M.M.M
Router(config-int)# line description <your description>
Router(config-int)#clockrate 64000			Only at DCE end 
Router(config-int)#no shutdown
Router(config-int)#exit
Router(config)#interface ethernet0 or fastethernet0/0	to configure ethernet interface
Router(config-int)# ip address A.A.A.A M.M.M.M
Router(config-int)# line description <your description>
Router(config-int)#no shutdown
Router(config-int)#exit




If you have done a mistake and want to remove the configuration, add NO in front.
Example: Router(config)# hostname R1			
R1(config)# no hostname R1
Router(config)# 

To configure static router
Router(config)# ip route N.N.N.N  M.M.M.M (destination network) S0/0 (local interface) or Next hop ip address 

To configure routing protocol RIP v1
Router(config)# router rip
Router(config-router)#network N.N.N.N
Router(config-router)# exit

To configure routing protocol RIP v2
Router(config)# router rip
Router(config)# version 2
Router(config-router)#network N.N.N.N
Router(config-router)# exit

	



