Typical IBM instruction cycle segmentation
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Figure 3.14 The reservation table for a typical Add or a Multiply function evaluated in the instruction pipeline of IBM 360/91.
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Figure 3.13 Functional segmentation of a typical storage-to-register floating-point instruction in the IBM 360/91.




