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Vertical graduated Pole

Meter rule



At different height intervals, you must make an horizontal measurement, from the graduated pole to the bank and enter the readings in the table below, for later processing using excel.







	Bank
	height
	Distance bank to pole
	comments

	left
	right
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



Once you have plotted the profile you can ascertain the bank’s levels of structural stability by reference to the curve below
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