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1#show ip int brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES unset  administratively down down
GigabitEthernet0/0         141.240.10.1    YES manual up                    up  
GigabitEthernet0/1         141.240.11.1    YES manual up                    up  
Serial0/0/0                unassigned      YES unset  administratively down down
Serial0/0/1                unassigned      YES unset  administratively down down
R1#

R1#show run
R1#show running-config
Building configuration...

Current configuration : 1448 bytes
!
! Last configuration change at 14:30:34 UTC Tue Jan 14 2020
!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$talP$DmzisEnMBduA.1xK450pA/
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
multilink bundle-name authenticated
!
!
cts logging verbose
!
!
license udi pid CISCO2901/K9 sn FCZ1930C0TB
!
!
!
redundancy
!
!
!
!
!
!
interface Embedded-Service-Engine0/0
 no ip address
 shutdown
!
interface GigabitEthernet0/0
 ip address 141.240.10.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 ip address 141.240.11.1 255.255.255.0
 duplex auto
 speed auto
!
interface Serial0/0/0
 no ip address
 shutdown
 clock rate 2000000
!
interface Serial0/0/1
 no ip address
 shutdown
 clock rate 2000000
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
control-plane
!
!
banner motd ^Cwarning unatorized access prohibited^C
!
line con 0
 exec-timeout 0 0
 password 7 05080F1C2243
 login
line aux 0
line 2
 no activation-character
 no exec
 transport preferred none
 transport output pad telnet rlogin lapb-ta mop udptn v120 ssh
 stopbits 1
line vty 0 4
 password 7 104D000A0618
 login
 transport input none
line vty 5 15
 password 7 104D000A0618
 login
 transport input none
!
scheduler allocate 20000 1000
ntp server pnpntpserver.uni.local
!
End

Switch>
Switch>enable
Switch#host name Switch1
        ^
% Invalid input detected at '^' marker.

Switch#hostname Switch1
        ^
% Invalid input detected at '^' marker.

Switch#config terminal
Enter configuration commands, one per line.  End with CNTL/Z.
Switch(config)#host name Switch1
                         ^
% Invalid input detected at '^' marker.

Switch(config)#hostname Switch1
Switch1(config)#no ip domain-lookup
Switch1(config)#enable secret class
Switch1(config)#line console 0
Switch1(config-line)#password cisco
Switch1(config-line)#login
Switch1(config-line)#exit
Switch1(config)#line vty 0 15
Switch1(config-line)#password cisco
Switch1(config-line)#login
Switch1(config-line)#servivce password-encryption
                       ^
% Invalid input detected at '^' marker.

Switch1(config-line)#service password-encryption
Switch1(config)#banner MOTD "warning anautorize access"
Switch1(config)#exit
Switch1#
*Mar  2 01:22:00.472: %SYS-5-CONFIG_I: Configured from console by console
Switch1#show ip
% Ambiguous command:  "show i"
Switch1#config terminal
Enter configuration commands, one per line.  End with CNTL/Z.
Switch1(config)#interface VLAN 1
Switch1(config-if)#ip address 141.240.11.10 255.255.255.0
Switch1(config-if)#exit
Switch1(config)#show ip int brief
                  ^
% Invalid input detected at '^' marker.

Switch1(config)#show ip int brief
                  ^
% Invalid input detected at '^' marker.

Switch1(config)#ip default gateway 141.240.11.1
                           ^
% Invalid input detected at '^' marker.

Switch1(config)#ip address 141.240.11.1
                          ^
% Invalid input detected at '^' marker.

Switch1(config)#

No time to ping each other 
Disable firewall
Put manually ip addresses to both computers
And than ping by ip each other
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