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Trent Drilling Summary Log Number 422
T Locaton
John Smith Derwent Road NGR_SK387274
Equpment Notiinghar Level 64.1m OD
Cable Percussion 60m "Sie co ordmates
Fotary Coring _ 24.0m 267.1N_303.0E .
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D Disturbed sample
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