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1. [bookmark: _Toc194858646]Introduction
Maintenance is an essential task in manufacturing, ensuring efficient operation. According to Salonen and Delervd (2011), without proper maintenance, the performance of machinery will deteriorate over time, resulting in increased downtime, higher repair costs, and potential disruptions in production.
Sony UK Technology Centre (Sony UKTec) is an electronics manufacturer in Pencoed, Wales. It is the primary manufacturer of Raspberry Pi products, as illustrated in Figure 1 below.

[image: ]
Figure 1- Raspberry Pi Models (NextPCB, 2024)
Since the introduction of the Raspberry Pi in the early 2010s, demand for these products has grown significantly, necessitating increased production capacity and efficiency. In response, Sony UKTec has implemented automated processes across its production lines, resulting in faster throughput and reduced reliance on manual labour. This report aims to critically evaluate the maintenance practices for one of the key pieces of equipment at Sony UKTec: the Top Load Carton Former, which is used in the automated production of Raspberry Pi units. This report will assess the current maintenance strategy, identify areas for improvement, and propose a more comprehensive maintenance approach.
2. [bookmark: _Toc194858647]Maintenance Strategies
Different maintenance strategies exist, each providing various benefits. The following sections outline these approaches and explain their importance.

[bookmark: _Toc194858648]2.1. Types of Maintenance Strategies
Different maintenance strategies exist because operational requirements, assets and risk factors vary across industries. Table 1 presents seven types of maintenance strategies.

Table 1- Types of Maintenance Approaches (Afolalu et al., 2024)
	Maintenance Strategy
	Description

	Breakdown 
	A reactive approach that occurs only after a failure occurs, resulting in downtime and higher costs

	Preventative
	Scheduled Maintenace to prevent failures before they happen

	Centralised
	A team or department who are responsible for maintenance across multiple areas

	De-Centralised
	Handling local within departments, responsible for own area

	Outsourced
	Maintenance is done externally by a third party, often specialist for the specific equipment

	Condition-Based
	Maintenance is performed based on real-time condition monitoring

	Reliability-Centred
	A strategy that focusses on asset criticality, optimising cost effectiveness and reliability



These different strategies have different advantages and limitations. Multiple maintenance strategies are typically adopted for the best results (Zhao, Gao, and Tang, 2022). The following section will discuss a fatal example of poor maintenance, highlighting the importance of proper maintenance.

[bookmark: _Toc194858649]2.2. Why Maintenance is Important – Morbi Bridge Disaster 
When an organisation neglects or improperly conducts maintenance, overall safety can be compromised. The Morbi pedestrian suspension bridge collapse in Machchhu Pichu, pictured in Figure 2, is a fatal example of why maintenance practices are vital. 

[image: ]
Figure 2 - Morbi Bridge Collapse (Pandey, 2022)

Two days after reopening from maintenance, the bridge collapsed, resulting in 141 fatalities and many more injuries. The maintenance involved replacing the wooden deck with aluminium. The aged and rusted structural supports, such as the cables, bolts, and anchors, were neglected, and no assessment was made of how the new decking may affect the bridge's structural performance. The added weight and neglected structural components led to catastrophic failure (Hakimian, 2022).
Investigations revealed that no assessments were conducted to evaluate the impact of the new decking or the condition of the existing supports. Additionally, local authorities had not authorised the bridge’s reopening (Shah, 2022). 
This failure highlights the importance of adhering to correct maintenance protocols, conducting thorough inspections, and assessing the implications of replacing components with materials of different specifications.

3. [bookmark: _Toc194858650]Investigation of a Maintenance Approach at Sony UKTec
Automation at the Sony UK Technology Centre has progressed significantly, with the Raspberry Pi production lines being the most automated. Figure 3 depicts the second of the three Raspberry Pi production lines at the Pencoed site.

IMAGE OF LINE LAYOUT

This production line uses various equipment, including routers, conveyors, test pods, pick-and-place machines, and various packaging machines. The following section will discuss the current maintenance practices for the 'Top Load Carton Former' used on Line Two and highlight any potential improvements.

[bookmark: _Toc194858651]3.1. Top Load Carton Former - Overview
This equipment is essential in automating the packaging process and is used on all three of the Raspberry Pi lines. Its primary function is to form cartons for the product to be placed in.
[image: ]
Figure 3- Top Load Carton Former
An operator stacks the unfolded carton into the feeder. It is then fed on a chain, glue is applied, and a piston pushes the carton down a shaft, folding the box and placing it onto the conveyor. Further down the line, a single-arm pick-and-place robot picks up the product and places it into the empty carton. This machine is essential to the production line; any breakdowns can cause bottlenecks and downtime for the whole line.

[bookmark: _Toc194858652]3.2. Preventative Maintenance
Sony’s production engineering team maintains this piece of equipment. All maintenance is logged using Limble, a maintenance management system. The following section will discuss the current maintenance strategy.

[bookmark: _Toc194858653]3.2.1. Details & Reasoning for Current Preventative Maintenance Strategy
The primary maintenance strategy for the carton former is preventive maintenance (PM), involving scheduled inspections, lubrication, adjustments, and part replacements to minimise breakdowns. Maintenance tasks are carried out weekly, monthly, and six-monthly to ensure the machine operates efficiently and reliably. The details of the PM are listed in Table 2.


Table 2 - Current Preventative Maintenance Strategy
[image: ]

PM actions have been historically implemented to reduce unexpected downtime, maintain consistent performance, extend equipment lifespan, improve safety and compliance, and control costs. PM is planned and expected, allowing for accurate production scheduling by the planning team and planning by the production engineering team.
Graph 1 highlights the significance of minimising downtime, which displays the downtime cost per minute for each Raspberry Pi 5 variant.

Graph 1 - Pi 5 Variant Downtime Cost Per Minute
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The 16GB Pi 5 is the most expensive variant, with downtime costs exceeding £1,800 per minute. This reinforces the importance of reducing breakdowns to mitigate financial losses and sustain production efficiency.
This strategy is particularly crucial in Sony’s fast-paced manufacturing environment, where preventive maintenance is coordinated with the production planning team. This ensures minimal disruption while maintaining reliability and performance.

[bookmark: _Toc194858654]3.2.2. Pros of the Current Preventative Maintenance Strategy
One key benefit of PM is that it introduces predictability into the maintenance schedule, allowing for better resource allocation, reduced unexpected failures, and cost control (Al Ameeri, Ab Rahman, and Muhamed, 2023). Graph 2 shows the equipment's split between preventative and breakdown maintenance for the past year.


Graph 2 – Type of maintenance for the Top load Carton Former 2024
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By prioritising preventative maintenance, Sony has significantly reduced the requirement for breakdown repairs. Spare parts are purchased in accordance with the maintenance schedule, allowing for accurate planning against long-lead-time components, decreasing downtime, and reducing the high costs that come with emergency purchases (Shokri et al., 2025). 
Scheduled Inspections of components such as the pistons, chains, and motors improve detection of potential failures before they happen (Assis and Marques, 2021). Lubrication of mechanical parts reduces wear, extending the lifespan of critical components. For the carton loader, this is essential for pistons, rotary drives and chain systems. Evidence of this can be found on Limble, showing that the mean time before failure (MTBF) is 711.1 hours.
Regular checks on E-stops, interlocks, and sensors ensure the equipment is safe and compliant with workplace safety regulations, safeguarding the carton's former users.
Overall, the preventative maintenance strategy ensures predictability, optimises resource allocation, reduces unexpected failures, and controls costs. Routine inspections and maintenance, such as lubrication, extend component life span and performance. Routine safety checks ensure the equipment remains compliant and safe for operator use.

[bookmark: _Toc194858655]3.2.3. Cons of the Current Preventative Maintenance Strategy
With PM, significant resources are required to carry out the work, manage the schedule, inventory, and analyse data. Li, Ran, and Zhang (2022) highlight the potential for over-maintenance. This can mean that parts are replaced prematurely, and additional manual labour is required to carry out the maintenance. This can result in unscary costs due to wasted resources and time. 
Although PM is planned, the top-load carton former still requires complete isolation. This leads to downtime during three-shift operations (24 hours) and can disrupt operations if they are not effectively aligned with production demands.
While PM reduces breakdowns, thirteen breakdowns have been logged this year, showing that unexpected failures still occur, as shown in Graph 3.

Graph 3 – Occurrence of breakdowns and average downtime 2024
[image: ]
This suggests that the current PM strategy does not fully address some failure modes, indicating that further refinements are required.
Overall, PM requires significant resources to carry out maintenance actions, manage schedules, inventory and analyse data, especially when applied to many types of machinery across a production site. Unnecessary maintenance is likely to happen, leading to wasted resources and time. While the PM is planned, disruption is still present due to the machine requiring complete isolation. Breakdowns are reduced. However, failures are still present, highlighting the need for further refinements.

[bookmark: _Toc194858656]3.2.4. Improvements to the Current Strategy
The current PM strategy could be enhanced by adjusting the interval frequency based on failure trends. For example, Graph 3 shows six breakdowns related to glue blockages, causing a total average of 5.7 hours of downtime. By increasing the PM frequency for the glue system from monthly to bi-weekly, these failures are more likely to be identified early, reducing the risk of breakdown and downtime.
Introducing a Total Productive Maintenance (TPM) approach is another improvement that would strengthen the current strategy. Figure 5 shows the eight pillars of TPM.

[image: ]
Figure 4 - Eight Pillars of TPM (4Industry, 2024)

TPM is a proactive strategy aimed at improving equipment reliability and reducing downtime. The image illustrates the eight pillars of TPM, which work together to enhance maintenance efficiency and overall performance. These pillars include Autonomous Maintenance, Planned Maintenance, Quality Maintenance, Focused Improvement, Early Equipment Management, Training and Education, Safety, Health and Environment, and Office TPM. Each pillar contributes to a holistic approach to continuous improvement in maintenance practices. TPM encourages operator involvement to maximise overall equipment effectiveness (OEE) (Wan Saidin, 2015). In the case of the Carton Former, operators could be trained to perform monitoring tasks and daily inspections, improving fault detection and easing the technician’s workload.
Alongside PM, Condition-Based Maintenance (CBM) could be implemented by fitting sensors to key components to collect real-time data (Mohammed, Abdulateef and Hamad, 2023). For instance, temperature sensors could monitor glue conditions, and flow sensors could ensure correct glue dispensing. CBM is efficient as it monitors actual component condition, meaning parts are only replaced when necessary. Teixeira and Lopes (2022) highlight that CBM reduces unnecessary maintenance, saving on labour and spare parts costs.
Overall, the current PM strategy could be improved by adjusting maintenance intervals based on failure trends. TPM would enhance overall equipment reliability and reduce technicians' workload through operator involvement. Additionally, CBM using sensors could capture live data, highlighting failures and ensuring performance is maintained while unnecessary maintenance is reduced.

[bookmark: _Toc194858657]3.2.4. Implementation Considerations for the Suggest Improvements
Implementing the proposed improvements will improve the current maintenance strategy; however, careful consideration of costs and resources is necessary (Ye et al., 2009).
Adjusting PM frequency will require additional resources, increasing labour and parts costs (Doostparast and Kolahan, 2015). However, by reducing the likelihood of breakdowns, the costs associated with downtime and reactive repairs are lowered, helping to offset the additional resource costs.
Successful TPM will require pilot programmes to refine analytical techniques and financial investment in training programmes to develop operators' basic maintenance skills. This will involve experienced technicians working with the on-site development team to build structured sessions. Operations standards must also be created for maintenance procedures and regularly updated. As TPM promotes a culture of Kaizen (Plescaci, 2022), the company must ensure financial investment is available to support improvements; otherwise, the TPM approach will not be practical (Dureja et al., 2011). A key benefit is the reduction of low-value-added tasks for technicians, allowing them to focus on higher-priority work while operators take on the basic actions.
To implement CBM, an initial investment in sensor technology will be needed, along with ongoing costs and resources to maintain the sensors. Data must also be captured and accessible to technicians, requiring input from the software development team to design and build dashboards. This may require additional fees for software licenses and training.

[bookmark: _Toc194858658]3.2.5. Change Management Implications
Effective change management needs to be considered to ensure successful implementation (Bassi and Shinde, 2024). Change disrupts established routines, which can be met with resistance from employees (Trader-Leigh, 2022). Some employees may feel uncertain about the changes, especially when required to learn new systems or take on new responsibilities. In the case of TPM, operators may not understand the value of the maintenance activities or feel unsupported, leading to a decline in motivation and a risk of non-compliance.
Initial capability can often be an implication, with employees struggling to adapt to new systems. The ADKAR model in Figure 6 highlights this.
[image: ]
Figure 5 - ADKAR Chanage Management (Jamieson, 2022)

This model highlights knowledge and ability as two critical factors in successful change. This model further strengthens the requirement for structured training and operation standards.
Change fatigue is a risk when organisations implement too many changes at once or fail to show early success. Employees can become disengaged by change if overwhelmed, or the benefits are not visible (Cox et al., 2022). This aligns with William Bridges’ Transition model, highlighting that people require time to adjust to change Samuel and Tsapayi, 2023).
Overall, effective change management is required to improve the current maintenance strategy. Employee engagement and clear communication are critical to the improvements' success. Sony should consider key models like ADKAR and Bridges’ Transition model; the Sony development team could do this.

4. [bookmark: _Toc194858659]Conclusion
Maintenance is critical in any industry, and improper practices can lead to significant operational disruptions. At Sony UKTec, effective maintenance is essential to ensure the seamless operation of production lines, with the Top Load Carton Former being a vital piece of equipment. The current maintenance approach, PM, has proven effective in reducing downtime, controlling costs, enhancing safety, and extending the lifespan of key components.
While the PM strategy has been successful, there is potential to further reduce breakdowns by increasing the frequency of specific maintenance tasks. Additional strategies like TPM and CBM would strengthen the overall maintenance approach. However, implementing these strategies will require careful consideration of the associated costs, resource allocation, and the potential challenges related to change management. Resistance to change is common; thus, it is essential to provide proper training, communication, and support to ensure the successful adoption of these practices.
Overall, adopting a more proactive, data-driven maintenance strategy, underpinned by TPM and CBM, will enhance the reliability and efficiency of the Top Load Carton Former. By effectively investing in these improvements and managing the change process, Sony UKTec can reduce downtime, increase operational resilience, and ensure long-term cost savings.

5. [bookmark: _Toc194858660]Recommendations for Further Work
Accurate cost analysis, including a cost-benefit analysis and return on investment (ROI) calculation, should be performed to justify the investment in TPM, CBM, and increased PM frequencies. Implementing change management strategies, using models like Kotter’s or Lewin’s, will ensure smooth adoption while training staff in new practices and fostering employee engagement. Further exploration of maintenance theories like Reliability-Centred Maintenance (RCM) and Predictive Maintenance (PdM) can optimise the maintenance strategy. Additionally, tracking equipment performance metrics such as MTBF and OEE will provide insights into maintenance effectiveness. Environmental sustainability and safety must remain priorities in any new strategies, alongside developing KPIs for monitoring performance and fostering a culture of continuous improvement. These steps will refine the maintenance approach, reduce downtime, improve cost efficiency, and ensure long-term operational success.













[bookmark: _Toc194858661]
References
4Industry. (2024). A Complete Guide of the 8 TPM Pillars. [Online]. 4industry.com. Available at: https://4industry.com/manufacturing-glossary/8-pillars-of-tpm/ [Accessed 5 April 2025].

Afolalu, S.A., Akinlabi, E.T., Akinlabi, S.A., Salawu, E.Y., Udo, M.O., Ajayi, O.O. (2024). Maintenance strategies and procedures: an overview. 2024 International Conference on Science, Engineering and Business for Driving Sustainable Development Goals (SEB4SDG). IEEE, pp. 1–8. [Online]. Available at: https://doi.org/10.1109/SEB4SDG60871.2024.10630278 [Accessed 24 February 2025]. 

Al Ameeri, T.A., Ab Rahman, M.N., Muhamad, N. (2023). Analysing effective and ineffective impacts of maintenance strategies on electric power plants: A comprehensive approach. Energies (Basel), 16(17), pp. 6243-. [Online]. Available at: https://doi.org/10.3390/en16176243 [Accessed 24 February 2025].

Assis, R., Marques, P.C. (2021). A dynamic methodology for setting up inspection time intervals in conditional preventive maintenance. Applied sciences, 11(18), pp. 8715-. [Online]. Available at: https://doi.org/10.3390/app11188715 [Accessed 24 February 2025].

Bassi, D., Shinde, A. (2024). Barriers to successful change management. Management in healthcare, 8(3), pp.271–283.

Cox, C.B., Gallegos, E., Pool, G.J., Gilley, K.M., Haight, N. (2022). Mapping the nomological network of change fatigue: identifying predictors, mediators and consequences. Journal of organizational change management, 35(4/5), pp.718–733. [Online]. Available at: https://doi.org/10.1108/JOCM-12-2021-0369 [Accessed 6 April 2025].

Doostparast, M., Kolahan, F., Doostparast, M. (2015). Optimisation of PM scheduling for multi-component systems - a simulated annealing approach. International journal of systems science, 46(7), pp.1199–1207. [Online]. Available at: https://doi.org/10.1080/00207721.2013.815822 [Accessed 31 March 2025].
Dureja, J.S., Sachdeva, A., Sharma, V.S., Dogra, M. (2011). TPM – A Key Strategy for Productivity Improvement. Journal of Engineering Science & Technology, 6(1), pp.1–16. [Accessed 6 April 2025].

Hakimian, R. (2022). Early theories for India footbridge collapse. New Civil Engineer. (3017), pp. 13-. [Online]. Available at: https://librarysearch.uwtsd.ac.uk/discovery/fulldisplay?docid=cdi_proquest_reports_2770357263&context=PC&vid=44WHELF_UWTSD:44WHELF_UWTSD_VU1&lang=en
 [Accessed 24 February 2025].

Jamieson, J. (2022). Prosci's Top 10 Tactics for Managing Resistance to Change. [Online]. prosci.com. Last Updated: 2025. Available at: https://www.prosci.com/blog/prosci-top-10-tactics-for-managing-resistance-to-change [Accessed 6 April 2025].

Li, X., Ran, Y., Zhang, G. (2022). Optimization of equal-cycle maintenance strategy considering imperfect preventive maintenance. Proceedings of the Institution of Mechanical Engineers. Part E, Journal of Process Mechanical Engineering, 236(4), pp. 1392–1402. [Online]. Available at: https://doi.org/10.1177/09544089211063852 [Accessed 24 February 2025].

Mohammed, N.A., Abdulateef, O.F., Hamad, A.H. (2023). An IoT and Machine Learning-Based Predictive Maintenance System for Electrical Motors. Journal Europeen des Systemes Automatises, 56(4), pp.651–. [Online]. Available at: https://doi.org/10.18280/jesa.560414 [Accessed 31 March 2025].

NextPCB. (2024). What Is Raspberry Pi? Models, Features, and Uses. [Online]. nextpcb.com. Available at: https://www.nextpcb.com/blog/what-is-raspberry-pi-models-features-and-uses [Accessed 13 March 2025].

Plescaci, D. (2022). Kaizen Costing – A Continuous Improvement Strategy of the Organisations. CECCAR Business Review, 3(2), pp.30–41. [Online]. Available at: https://doi.org/10.37945/cbr.2022.02.04 [Accessed 6 April 2025].

Salonen, A., Deleryd, M. (2011). Cost of poor maintenance: A concept for maintenance performance improvement. Journal of quality in maintenance engineering. 17(1), pp. 63–73. [Online]. Available at: https://doi.org/10.1108/13552511111116259 [Accessed 24 February 2025]. 

Shah, J. (2022). Morbi bridge collapse | Nail the villains: Fixing culpability in the Morbi tragedy is still a work in progress. Quick action needs to be taken to punish the guilty. New Delhi: Living Media India, Limited. [Online]. Available at: https://librarysearch.uwtsd.ac.uk/discovery/fulldisplay?docid=cdi_proquest_miscellaneous_2732447954&context=PC&vid=44WHELF_UWTSD:44WHELF_UWTSD_VU1&lang=en [Accessed 24 February 2025].

Shokri, A., Toliyat, S.M.H., Hu, S., Skoumpopoulou, D. (2025). Integrating spare part inventory management and predictive maintenance as a digital supply chain solution. Journal of modelling in management, 20(3), pp. 1003–1029. [Online]. Available at: https://doi.org/10.1108/JM2-05-2024-0131 [Accessed 24 February 2025].

Teixeira, H.N., Lopes, I.S. (2025). Supporting condition-based maintenance implementation: a methodology. Journal of quality in maintenance engineering, 31(1), pp.48–82. [Online]. Available at: https://doi.org/10.1108/JQME-07-2023-0067 [Accessed 31 March 2025]. 

Trader-Leigh, K.E. (2002). Case study: identifying resistance in managing change. Journal of organizational change management, 15(2), pp.138–155. [Online]. Available at: https://doi.org/10.1108/09534810210423044 [Accessed 6 April 2025].

Wan Saidin, W.A.N., Kasim, N.I., Musa, M.A., Mohamad Noor, N. and Razali, A.R. (2015). Improvement of Overall Equipment Effectiveness (OEE) through Implementation of Total Productive Maintenance (TPM) in Manufacturing Industries. Applied Mechanics and Materials, 761(Recent Technologies in Design, Management and Manufacturing), pp.180–185. [Online]. Available at: https://doi.org/10.4028/www.scientific.net/AMM.761.180 [Accessed 31 March 2025].

Ye, Z., Strong, C.K., Shi, X., Conger, S.M., Huft, D.L. (2009). Benefit–cost analysis of maintenance decision support system. Transportation research record, 2107(1), pp.95–103. [Online]. Available at: https://doi.org/10.3141/2107-10 [Accessed 31 March 2025].

Zhao, J., Gao, C., Tang, T. (2022). A review of sustainable maintenance strategies for single component and multicomponent equipment. Sustainability, 14(5), pp. 2992-. [Online]. Available at: https://doi.org/10.3390/su14052992 [Accessed 24 February 2025].
image4.png
Frequency

Details

Check gluedispenservalues and ensure correct temperature and pressure

Daily Inspect carton infeed and ensure correct width for product carton

Lubricate push arms with PTFE Spray
Inspect vacuum suction cups and replace if damaged
Inspect air feeds, air pressure, joins & pipes for wear/leakage

Weekly Lubricate drive chain with dry PTFE spray (spray on drive gear and idler)
Inspect drive belt tension (should have 5mm of deformation mm +/-2mm), adjust if required
Inspect and tighten all former position bolts (15NM +/-2NM) & chain tensionerbolts (18NM +/-2NM)
Inspect and test E Stop & Interlocks
Clean rails, guides and pushers
Inspect forming heads operation reaches top and bottom position smoothly
Inspect the box removal cylinder sensors and forming heads cylinder sensors are working
Inspect Rotary Drive condition, including grubs screws, rotation play, etc.
Clean old grease off chain and re-lube with dry PTFE (whole chain and gears)
Check tension on both chains (should be 10mm of deformation +/-2mm)
Remove blue brackets securing the brass collars on the frontaxle, clean brackets and collars, re-lube with PTFE & refit
Check play on swing arm on removal piston for wear, replace pin if worn
Check condition of swing arm stopper for wear
Check condition of pistons that drive the removal fingers, check no play orwear in any of the components.

Monthly Check condition of power supply cables (including caravan plug to drop)
Check all 5 interlocks are working correctly
Check E-stop is working correctly (on HMI panel)
Inspect all sensors and reed switches on the machine are working correctly and in good condition
Tighten guide nuts on channels
Check and tighten glue pipe joints
Check and adjust glue air pressure (2.5bar +/-0.1 bar)
Check any glue pipe unions forleaks, torque check/replace O-rings if leaks found
Purge glue & test/inspect gluing position
Clean nozzles to remove any external glue build up/burnt glue then test packing machine to inspect glue timings and positions
Mark position of chain tensioner, flight position, front drive axel gear & TDC of drive motor system
Remove chains by removing drive belts (undoing tensioning roller and lifting off drive gear), then moving splitlinks to
accessible position and removing

6 Monthly |Clean alldrive gears &idlers, clean all chain guides with hand wipes

Re-lube chains with PTFE spray (whole chain and gears)
Check the gain of the glue sensor
Check box push distance of the motor, check italigns correctly with the former
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