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Lab - Accessing Network Devices with SSH

Lab - Accessing Network Devices with SSH 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.1.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.11
	255.255.255.0
	192.168.1.1

	PC-A
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.1


Objectives
Part 1: Configure Basic Device Settings
Part 2: Configure Basic Security Measures on the Router and Switch
Part 3: Configure the Router for SSH Access
Part 4: Configure the Switch for SSH Access
Part 5: SSH from the CLI on the Switchline 
Background / Scenario
In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.
Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands; however, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.
The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.
Note: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.
Note: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.
Required Resources
1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
1 Switch (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
1 PC (Windows 7 or 8 with terminal emulation program, such as Tera Term, and Wireshark installed)
Console cables to configure the Cisco IOS devices via the console ports
Ethernet cables as shown in the topology
Configure Basic Device Settings
In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.
Cable the network as shown in the topology.
Step 1: Initialize and reload the router and switch.
Step 2: Configure the router.
a. Console into the router and enable privileged EXEC mode.
b. Enter configuration mode.
c. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
d. Assign class as the privileged EXEC encrypted password.
e. Assign cisco as the console password and enable login.
f. Assign cisco as the VTY password and enable login.
g. Encrypt the plaintext passwords.
h. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
i. Configure and activate the G0/1 interface on the router using the information contained in the Addressing Table.
j. Save the running configuration to the startup configuration file.
Configure PC-A.
Configure PC-A with an IP address and subnet mask.
Configure a default gateway for PC-A.
Verify network connectivity.
Ping R1 from PC-A. If the ping fails, troubleshoot the connection.



1. Configure Basic Security Measures on the Router
b. Encrypt the clear text passwords.
R1(config)# service password-encryption
b. Strengthen passwords.
An administrator should ensure that passwords meet the standard guidelines for strong passwords. These guidelines could include combining letters, numbers and special characters in the password and setting a minimum length.
Note: Best practice guidelines require the use of strong passwords, such as those shown here, in a production environment. However, the other labs in this course use the cisco and class passwords for ease in performing the labs.
2. Change the privileged EXEC encrypted password to meet guidelines.
R1(config)# enable secret Enablep@55
2. Require that a minimum of 10 characters be used for all passwords.
R1(config)# security passwords min-length 10
b. Secure the console and VTY lines.
3. You can set the router to log out of a connection that has been idle for a specified time. If a network administrator was logged into a networking device and was suddenly called away, this command automatically logs the user out after the specified time. The following commands cause the line to log out after five minutes of inactivity.
R1(config)# line console 0
R1(config-line)# exec-timeout 5 0
R1(config-line)# line vty 0 4
R1(config-line)# exec-timeout 5 0
R1(config-line)# exit
R1(config)#
3. The following command impedes brute force login attempts. The router blocks login attempts for 30 seconds if someone fails two attempts within 120 seconds. This timer is set especially low for the purpose of this lab.
R1(config)# login block-for 30 attempts 2 within 120
What does the 2 within 120 mean in the above command?
_The user will be blocked from logging in after 2 failed attempts to log in within a 120 second time period______________________________________________________________________
What does the block-for 30 mean in the above command?
_The router will not allow an attempt at login access for a period of 30 seconds after login access is blocked___________________________________________________________________________
b. Verify that all unused ports are disabled.
Router ports are disabled by default, but it is always prudent to verify that all unused ports are in an administratively down state. This can be quickly checked by issuing the show ip interface brief command. Any unused ports that are not in an administratively down state should be disabled using the shutdown command in interface configuration mode.


R1# show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/0         unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/1         192.168.1.1     YES manual up                    up      
Serial0/0/0                unassigned      YES NVRAM  administratively down down    
Serial0/0/1                unassigned      YES NVRAM  administratively down down    

Configure the Router for SSH Access
Using Telnet to connect to a network device is a security risk because all information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.
Configure device authentication.
The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the crypto key command.
Configure the domain for the device.
R1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
R1(config)# crypto key generate rsa modulus 1024
The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds) 

R1(config)#
*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled
Configure a local database username.
R1(config)# username admin privilege 15 secret adminpass
Note: A privilege level of 15 gives the user administrator rights.
Enable SSH on the VTY lines.
Enable Telnet and SSH on the inbound VTY lines using the transport input command.
R1(config)# line vty 0 4
R1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
R1(config-line)# login local
R1(config-line)# end
R1#
Save the running configuration to the startup configuration file.
R1# copy running-config startup-config
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
Establish an SSH connection to the router.
Start Tera Term from PC-A.
Use Tera Term to telnet to R1.
Does R1 accept the Telnet connection? Explain.
No, telnet was not enabled on the inbound VTY lines. SSH was.____________________________________________________________________________________
____________________________________________________________________________________
Use Tera Term, establish an SSH session to R1. Use the username admin and password adminpass1. You should be able to establish an SSH session with R1.
Does R1 accept the SSH connection? ___Yes_______ 
Intentionally mistype the user and password information to see if login access is blocked after two attempts.
What happened after you failed to login the second time?
_The connection was terminated and I was unable to reconnect for 30 seconds ___________________________________________________________________________________
____________________________________________________________________________________
From your console session on the router, issue the show login command to view the login status. In the example below, the show login command was issued within the 30 second login blocking period and shows that the router is in Quiet-Mode. The router will not accept any login attempts for 14 more seconds.
R1# show login
     A default login delay of 1 second is applied.
     No Quiet-Mode access list has been configured.

     Router enabled to watch for login Attacks.
     If more than 2 login failures occur in 120 seconds or less,
     logins will be disabled for 30 seconds.

     Router presently in Quiet-Mode.
     Will remain in Quiet-Mode for 14 seconds.
     Denying logins from all sources.
R1#
After the 30 seconds has expired, SSH to R1 again and login using the SSHadmin username and Admin1p@55 for the password.
After you successfully logged in, what was displayed? ___The motd banner configured earlier _____________________ 
Enter privileged EXEC mode and use Enablep@55 for the password.
If you mistype this password, are you disconnected from your SSH session after two failed attempts within 120 seconds? Explain.
_No, the login block-for command only applies to the SSH connection. ___________________________________________________________________________________
____________________________________________________________________________________
Issue the show running-config command at the privileged EXEC prompt to view the security settings you have applied.
Configure the Switch for SSH Access
In Part 3, you will configure the switch in the topology to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.
Configure the basic settings on the switch.
Console into the switch and enable privileged EXEC mode.
Enter configuration mode.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plain text passwords.
Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.
Save the running configuration to the startup configuration file.
Configure the switch for SSH connectivity.
Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.
Configure the device name as listed in the Addressing Table.
Configure the domain for the device.
S1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
S1(config)# crypto key generate rsa modulus 1024
Configure a local database username.
S1(config)# username admin privilege 15 secret adminpass
Enable Telnet and SSH on the VTY lines.
S1(config)# line vty 0 15
S1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
S1(config-line)# login local
S1(config-line)# end
Establish an SSH connection to the switch.
Start Tera Term from PC-A, and then SSH to the SVI interface on S1.
Are you able to establish an SSH session with the switch?
____Yes________________________________________________________________________________
SSH From the CLI on the Switch
The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.
View the parameters available for the Cisco IOS SSH client.
Use the question mark (?) to display the parameter options available with the ssh command.
S1# ssh ?
  -c    Select encryption algorithm
  -l    Log in using this user name
  -m    Select HMAC algorithm
  -o    Specify options
  -p    Connect to this port
  -v    Specify SSH Protocol Version
  -vrf  Specify vrf name
  WORD  IP address or hostname of a remote system
SSH to R1 from S1.
You must use the –l admin option when you SSH to R1. This allows you to log in as user admin. When prompted, enter adminpass for the password.
S1# ssh -l admin 192.168.1.1
Password: 
***********************************************
  Warning: Unauthorized Access is Prohibited!
***********************************************

R1#
You can return to S1 without closing the SSH session to R1 by pressing Ctrl+Shift+6. Release the Ctrl+Shift+6 keys and press x. The switch privileged EXEC prompt displays.
R1#
S1#
To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.
S1#
[Resuming connection 1 to 192.168.1.1 ... ]

R1#
To end the SSH session on R1, type exit at the router prompt.
R1# exit

[Connection to 192.168.1.1 closed by foreign host]
S1#

What versions of SSH are supported from the CLI?
Versions 1 and 2, displayed by running the command “ssh -v ?”
______________________________________________________________________________________
_______________________________________________________________________________________

How would you provide multiple users, each with their own username, access to a network device?
You could add additional users to the local database using the username command _______________________________________________________________________________________

Reflection (max 800 words): 
Write a research report comparing various Encryption standards, e.g AES, SHA, DES, RSA.  

Introduction - What is encryption?
According to the National institute of Standards and Technology (NIST), Encryption is “The process of changing plaintext into ciphertext using a cryptographic algorithm and key” [1]. Encryption algorithms use an encryption key that is used to convert plaintext into ciphertext, increasing the likelihood that transmitted data remains confidential. Network data encryption is provided at the IP packet level [2].

There are two main encryption techniques that are used to encrypt and decrypt data: 

Symmetric Encryption
This method uses the same secret key to both encrypt and decrypt data. The data sender uses the key to encrypt plaintext to ciphertext, and the data receiver uses the same key to decrypt the data from ciphertext to plaintext. Symmetric key encryption does not require large amounts of computational power to perform its cryptographical functions and is faster to use than asymmetrical encryption (described later). Virtual Private Networks (VPNs) make use of this characteristic to encrypt the data that flows across them.

Below are some common examples of symmetric encryption algorithms:

Data Encryption Standard (DES): This older algorithm was developed by IBM in the 70’s. A 64-bit cryptographic key is used to encrypt data, however 1 parity bit is used from each byte resulting in a relatively short 56-bit randomly generated symmetric key to encrypt data. DES is a block cipher algorithm that encrypts 64-bit data blocks and is run 16 times to produce the final ciphertext. The ciphertext output using DES is usually larger than the original plaintext due to artificial data being added if a 64-bit data block is not full at the time of encryption. It is susceptible to brute force attacks and is no longer considered secure, having been broken in public for the first time in June 1997. 
· Advanced Encryption Standard (AES): Advanced Encryption Standard (AES) is a more recent encryption method that is deemed secure and intended to replace DES and 3DES standards. AES was approved by NIST in December 2001. AES can use 128-bit, 192-bit, or 256-bit cryptographic keys to encrypt 128-bit data blocks depending on requirements. The number of transformation rounds that produce the ciphertext in AES is dependent on the key size, with a 128-bit key performing 10 rounds, a 192-bit key performing 12 rounds and a 256-bit key performing 14 rounds.

Asymmetric Encryption
Also known as Public Key Encryption, Asymmetric encryption involves the use of 2 separate keys (a key pair), known as a public key and a private key. One key is used for encryption and the other is used for decryption. If a data transmitter wishes to send an encrypted message to a recipient, they must first know the recipients public key and use it to encrypt the data. The encrypted data can then only be decrypted by the recipient using the recipients private key, which is secret. 

If the data receiver also wishes to authenticate a sender, a hash value of the plaintext is generated by the sender and encrypted using their own private key and attached as a digital signature to the message. The recipient uses the senders public key to decrypt the included hash value and compare it to the hash of the decrypted ciphertext.  It is not possible to calculate the private key based on knowledge of the public key.

A symmetric encryption algorithm in widespread use today is RSA (Rivest-Shamir-Adleman). This algorithm creates a public and private key from the product of 2 very large prime numbers of equal length. Due to the relatively slow speed at which RSA functions due to its high processing requirements, it is frequently used to encrypt and transfer symmetric keys that are then used to encrypt large amounts of data. 

To verify data integrity, a method known as hashing is used. A fixed-sized hash value is created from a block of data using a one-way hash function. The fixed length hash created by the data sender should be identical to the hash value of the data when the same hash function is run on it by the receiving party. If the hash values do not match it would indicate a problem with data integrity of the packets. 

A family of cryptographic hash functions published by NIST known as the Secure Hash Algorithms or SHA are in widespread use today. Three of the algorithms that make up SHA are:

· SHA-1: Produces a 160-bit hash value.
· SHA-2: Two hash functions that can produce hash values between 224-bits and 512-bits in length.
· SHA-3: Produces similar length hash values as SHA-2, but is based off a different cryptographic function and is faster [4]


Conclusion
Cryptography is crucial when the confidentiality, data integrity and authentication of communications across modern networks is required. Encryption algorithms are increasingly challenged as computing power increases over time.
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