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Lab - Accessing Network Devices with SSH

Lab - Accessing Network Devices with SSH 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.1.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.11
	255.255.255.0
	192.168.1.1

	PC-A
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.1


Objectives
Part 1: Configure Basic Device Settings
Part 2: Configure Basic Security Measures on the Router and Switch
Part 3: Configure the Router for SSH Access
Part 4: Configure the Switch for SSH Access
Part 5: SSH from the CLI on the Switch
Background / Scenario
In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.
Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands; however, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.
The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.
Note: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.
Note: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.
Required Resources
1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
1 Switch (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
1 PC (Windows 7 or 8 with terminal emulation program, such as Tera Term, and Wireshark installed)
Console cables to configure the Cisco IOS devices via the console ports
Ethernet cables as shown in the topology
Configure Basic Device Settings
In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.
Cable the network as shown in the topology.
Step 1: Initialize and reload the router and switch.
Step 2: Configure the router.
a. Console into the router and enable privileged EXEC mode.
b. Enter configuration mode.
c. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
d. Assign class as the privileged EXEC encrypted password.
e. Assign cisco as the console password and enable login.
f. Assign cisco as the VTY password and enable login.
g. Encrypt the plaintext passwords.
h. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
i. Configure and activate the G0/1 interface on the router using the information contained in the Addressing Table.
j. Save the running configuration to the startup configuration file.
Configure PC-A.
Configure PC-A with an IP address and subnet mask.
Configure a default gateway for PC-A.
Verify network connectivity.
Ping R1 from PC-A. If the ping fails, troubleshoot the connection.



1. Configure Basic Security Measures on the Router
b. Encrypt the clear text passwords.
R1(config)# service password-encryption
b. Strengthen passwords.
An administrator should ensure that passwords meet the standard guidelines for strong passwords. These guidelines could include combining letters, numbers and special characters in the password and setting a minimum length.
Note: Best practice guidelines require the use of strong passwords, such as those shown here, in a production environment. However, the other labs in this course use the cisco and class passwords for ease in performing the labs.
2. Change the privileged EXEC encrypted password to meet guidelines.
R1(config)# enable secret Enablep@55
2. Require that a minimum of 10 characters be used for all passwords.
R1(config)# security passwords min-length 10
b. Secure the console and VTY lines.
3. You can set the router to log out of a connection that has been idle for a specified time. If a network administrator was logged into a networking device and was suddenly called away, this command automatically logs the user out after the specified time. The following commands cause the line to log out after five minutes of inactivity.
R1(config)# line console 0
R1(config-line)# exec-timeout 5 0
R1(config-line)# line vty 0 4
R1(config-line)# exec-timeout 5 0
R1(config-line)# exit
R1(config)#
3. The following command impedes brute force login attempts. The router blocks login attempts for 30 seconds if someone fails two attempts within 120 seconds. This timer is set especially low for the purpose of this lab.
R1(config)# login block-for 30 attempts 2 within 120
What does the 2 within 120 mean in the above command?
Two failed attempts within 120 seconds. 
What does the block-for 30 mean in the above command?
Blocks login attempts for 30 seconds if there are 2 failed attempts within 120 seconds. 
b. Verify that all unused ports are disabled.
Router ports are disabled by default, but it is always prudent to verify that all unused ports are in an administratively down state. This can be quickly checked by issuing the show ip interface brief command. Any unused ports that are not in an administratively down state should be disabled using the shutdown command in interface configuration mode.


R1# show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/0         unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/1         192.168.1.1     YES manual up                    up      
Serial0/0/0                unassigned      YES NVRAM  administratively down down    
Serial0/0/1                unassigned      YES NVRAM  administratively down down    

Configure the Router for SSH Access
Using Telnet to connect to a network device is a security risk because all information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.
Configure device authentication.
The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the crypto key command.
Configure the domain for the device.
R1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
R1(config)# crypto key generate rsa modulus 1024
The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds) 

R1(config)#
*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled
Configure a local database username.
R1(config)# username admin privilege 15 secret adminpass
Note: A privilege level of 15 gives the user administrator rights.
Enable SSH on the VTY lines.
Enable Telnet and SSH on the inbound VTY lines using the transport input command.
R1(config)# line vty 0 4
R1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
R1(config-line)# login local
R1(config-line)# end
R1#
Save the running configuration to the startup configuration file.
R1# copy running-config startup-config
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
Establish an SSH connection to the router.
Start Tera Term from PC-A.
Use Tera Term to telnet to R1.
Does R1 accept the Telnet connection? Explain.
No, because Telnet was disabled because we had used the transport input SSH command. 
Use Tera Term, establish an SSH session to R1. Use the username admin and password adminpass. You should be able to establish an SSH session with R1.
Does R1 accept the SSH connection? Yes 
Intentionally mistype the user and password information to see if login access is blocked after two attempts.
What happened after you failed to login the second time?
It says: The connection to R1 was disconnected, if you attempt to reconnect in 30 seconds the connection will be refused. 
From your console session on the router, issue the show login command to view the login status. In the example below, the show login command was issued within the 30 second login blocking period and shows that the router is in Quiet-Mode. The router will not accept any login attempts for 14 more seconds.
R1# show login
     A default login delay of 1 second is applied.
     No Quiet-Mode access list has been configured.

     Router enabled to watch for login Attacks.
     If more than 2 login failures occur in 120 seconds or less,
     logins will be disabled for 30 seconds.

     Router presently in Quiet-Mode.
     Will remain in Quiet-Mode for 14 seconds.
     Denying logins from all sources.
R1#
After the 30 seconds has expired, SSH to R1 again and login using the SSHadmin username and Admin1p@55 for the password.
After you successfully logged in, what was displayed? The MOTD warning login banner 
Enter privileged EXEC mode and use Enablep@55 for the password.
If you mistype this password, are you disconnected from your SSH session after two failed attempts within 120 seconds? Explain.
If you mistype the password MORE THAN twice within 120 seconds, it will be disabled for 30 seconds, and this will put the router in quiet mode. 
Issue the show running-config command at the privileged EXEC prompt to view the security settings you have applied.
Configure the Switch for SSH Access
In Part 3, you will configure the switch in the topology to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.
Configure the basic settings on the switch.
Console into the switch and enable privileged EXEC mode.
Enter configuration mode.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plain text passwords.
Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.
Save the running configuration to the startup configuration file.
Configure the switch for SSH connectivity.
Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.
Configure the device name as listed in the Addressing Table.
Configure the domain for the device.
S1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
S1(config)# crypto key generate rsa modulus 1024
Configure a local database username.
S1(config)# username admin privilege 15 secret adminpass
Enable Telnet and SSH on the VTY lines.
S1(config)# line vty 0 15
S1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
S1(config-line)# login local
S1(config-line)# end
Establish an SSH connection to the switch.
Start Tera Term from PC-A, and then SSH to the SVI interface on S1.
Are you able to establish an SSH session with the switch?
Yes, you are able to establish a connection with the switch if you repeat the commands used for the router. 
SSH From the CLI on the Switch
The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.
View the parameters available for the Cisco IOS SSH client.
Use the question mark (?) to display the parameter options available with the ssh command.
S1# ssh ?
  -c    Select encryption algorithm
  -l    Log in using this user name
  -m    Select HMAC algorithm
  -o    Specify options
  -p    Connect to this port
  -v    Specify SSH Protocol Version
  -vrf  Specify vrf name
  WORD  IP address or hostname of a remote system
SSH to R1 from S1.
You must use the –l admin option when you SSH to R1. This allows you to log in as user admin. When prompted, enter adminpass for the password.
S1# ssh -l admin 192.168.1.1
Password: 
***********************************************
  Warning: Unauthorized Access is Prohibited!
***********************************************

R1#
You can return to S1 without closing the SSH session to R1 by pressing Ctrl+Shift+6. Release the Ctrl+Shift+6 keys and press x. The switch privileged EXEC prompt displays.
R1#
S1#
To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.
S1#
[Resuming connection 1 to 192.168.1.1 ... ]

R1#
To end the SSH session on R1, type exit at the router prompt.
R1# exit

[Connection to 192.168.1.1 closed by foreign host]
S1#

What versions of SSH are supported from the CLI?
Protocol versions one and two

How would you provide multiple users, each with their own username, access to a network device?
Use the user name command to add the account details onto the local database. 

Reflection (max 800 words): 
Write a research report comparing various Encryption standards, e.g AES, SHA, DES, RSA.  

Comparing various encryption standards 

	Encryption is a way of encoding the data or the message, for the purpose of restricting access to that data. This will keep any private information secure from any unauthorised access, as only the correct users can recover and access the original information.  The national institute of standards and technology or NIST, is the organisation that sets these encryption standards, these standards are also known as federal information processing standards (FIPS).
	
Encryption standards can be part of one of three of the following categories:
· Symmetric Key Algorithms 
· Asymmetric Key Algorithms 
· Cryptographic Hash Functions 

Asymmetric encryption uses key algorithms to encrypt data. This is also known as one-way encryption because it uses public and private keys, using both to decrypt the data. This is beneficial for authentication. Examples of asymmetric key algorithms are DSA and RSA. 
Symmetric encryption is also known as two-way encryption because the same keys are able to encrypt and also decrypt the data. This method is more suited to communication needs. Examples of symmetric key algorithms are; DES, Triple DES and also AES. 
Cryptographic Hash Functions uses a type of mathematical solution to map the data to a fixed length output, known as a hash value. When transmitting data, the data is sent along with the hash value. When it is received at the other end of the transmission, the data goes back through the hash function to check if the hash values match. If the hash values match, it means the integrity of the data is still intact, if the hash values are not the same it means the data has been unlawfully accessed during the transmission. 


Encryption methods can provide services such as:
· Integrity 
· Authorisation
· Confidentiality
· Authentication 

DES
Data encryption standard is a symmetric key algorithm, with a key length of 56-bits. The DES standard was published in 1977 by NIST. However, this standard is no longer in use because the 56-bit key size was too small, therefore making DES vulnerable to attacks. The key size made it possible for users to break the encryption. 
After DES, the Triple DES or 3DES standard was put in place, which is simply using the DES standard three times. However, this again was still vulnerable to attacks. 

AES
The Advanced Encryption Standard was developed by NIST to replace DES, and was published in 2001. AES gives the choice of using a 128-bit, 192-bit or a 256-bit key. 128, 192 and 256 are the highest key sizes, and the higher the key size, the stronger and more secure the algorithm. AES also have an advanced encryption method compared to the DES encryption method. This advanced method of encryption ‘involves a series of substitution and permutation steps to create the encrypted block.’ [1]

Benefits of AES 
· Higher Key sizes therefore better security 
· Can be implemented in both hardware and software 
· [bookmark: _GoBack]Most popular solution used worldwide – good availability
· Fast 
Drawbacks of AES
· Difficult to implement with software
· Uses a simplified mathematical structure 
· Every block is always encrypted in the same way 

SHA 
SHA or secure hash algorithm is an example of a cryptographic hash function. Using a mathematical solution to create a hash value, for the purpose of testing the integrity of the data, but not encrypting the data. SHA has lots of different versions from SHA-1 producing 160-bit hash values, to SHA-256 producing 256-bit hash values and SHA-512 producing 512-bit hash values. This hash value will be sent along with the data and compared after transmission to verify the integrity. This is more of an authentication process rather than an encryption process, but it can work alongside an encryption process like AES. 

RSA
Another encryption standard is the RSA standard, named after the three developers; Rivest, Shamir and Adelman. RSA is an example of an asymmetric key algorithm. This method of encryption is also known as one-way encryption, as it uses public and private keys to decrypt the encrypted data. RSA is used to encrypt and distribute the symmetric key, providing an authentication service. However, asymmetric encryption is much slower than a symmetric encryption method. RSA is used worldwide for online banking, password exchange, online shopping, and many more. 

These encryption standards have many pros and cons and some, like DES are no longer efficient to use due to the advancement in technologies which means the security threats have become real attacks. The most effective encryption standards are those with the largest key sizes which is now going into the thousands. However, the different encryption standards can be used for different services that are required. The encryption standard selected will come down to what it is being used for and why. As discussed previously, AES is used for confidentiality purposes, but SHA is used for authentication, by verifying the integrity of the data. 
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