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Introduction
The following assessment will produce 3 risk assessments, 3 methods statements and a phase plan for a new build domestic property, the risk assessments and method plans will relate to works that will be carried out during the build. It will also look in to key legislations that cover this kind of construction project. 
The proposed site is based at Kings road Kings road, Saint Thomas, Swansea, SA1 8AH.
[image: ]
The proposed development is for a single, two story detached house with a room to the loft for extra living space. The principal contractor will oversee the build while communicating with the client and designer on a frequent basis. The major building works and external works i.e. the ground works, blockwork, roof etc. will be done by the main contractor, the other works such and the plumbing/Heating, electrics, carpentry and painting will all be sub-contractors. The build is proposed to start on the 6th of May 20202.  







Phase plan

	Construction Phase Plan



	Contractor:

	Jones Construction

	Description of project:

	New build 2 storey detached home

	
	

	Location of project:
	Kings road 
Saint Thomas 
Swansea
SA1 8AH


	Project Start/End dates:

Site Hours:
	06/05/2020 – 30/09/2020

07.30 - 1700

	
	

	Main contractor duties:
	· To plan manage and monitor the work from start to finish while being in constant contact with the designer, client, contractors and employees.
· Ensure welfare facilities are provided
· Ensure site is safe and secure
· Make sure all workers have had a site induction and have correct training and qualifications
· Health and safety 


	
	

	Site supervisor:
	S. Jones


	
	

	Sub-Contractors:
	· Plumbing/Heating
· Electricians
· Tilers
· Plasterers
· Painters
· Carpenters


	
	

	Welfare arrangements:
	Portaloo toilets, Cabins for lunch breaks.

	
	

	Minimum PPE:
	Hard hats, Safety boot/shoes and hi-vis vests

	
	

	Site access and Egress:
	Access from main road.
Parking only in designated area


	
	

	Site Security and Emergency procedures:
	· Security cabin and security guard.
· All tools and equipment to be stored in the secure storage at the end of each day.
· Any access to height i.e. scaffolding or ladders to me made inaccessible
· Any chemicals to be stored correctly and securely. 
· Fire safety points clearly marked as advised on site induction

	
	

	Co-ordination of contractors:
	Meetings each day in order for all persons to keep up to date with going on.

	
	

	Site Inductions:
	Site supervisor to carry out inductions to all contractors prior to them starting work

	
	

	Site Inspections:
	Carried out daily by site Supervisor

	
	

	Site Rules:
	· PPE to be worn at all times
· Smoking only in smoking area
· No noise i.e. Drilling before 8am
· Waste/rubbish to be cleaned up and disposed of correctly before end of shift.

	
	



	Risks Present On Site



	Asbestos:
	N/A - New build 

	
	

	Working at Height:
	· All workers to be made aware of the dangers and consequences of falling from height.
· Only competent workers to work at height 
· All work at height to be supervised
· Only work at height once ensuring working conditions are safe to do so 
· Wearing and using correct PPE	
· Risk assessment to be carried out and followed.


	
	

	Dust/Chemicals
	Dust mask, gloves and Eye protection to be worn when necessary

	
	

	Excavations
	· Details from local water, gas and electric companies of positions of possible main lines in the vicinity.
· Barriers around trenches
· Reinforce trenches

	
	

	Members of Public/employees/sub-contractors
	· Access to site to be controlled by the site supervisor 
· Anti-climb safety fence to cordon off the site
· All workers to have site induction and be signed in and out every day. 

	
	

	Other Risks
	· Site to be secured at the end of each day
· Access to sight only during working hours
· Deliveries to site to be planned around busy periods of the day to reduce disruption
· Site cleanliness to be kept up at all times








Risk Assessments 
	Activity to be Assessed
	Assessment Number

	Plumbing and Heating
	001

	Persons undertaking or affected by the activity

	

	
	×
	Employees
	×
	Contractor
	
	Public
	×
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Fire from hot works
	2
	4
	8

	2
	Power tools
	3
	4
	12

	3
	Hand tools
	2
	3
	6

	4
	Fumes from soldering and solvent cement
	2
	4
	8

	5
	Trips/Slips/Falls
	3
	3
	9

	Existing Control Measures / Additional Control Measures Required

	1
	Area to be examined 30mins after completion/ No hot works to be done within 1hour of leaving site.
Fire extinguishers to be available.
Use of Heat mats to protect combustible material.  

	2
	Trained operatives only to use power tools.
Tools to be PAT tested.
Use battery tools where possible.
110v power tools only.
Tools to be visually check before and after use. 

	3
	Trained/competent to use tools.
All tools to be inspected.
Tools to be safely stored when not in use.

	4
	Adequate ventilation in/around workspace where possible.
PPE where necessary i.e. face masks
COSHH assessment to be carried out 

	5
	All working areas to be kept clear.
Remove any trip hazards immediately if safe to do so.
Correct PPE i.e. Footwear 

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Fire from hot works
	1
	4
	4

	2
	Power tools
	2
	4
	8

	3
	Hand tools
	2
	2
	4

	4
	Fumes from soldering and solvent cement
	1
	4
	4

	5
	Trips/Slips/Falls
	2
	2
	4

	Name  Stuart Jones
Position  Site Manager
	Signed. S. Jones


	   Date of Completion: 30.03.2020

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury



	Activity to be Assessed
	Assessment Number

	Blockwork
	002

	Persons undertaking or affected by the activity

	

	
	×
	Employees
	×
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Falling from height
	3
	4
	12

	2
	Manual handling
	2
	2
	4

	3
	Material storage/Falling objects
	2
	2
	4

	4
	Cement burns
	2
	3
	6

	Existing Control Measures / Additional Control Measures Required

	1
	Operatives to be competent and trained.
Scaffolding to be erected by competent company/persons.
Ladders to be secured.
Harnesses to be used if needed.
Work carried out in compliance with working at height regulations.


	2
	In house manual handling training.
Clear any obstructions.
PPE

	3
	Blocks to be securely and correctly stacked.
Do not overload scaffolding platforms.
Brick guards on scaffolding.


	4
	Follow HSE guidelines
Appropriate washing facilities
PPE i.e. gloves/goggles

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Falling from height
	2
	4
	8

	2
	Manual Handling
	1
	2
	2

	3
	Material storage/falling objects
	1
	2
	2

	4
	Cement burns
	1
	3
	3

	Name  Stuart Jones
Position  Site Manager
	Signed. S. Jones


	   Date of Completion: 30.03.2020

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury




	Activity to be Assessed
	Assessment Number

	Slate Roofing
	003

	Persons undertaking or affected by the activity

	

	
	×
	Employees
	×
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Working at height
	2
	5
	10

	2
	Falling objects
	2
	4
	8

	3
	Manual handling
	2
	3
	6

	4
	Power tools
	2
	4
	8

	Existing Control Measures / Additional Control Measures Required

	1
	Work to be carried out by competent workers.
Platform to work from at correct height.
Harnesses where possible.
Correct roof ladders.

	2
	Close off work area below.
Warning signs of possible falling objects.
Hard hats to be worn at all times on site.

	3
	Manual handling training.
Mechanical lifts where possible.
PPE


	4
	Competent workers only to use tools.
Tools to be inspected before and after use.
Battery power tools where possible.
PAT testing

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Working at height
	1
	5
	5

	2
	Falling objects
	1
	4
	4

	3
	Manual handling
	1
	2
	2

	4
	Power tools
	1
	4
	4

	Name  Stuart Jones
Position  Site Manager
	Signed. S. Jones


	   Date of Completion: 30.03.2020

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury




Method Statement.
General precautions
The following are to be adhered to at all times by all workers when on site:-
Site Induction
All workers will have a site induction carried out by the site manager including safety talks, prior to the commencement of work and therefore will be expected to follow all safety guidelines. In house manual handling training will be given if required. 
PPE
All site workers/visitors will wear hard hats, safety boots and hi-vis vests. Dependant on job role other PPE items such as gloves, dust masks, ear plugs and safety goggles are to be worn when necessary.
Manual Handling
All workers will be mad aware of manual handling dangers. Workers will not try to lift any objects deemed too heavy for single a person. Heavy items must either be separated to make smaller loads where possible or dual lifted. Mechanical equipment to be available and used where necessary. 
Staff and training/sub-contractors
Work will be carried out by competent members of staff with the correct qualifications required. A supervisor will be appointed to ensure safety and quality of work. Apprentices and trainees will be supervised at all times and must not carry out any work that they are not competent in doing.
Tools and Electrical Equipment
All tools hand/power will be visually inspected before use, damaged items to be removed. Electrical tools are to be 110v and must have a current PAT certificate. Use of battery power tools where possible. Sub-contractors are not permitted to bring faulty or damaged tools on site. Site foreman will be responsible for ensuring all tool checks have been carried out and are fit for purpose.
Working at Height
As falling from height is the biggest cause of death in the workplace, all applicable workers to be made aware of the dangers and consequences of falling from height. All works will be properly planned and supervised. Conditions are to be deemed safe by the site foreman before working at height may commence and all workers are to be competent/trained in working at heights. Risk assessments to be carried out and safety measures put in place.
First Aid
A trained first aider will be appointed who is fully up to date with training. Adequate first aid kit will be available.  
Welfare
Toilet, washing facilities and break room facilities will be provided for staff and sub-contractors. The principal contractor is to ensure these facilities are well maintained and cleaned. Though all users are expected to clean after themselves as reasonably expected.  
Environmental Protection
· All waste and packaging to be disposed of in correct designated area.
· Hazardous materials/substances to be disposed of in compliance with local guidelines.
Preventative Measures
· Workers to be competent in their task
· Barriers and warning signs to be used where appropriate
· Correct safety equipment to be used/ available
· Visitors to enter only when accompanied by appropriate person and issued with PPE.
· Read all risk assessments and COSHH sheets associated with your tasks.












Specific Method Statements
Method Statement 1 – Plumbing and Heating
	1. Description of the Task/Activity:
	First fix Plumbing and Heating

	2. Project Name:
	UWTSD Care takers accommodation
	Project Ref:
	New build SA1

	3. Site Address/ Location:
	Kings road 
Saint Thomas
Swansea 
SA1 8AH
 
	Start Date/Time:
	01/07/20

	
	
	Finish Date/Time:
	3/07/20

	4. Personnel involved:
	Name
	Role/Trade

	
	Contractor
	Plumbing and Heating engineer

	
	Contractor
	Plumbing and Heating engineer

	5. Works Supervisor:	
	S Jones
	Role:
	Site Manager
	Tel:
	07807171110

	6. Key Plant and Tools Required:
	 Contractors to use own tools, tools to be correctly checked for faults.

	7. Key Materials Required:
	See plumbing specification

	8. Sequence of Operations:

	Report to site foreman for permit to work.
Put on personal protective equipment.
All plumbing first fix to be carried out as to plan. If hot works are to be carried out, hot works permit will be required from the site office. Two contractors to be present when hot works are being carried out. 



	9. Method of Access and egress to the work area:
	
Access from main road.
Parking only in designated area
Tools and equipment to be unloaded at designated location

	10. Fall Protection Measures: 

	Keep all walkways clear at all times externally and internally.
 Clear any spills up immediately.
Check ladders are safe to use, and 3 points of contact on ladder when in use.




	11. Exposure to Noise, Vibration, Dust and Chemicals
	All power tools to be analysed for noise and vibration levels, and the amount of time to use the equipment specified.
General site PPE, hard hats (to be checked they are still in date), safety boots and hi vis vests to be worn at all times. 
If drilling, the use of ear plugs, gloves, dust mask and safety goggles are required
The use of solvent weld will require a dust mask, gloves and safety goggles 
Take note of warning signs around the site

	Specific staff training
	Up to date cscs card.
Minimum NVQ level 2 plumbing
Gas safe registered where required


	12. Required Personnel Protective Equip.:
	[image: Boots]Safety Ankle Boots BS EN345
	[image: Hard Hats]Hard Hats BS EN 397
	[image: Gloves]Safety Gloves BS EN 388;1994
	[image: Ear Defenders]Ear Plugs BS EN 352-2;2002
	[image: Face Mask]Dust Mask
Task specific AS Above
FFP3
	[image: Goggles]Light Eye Protection
Task Specific BS EN 166
	Other:

1. Hi-Viz Top

2.

3. 

	
	Yes
	Yes
	Yes
	Yes
	Yes
	Yes
	

	13. Security and Emergency Procedures:
	Security cabin and security guard.
All tools and equipment to be stored in the secure storage at the end of each day.
Any access to height i.e. scaffolding or ladders to me made inaccessible
Any chemicals to be stored correctly and securely. 
Fire safety points clearly marked as advised on site induction




	
	14. First Aid Facilities:
	Name of On-Site First Aider:
	TBA

	
	
	First Aid Box Location:
	Site cabins



	
	
	Location of Nearest Hospital:
	Singleton Hospital, Sketty Ln, Sketty, Swansea SA2 8QA


	15. Other Information 
	
Break room cabins, washrooms and toilets to be situated opposite the site, by the technium 2 building.












Method Statement 2 – Slate roofing
	1,Description of the Task/Activity:
	Slate roofing

	2,Project Name:
	Care takers accommodation
	Project Ref:
	New build SA1

	3,Site Address/ Location:
	Kings road 
Saint Thomas
Swansea 
SA1 8AH
 
	Start Date/Time:
	22/06/20

	
	
	Finish Date/Time:
	06/07/20

	4,Personnel involved:
	Name
	Role/Trade

	
	Contractor
	Roofer

	
	Contractor
	Roofer

	5,Works Supervisor:	
	S Jones
	Role:
	Site Manager
	Tel:
	07807171110

	6,Key Plant and Tools Required:
	 Scaffolding.
 Ladders.
Tile lift
 MEWP’s where necessary/possible 

	7,Key Materials Required:
	Natural slate tiles 

	8,Other Essential Equipment:
	Harness


	9,Sequence of Operations:
(Specifying methods of working, tools, materials and equipment utilised)
	 Report to site foreman for permit to work 
Put on PPE.
Inform all contractors at start of work
Cordon off work area if practical and necessary to do so with barriers etc.
Ensure working area and exit points are clear of obstruction and safe
Large and/or heavy items will be assessed before lifting and carried by two or more persons if required.
   



	10,Method of Access and Egress to the work area:
	
Access from main road.
Parking only in designated area
Tools and equipment to be unloaded at designated location

	11,Fall Protection Measures: 
(Where work at height cannot be eliminated - consider both Personnel & Materials)
	All workers to be made aware of the dangers and consequences of falling from height.
Only competent workers to work at height 
All work at height to be supervised
Only work at height once ensuring working conditions are safe to do so 
Wearing and using correct PPE
Risk assessment to be carried out and followed.



	12,Exposure to Noise, Vibration and chemicals
	All power tools to be analysed for noise and vibration levels, and the amount of time to use the equipment specified.
General site PPE, hard hats (to be checked they are still in date), safety boots and hi vis vests to be worn at all times. 
If using angle grinder, the use of ear plugs, gloves, dust mask and safety goggles are required
The use of Portland cement will require a dust mask, gloves and safety goggles 
Take note of warning signs around the site

	13,Specific staff training
	Up to date CSCS card
NVQ level 2 roofing minimum
Working at heights 

	14. Required Personnel Protective Equip.:
	[image: Boots]Safety Ankle Boots BS EN345
	[image: Hard Hats]Hard Hats BS EN 397
	[image: Gloves]Safety Gloves BS EN 388;1994
	[image: Ear Defenders]Ear Plugs BS EN 352-2;2002
	[image: Face Mask]Dust Mask
Task specific AS Above
FFP3
	[image: Goggles]Light Eye Protection
Task Specific BS EN 166
	Other:

1. Hi-Viz Top

2.

3. 

	
	Yes
	Yes
	Yes
	Yes
	Yes
	Yes
	

	15,Security and Emergency Procedures:
	Security cabin and security guard.
All tools and equipment to be stored in the secure storage at the end of each day.
Any access to height i.e. scaffolding or ladders to me made inaccessible
Any chemicals to be stored correctly and securely. 
Fire safety points clearly marked as advised on site induction

	
	16,First Aid Facilities:
	Name of On-Site First Aider:
	TBA

	
	
	First Aid Box Location:
	Site cabins




	
	
	Location of Nearest Hospital:
	Singleton Hospital, Sketty Ln, Sketty, Swansea SA2 8QA


	17. Other information 
	
Break room cabins, washrooms and toilets to be situated opposite the site, by the technium 2 building.






Method Statement 3 - Blockwork
	1,Description of the Task/Activity:
	Block work

	2,Project Name:
	Care takers accommodation
	Project Ref:
	New build SA1

	3,Site Address/ Location:
	Kings road 
Saint Thomas 
Swansea
SA1 8AH
 
	Start Date/Time:
	18/05/20

	
	
	Finish Date/Time:
	015/07/20

	4,Personnel involved:
	Name
	Role/Trade

	
	Contractor
	Brick layer

	
	Contractor
	Brick layer

	5,Works Supervisor:	
	S Jones
	Role:
	Site Manager
	Tel:
	07807171110

	6,Key Plant and Tools Required:
	 Scaffolding.
 Ladders.



	7,Key Materials Required:
	Blocks
Sand and Cement

	8,Other Essential Equipment:
	Laser level
Chalk line


	9,Sequence of Operations:
(Specifying methods of working, tools, materials and equipment utilised)
	Report to site foreman for permit to work 
Put on PPE.
Inform all contractors at start of work
Cordon off work area if practical and necessary to do so with barriers etc.
Ensure working area and exit points are clear of obstruction and safe
Check all hand and power tools are safe to use, then take tools to work area. 
Stack blocks securely near to area of work
Carry out blockwork to drawings given ensuring walls are level and plumb
Build walls to specified level ready for scaffolding in order to carry on
Scaffolding to be erected by competent company

  

  
 

   



	10,Method of Access and Egress to the work area:
	
Access from main road.
Parking only in designated area
Tools and equipment to be unloaded at designated location

	11,Fall Protection Measures: 
(Where work at height cannot be eliminated - consider both Personnel & Materials)
	All workers to be made aware of the dangers and consequences of falling from height.
Only competent workers to work at height 
All work at height to be supervised
Only work at height once ensuring working conditions are safe to do so 
Wearing and using correct PPE
Risk assessment to be carried out and followed.



	12,Exposure to Noise, Vibration and chemicals
	All power tools to be analysed for noise and vibration levels, and the amount of time to use the equipment specified.
General site PPE, hard hats (to be checked they are still in date), safety boots and hi vis vests to be worn at all times. 
If using angle grinder, the use of ear plugs, gloves, dust mask and safety goggles are required
The use of Portland cement will require a dust mask, gloves and safety goggles 
Take note of warning signs around the site

	13,Specific staff training
	Up to date CSCS card
NVQ level 2 roofing minimum
Working at heights 

	14, Required Personnel Protective Equip.:
	[image: Boots]Safety Ankle Boots BS EN345
	[image: Hard Hats]Hard Hats BS EN 397
	[image: Gloves]Safety Gloves BS EN 388;1994
	[image: Ear Defenders]Ear Plugs BS EN 352-2;2002
	[image: Face Mask]Dust Mask
Task specific AS Above
FFP3
	[image: Goggles]Light Eye Protection
Task Specific BS EN 166
	Other:

1. Hi-Viz Top

2.

3. 

	
	Yes
	Yes
	Yes
	Yes
	Yes
	Yes
	

	15,Security and Emergency Procedures:
	Security cabin and security guard.
All tools and equipment to be stored in the secure storage at the end of each day.
Any access to height i.e. scaffolding or ladders to me made inaccessible
Any chemicals to be stored correctly and securely. 
Fire safety points clearly marked as advised on site induction

	
	16,First Aid Facilities:
	Name of On-Site First Aider:
	TBA

	
	
	First Aid Box Location:
	Site cabins




	
	
	Location of Nearest Hospital:
	Singleton Hospital, Sketty Ln, Sketty, Swansea SA2 8QA


	17. Other information 
	
Break room cabins, washrooms and toilets to be situated opposite the site, by the technium 2 building.














Key Legislations
The construction industry can be perceived as a dangerous environment, this is due largely to the fact that it has the largest death rate in the work place in the UK. The majority of deaths are reported due to falls from height (Health and Safety Executive, 2019). Therefore, Legislations and Regulations are put in place to try and keep harm and fatal accidents to a minimum.
The Health and Safety at Work Act 1974 is considered as the main legislation regarding the construction industry as it applies to every person in a work place. It is there to ensure all employers provide health, safety and welfare in the workplace for all employees. 
Because the legislation is an Act of Parliament, the legislation is Primary legislation. As such, primary legislation have the provisions to create secondary legislations under this Act, or regulations as they are referred too. 
Secondary regulations that were brought in, which cover the construction industry are:-
· Management of Health and Safety at Work Act 1999
· Manual Handling Operations Regulation 1992 
· Personal Protective Equipment at work Regulations 2002
· Provision and Use of Work Equipment Regulations 1998 
· Working at Height Regulations 2005
· Reporting of Injuries, Diseases and Dangerous Occurrences Regulations 2013 (RIDDOR)
· Gas Safety (installation and use) Regulations 1998
· ​Electricity at Work Regulations 1989
· Control of Substances Hazardous to Health Regulations 2002. (COSHH)
Even though COSHH covers hazardous materials it does not cover lead, asbestos or radioactive substances as they have their own regulations.
Construction Design and Management Regulations 2015 (CDM 2015) is considered the most well-known regulation in construction as it is specific to this sector. CDM was introduced in 2015 previously replacing CDM 2007, the purpose of CDM 2015 is in principle to carry out a detailed plan of the job, to identify possible risks before they happen and to put in controlled measures to reduce or eliminate those risks, such as employing the correct and qualified trades persons for the correct jobs and carrying out risk assessments. 
Health and safety needs to be implemented right at the start of any proposed works, and there are key roles/jobs that are to ensure that this is the case. 
It is the job of the principal designer to plan, manage and monitor the works before they begin, to ensure that all work can be carried out safely. 
The principal contractor must then also plan, manage and monitor all work, but continuously. Further, according to the CDM it is the sites co-ordinator to ensure that all workers on site be it employed or self-employed are adhering to general health and safety procedures.   
The client also has a key role in the health and safety of the proposed works, it is their responsibility to make the suitable arrangements for the project to be managed fairly giving sufficient time and resources. As long as the works can then be carried out without risk to the health or safety to any persons involved in the project, then it can be deemed suitable (The Construction (Design and Management) Regulations 2015).
It is imperative that all Health and Safety guidelines, legislations and regulations are followed in order to prevent harm and/or fatalities. Therefore, there is an onus on every contractor, employer and employees to ensure their own health and safety is carried out.
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