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This is an individual practical lab-test, held under examination conditions. You will be assigned 3 Routers, 2 Switches and two PCs; you should configure these devices based on the following specifications. 

This paper is marked out of 100.
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Task 1: IP addressing scheme (5 marks)

	Device
	Interface
	IP Address
	Subnet Mask
	IPv6 Address

	R1
	Ge0/1
	
	
	

	
	S0/0/0
	
	
	

	
	
	
	
	Link-local:

	R2
	S0/0/0
	
	
	

	
	
	
	
	Link-local:

	
	S0/0/1
	
	
	

	
	
	
	
	Link-local:

	
	Ge0/0
	
	
	

	
	
	
	
	Link-local:

	
	Lo0
	
	
	

	R3
	S0/0/1
	
	
	

	
	
	
	
	Link-local:

	
	Lo4
	
	
	

	
	Lo5
	
	
	

	
	Lo6
	
	
	

	
	Lo7
	
	
	

	S1
	VLAN99
	
	
	

	S2
	VLAN99
	
	
	

	Internet Server
	
	
	
	

	
	
	
	
	Link-local:



	

Task 2: Network Connection (5 Marks)
	
Physically cable the network as shown in the topology diagram. 


Task 3: Configure the basic configuration (10 Marks)

1. Configure all devices with hostname
2. Disable DNS lookup 
3. Configure all devices with interfaces as shown in the topology. 
4. Configure Internet PC with IPv4 and IPv6 address. 
Part 2: 






Task 4: Configure Routers and Switches (65 marks)

1. Configure RIPv2 on all routers and advertise networks shown in the topology. Disable auto summary.
2. Configure IPv6 static route with exit interface on all routers.  
3. On R2, configure IPV4 and IPv6 default route out Gi0/0 
4. On S1 and S2, configure VLANs
5. Assign the IPv4 address to Management VLAN on S1 and S2. 
6. Assign default gateway on switches
7. On S1, force trunking on Fa0/5 and Fa0/3. Use VLAN1 as the Native VLAN
8. on S2, force trunking on Fa0/3. Use VLAN1 as the Native VLAN. 
9. On S1, assign Fa0/6 to VLAN21 and on S2, assign Fa0/18 to VLAN23.
10. On both switches, shutdown all unused ports.
11. Configure Router-on-Stick inter-VLAN routing.
12. On all Routers, configure all Loopback and Ethernet interfaces as passive.  
13. Configure R1 as the DHCP server for VLANs 21 and 23. Reserve first 10 IP addresses for static configurations. 

	VLAN21: Name: ACCT
DNS-Server: 10.10.10.10
Domain-Name: SoAC.com
Set the default gateway
	Name: ENGNR
DNS-Server: 10.10.10.10
Domain-Name: SoAC.com
Set the default gateway.


 
14. Create a local database with 1 user account: username: webuser, password: soac1234, privilege: 15. 
15. On R2, configure a static NAT to the Web Server. Assign the inside and outside interface for static NAT.
16. Configure the dynamic NAT. Allow VLAN 21 and 23 networks on R1 to be translated. 
17. Define the pool of usable public IP addresses, 209.165.200.225 to 209.165.200.228.
18. Define the dynamic NAT translation. 



Task 5: Verify connectivity (15 marks)

After configuring each host computer, record the host network settings with the ipconfig /all command. 


	Host PC-A Network Configuration

	Description
	

	Physical Address
	

	IP Address
	

	Subnet Mask
	

	Default Gateway
	



	Host PC-B Network Configuration

	Description
	

	Physical Address
	

	IP Address
	

	Subnet Mask
	

	Default Gateway
	




Verify PC-A can ping PC-B. Is it successful? __________________

Use a Web browser on the Internet PC to access the Web Server (209.165.200.229). Login with Username: webuser and password: soac1234.
Is the Web server accessible? _____________________________




Submission Requirement 
On each device the following outputs should be copied on to a text file. The file name should be as studentname_Pno_routername.txt

Show running-configuration
Show ip interface brief
Show ip route

All documentation for your solution should be submitted electronically on Moodle.
It is your responsibility that you copy all the outputs and files correctly.
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