	
Router>?
Exec commands:
  access-profile   Apply user-profile to interface
  app-hosting      Application hosting
  clear            Reset functions
  connect          Open a terminal connection
  crypto           Encryption related commands.
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  do-exec          Mode-independent "do-exec" prefix support
  enable           Turn on privileged commands
  ethernet         Ethernet parameters
  exit             Exit from the EXEC
  help             Description of the interactive help system
  ip               IP SLA Exec Command
  license          Smart licensing Commands
  lock             Lock the terminal
  login            Log in as a particular user
  logout           Exit from the EXEC
  mrinfo           Request neighbor and version information from a multicast
                   router
  mstat            Show statistics after multiple multicast traceroutes
  mtrace           Trace reverse multicast path from destination to source
  name-connection  Name an existing network connection
  ping             Send echo messages
  ppp              Start IETF Point-to-Point Protocol (PPP)
  release          Release a resource
  renew            Renew a resource
  resume           Resume an active network connection
  rlogin           Open an rlogin connection
  routing-context  Routing Context
  set              Set system parameter (not config)
  show             Show running system information
  slip             Start Serial-line IP (SLIP)
  ssh              Open a secure shell client connection
  systat           Display information about terminal lines
  tclquit          Quit Tool Command Language shell
  telnet           Open a telnet connection
  terminal         Set terminal line parameters
  traceroute       Trace route to destination
  tunnel           Open a tunnel connection
  where            List active connections
  who              who

Router>config t
          ^
% Invalid input detected at '^' marker.

Router>ip add
          ^
% Invalid input detected at '^' marker.

Router>en
Router#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#?
Configure commands:
  aaa                         Authentication, Authorization and Accounting.
  access-list                 Add an access list entry
  access-session              Access Sesion Global Configuration Commands
  accounting                  Policy accounting feature
  alg                         ALG configuration commands
  alias                       Create command alias
  ancp                        Configure ANCP
  app-hosting                 Application hosting configuration mode
  archive                     Archive the configuration
  arp                         Set a static ARP entry
  async-bootp                 Modify system bootp parameters
  authentication              Auth Manager Global Configuration Commands
  autoconf                    Configure autoconf
  avc                         Application visibility and control
  banner                      Define a login banner
  bba-group                   Configure BBA Group
  beep                        Configure BEEP (Blocks Extensible Exchange
                              Protocol)
  bfd                         BFD configuration commands
  bfd-template                BFD template configuration
  boot                        Modify system boot parameters
  boot-end-marker             boot-end-marker
  boot-start-marker           boot-start-marker
  bridge                      Bridge Group.
  bridge-domain               Bridge-domain global configuration commands

Router(config)#ostname
                ^
% Invalid input detected at '^' marker.

Router(config)#hostname
% Incomplete command.

Router(config)#exe
                 ^
% Invalid input detected at '^' marker.

Router(config)#hostname R1
R1(config)#config int
                  ^
% Invalid input detected at '^' marker.

R1(config)#config t
                  ^
% Invalid input detected at '^' marker.

R1(config)#ip address 192.168.30.1 255.255.255.0
                     ^
% Invalid input detected at '^' marker.

R1(config)#int g0/1
% Incomplete command.

R1(config)#int g0/1.10
                   ^
% Invalid input detected at '^' marker.

R1(config)#int g0/1
% Incomplete command.

R1(config)#em
            ^
% Invalid input detected at '^' marker.

R1(config)#int G0/0/1.11
R1(config-subif)#ip address 209.165.201 255.255.255
                                       ^
% Invalid input detected at '^' marker.

R1(config-subif)#int G0/0/1.11
R1(config-subif)#
Switch>#config t
Switch>en
Switch#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Switch(config)#int vlan 9
Switch(config-if)#
*Aug 21 10:10:48.681: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan9, cha              nged state to down
Switch(config-if)#ip address 192.168.40.2
% Incomplete command.

Switch(config-if)#ip address 192.168.40.2 255.255.255.0
Switch(config-if)#no shutdown
Switch(config-if)#exit
Switch(config)#ip default-gateway 192.168.40.1
Switch(config)#?
Configure commands:
  aaa                         Authentication, Authorization and Accounting.
  access-list                 Add an access list entry
  access-session              Access Sesion Global Configuration Commands
  alias                       Create command alias
  archive                     Archive the configuration
  arp                         Set a static ARP entry
  authentication              Auth Manager Global Configuration Commands
  auto                        Configure Automation
  autoconf                    Configure autoconf
  banner                      Define a login banner
  beep                        Configure BEEP (Blocks Extensible Exchange
                              Protocol)
  boot                        Modify system boot parameters
  buffers                     Adjust system buffer pool parameters
  bulkstat                    Bulkstat Application
  call-home                   Enter call-home configuration mode
  captive-portal-bypass       Enable Captive portal bypass for apple devices
  cdp                         Global CDP configuration subcommands
  cfg-mode                    Enter configuration mode
  cisp                        Set CISP parameters
  class-map                   Configure CPL Class Map

Switch(config)#1
               ^
% Invalid input detected at '^' marker.

Switch(config)#en
% Incomplete command.

Switch(config)#config t
                     ^
% Invalid input detected at '^' marker.

Switch(config)#en
% Incomplete command.

Switch(config)#vlan9
                   ^
% Invalid input detected at '^' marker.

Switch(config)#vlan 9
Switch(config-vlan)#name S1
Switch(config-vlan)#name S1
Switch(config-vlan)#S1
                     ^
% Invalid input detected at '^' marker.

Switch(config-vlan)#vlan9
                    ^
% Invalid input detected at '^' marker.

Switch(config-vlan)#int vlan9
Switch(config-if)#hostname S1
S1(config)#line console
% Incomplete command.

S1(config)#line consolo 0
                      ^
% Invalid input detected at '^' marker.

S1(config)#enable password
% Incomplete command.

S1(config)#enable password cisco123
 WARNING: Command has been added to the configuration using a type 0 password. H              owever, type 0 passwords will soon be deprecated. Migrate to a supported passwor              d type
S1(config)#
*Aug 21 10:24:40.373: %AAAA-4-CLI_DEPRECATED: WARNING: Command has been added to               the configuration using a type 0 password. However, type 0 passwords will soon               be deprecated. Migrate to a supported password type
S1(config)#login
% Incomplete command.

S1(config)# noip domanin-lookup
              ^
% Invalid input detected at '^' marker.

S1(config)#en
% Incomplete command.

S1(config)#configt
                 ^
% Invalid input detected at '^' marker.

S1(config)#config t
                 ^
% Invalid input detected at '^' marker.

S1(config)#no
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*Aug 21 10:35:57.818: %SYS-5-CONFIG_I: Configured from console by console
S1>interface
Translating "interface"...domain server (255.255.255.255)
% Unknown command or computer name, or unable to find computer address
S1>ping 192.17
% Unrecognized host or address, or protocol not running.

S1>ping 192.168.10.4
Type escape sequence to abort.
Sending 5, 100-byte ICMP Echos to 192.168.10.4, timeout is 2 seconds:
.....
Success rate is 0 percent (0/5)
S1>en
Password:
S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#int vlan
% Incomplete command.

S1(config)#int vlan
% Incomplete command.

S1(config)#int vlan9
S1(config-if)#ip address 192.168.10.2
% Incomplete command.

S1(config-if)#ip
% Incomplete command.

S1(config-if)#ip address 192.168.10.2 255.255.255.0
S1(config-if)#ip address 192.168.10.2 255.255.255.0
S1(config-if)#
R1>
R1>
R1>int 0/0/1
    ^
% Invalid input detected at '^' marker.

R1>int f0/5
    ^
% Invalid input detected at '^' marker.

R1>int f0/0
    ^
% Invalid input detected at '^' marker.

R1>en
R1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#int 0/0/0
               ^
% Invalid input detected at '^' marker.

R1(config)#int f0/5
% Incomplete command.

R1(config)#int f0/5
% Incomplete command.

R1(config)#int g0/5
% Incomplete command.

R1(config)#int 0?
% Unrecognized command
R1(config)#?
Configure commands:
  aaa                         Authentication, Authorization and Accounting.
  access-list                 Add an access list entry
  access-session              Access Sesion Global Configuration Commands
  accounting                  Policy accounting feature
  alg                         ALG configuration commands
  alias                       Create command alias
  ancp                        Configure ANCP
  app-hosting                 Application hosting configuration mode
  archive                     Archive the configuration
  arp                         Set a static ARP entry
  async-bootp                 Modify system bootp parameters
  authentication              Auth Manager Global Configuration Commands
  autoconf                    Configure autoconf
  avc                         Application visibility and control
  banner                      Define a login banner
  bba-group                   Configure BBA Group
  beep                        Configure BEEP (Blocks Extensible Exchange
                              Protocol)
  bfd                         BFD configuration commands
  bfd-template                BFD template configuration
  boot                        Modify system boot parameters
  boot-end-marker             boot-end-marker

R1(config)#int 0/0/1
               ^
% Invalid input detected at '^' marker.

R1(config)#int 0/0/1
               ^
% Invalid input detected at '^' marker.

R1(config)#int G0/0/0/1
                     ^
% Invalid input detected at '^' marker.

R1(config)#int G0/0/1
R1(config-if)#bash
                ^
% Invalid input detected at '^' marker.

R1(config-if)#ip domain-name
                  ^
% Invalid input detected at '^' marker.

R1(config-if)#exit
R1(config)#ip domain-name swre-lab.com
                    ^
% Invalid input detected at '^' marker.

R1(config)#en
% Incomplete command.

R1(config)#en
% Incomplete command.

R1(config)#ip domain-name swre-lab.com
                    ^
% Invalid input detected at '^' marker.

R1(config)#int G0/0/1
R1(config-if)##
R1(config-if)#bash
                ^
% Invalid input detected at '^' marker.

R1(config-if)#ip domain-name
                  ^
% Invalid input detected at '^' marker.

R1(config-if)#
R1(config-if)#
R1(config-if)#
R1(config-if)#ip domain-name
                  ^
% Invalid input detected at '^' marker.

R1(config-if)#exit
R1(config)#ip domain-name swre-lab.com
                    ^
% Invalid input detected at '^' marker.

R1(config)#ip domain-name
                    ^
% Invalid input detected at '^' marker.

R1(config)#ipeswre-lab.com
             ^
% Invalid input detected at '^' marker.

R1(config)#ip eswre-lab.com
               ^
% Invalid input detected at '^' marker.

R1(config)#
S1>
S1>en
Password:
S1#cong t
      ^
% Invalid input detected at '^' marker.

S1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#ip domain-name swre-lab.com
S1(config)#enable secret
% Incomplete command.

S1(config)#emable secret cisco123
            ^
% Invalid input detected at '^' marker.

S1(config)#enable secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#login
% Incomplete command.

S1(config)#line console 0
S1(config-line)#password cisco123
S1(config-line)#login
S1(config-line)#enable secret password
S1(config)#exit
S1#
*Aug 21 11:27:58.853: %SYS-5-CONFIG_I: Configured from console by console
S1#en
S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#ip domain-name swre-lab.com
S1(config)#enable secret
% Incomplete command.

S1(config)#enable secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#cisco123
              ^
% Invalid input detected at '^' marker.

S1(config)#login
% Incomplete command.

S1(config)#enable secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#cisco123
              ^
% Invalid input detected at '^' marker.

S1(config)#enable secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#line console 0
S1(config-line)#
S1(config-line)#pasword cisco123
                   ^
% Invalid input detected at '^' marker.

S1(config-line)#login
S1(config-line)#login
S1(config-line)#en
                 ^
% Invalid input detected at '^' marker.

S1(config-line)#logion
                    ^
% Invalid input detected at '^' marker.

S1(config-line)#login
S1(config-line)#concole 0
                ^
% Invalid input detected at '^' marker.

S1(config-line)#enable secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#enable secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#
S1(config)#
S1(config)#
S1(config)#
S1(config)#
S1(config)#
S1(config)#conf t
               ^
% Invalid input detected at '^' marker.

S1(config)#en
% Incomplete command.

S1(config)#conf t
               ^
% Invalid input detected at '^' marker.

S1(config)#config t
                 ^
% Invalid input detected at '^' marker.

S1(config)#en
% Incomplete command.

S1(config)#
R1>
R1>
R1>en
R1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#no 1p domain-lookup
              ^
% Invalid input detected at '^' marker.

R1(config)#no ip domain-lookup
                       ^
% Invalid input detected at '^' marker.

R1(config)#service password encryption
                            ^
% Invalid input detected at '^' marker.

R1(config)#en
% Incomplete command.

R1(config)#config t
                  ^
% Invalid input detected at '^' marker.

R1(config)#exit
R1#
*Aug 21 11:51:22.485: %SYS-5-CONFIG_I: Configured from console by console
S1(config)#en
% Incomplete command.

S1(config)#config t
                 ^
% Invalid input detected at '^' marker.

S1(config)#config t
                 ^
% Invalid input detected at '^' marker.

S1(config)#en
% Incomplete command.

S1(config)#en
% Incomplete command.

S1(config)#enable
% Incomplete command.

S1(config)#configure terminal
                   ^
% Invalid input detected at '^' marker.

S1(config)#
Switch>en
Switch#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Switch(config)#hostname 2
% Hostname contains one or more illegal characters.

2(config)#hostname S2
S2(config)#no ip domain-lookup
S2(config)#enable secret cisco123
S2(config)#service password-encryption
S2(config)#username cisco privilege 15 secret cisco123
S2(config)#linevt
               ^
% Invalid input detected at '^' marker.

S2(config)#line vty 0 4
S2(config-line)#login local
S2(config-line)#transport input ssh
S2(config-line)#exit
S2(config)#interface range f0/1 - 2
                           ^
% Invalid input detected at '^' marker.

S2(config)#interface range f0/1 - 2
                           ^
% Invalid input detected at '^' marker.

S2(config)#interface range f0/1
                           ^
% Invalid input detected at '^' marker.

S2(config)#

User Access Verification

Password:
S1>en
Password:
S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#vlan 7
S1(config-vlan)#vlan 7
S1(config-vlan)#name London
S1(config-vlan)#vlan8
                ^
% Invalid input detected at '^' marker.

S1(config-vlan)#save
                  ^
% Invalid input detected at '^' marker.

S1(config-vlan)#show ip interface
                  ^
% Invalid input detected at '^' marker.

S1(config-vlan)#show run
                  ^
% Invalid input detected at '^' marker.

S1(config-vlan)#show ip interface brief
                  ^
% Invalid input detected at '^' marker.

S1(config-vlan)#exit
S1(config)#exit
S1#
*Aug 21 12:18:17.850: %SYS-5-CONFIG_I: Configured from console by console
S1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
7    London                           active
9    S1                               active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0

S1#show interface brief
                   ^
% Invalid input detected at '^' marker.

S1#exit
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User Access Verification

Password:
S1>en
Password:
S1#run
Translating "run"...domain server (255.255.255.255)
% Unknown command or computer name, or unable to find computer address
S1# show ru
Building configuration...

Current configuration : 1845 bytes
!
! Last configuration change at 12:18:17 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$oloVoa/2JTtu/Z$oVcepVxNAYa5FkCq5GLffIeFaiN9XbH.yf/.mhb03pU
enable password cisco123
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan9
 ip address 192.168.10.2 255.255.255.0
!
ip default-gateway 192.168.40.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password cisco123
 login
line vty 0 4
 login
 transport input none
line vty 5 15
 login
 transport input none
!
end

S1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
Vlan9                  192.168.10.2    YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
7    London                           active
9    S1                               active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
7    enet  100007     1500  -      -      -        -    -        0      0
9    enet  100009     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S1#
R1>en
R1#show ip interface brief
Any interface listed with OK? value "NO" does not have a valid configuration

Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   unassigned      YES unset  administratively down down
Gi0/0/1.11             unassigned      YES unset  administratively down down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      NO  unset  down                  down
Serial0/1/1            unassigned      NO  unset  down                  down
R1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

R1#show runing config
           ^
% Invalid input detected at '^' marker.

R1#show config
startup-config is not present
R1#show run
R1#show running-config
Building configuration...

Current configuration : 5934 bytes
!
! Last configuration change at 11:51:22 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-2451180461
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2451180461
 revocation-check none
 rsakeypair TP-self-signed-2451180461
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-2451180461
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 32343531 31383034 3631301E 170D3234 30383231 30383033
  34315A17 0D333430 38323130 38303334 315A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 34353131
  38303436 31308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100D29E CFDDF758 6715DCB0 23420DDF 50CD1BED D8189DAA 1DCB1692
  40845BCA E2930B87 66A834A2 4DD7336F 24005B2C 58EB67A1 4E7FD174 926F5282
  AC4374F9 7BB68985 7FC61FD9 C08B65B5 2F9C3897 4BC3DC0C C7A8D7F3 06892CBE
  4AA9EB25 423E0C04 F9E53F18 ABA9183C 64D87242 CB860905 2F57B027 D2C4401C
  5D08FB0E 1A86BF72 1E51C5AD 6DB6ED7E 7F1C71B3 15E24658 9EAC4184 B0E4D2A2
  FA90B49A A564C63B 59E4E59A 917BEF2E B2DA3F42 57574598 78B84DC5 16D40161
  7725B4AA 2ACD3DA9 B449ECC6 307A87EE E7D1E096 11CC4458 AB9404AE EDFA2A75
  892C51B0 982590ED B61D5298 F3DDBDFA FD3E9C34 48D5EDAD 5D203725 F26668C5
  B77AEB43 D52B0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14853668 C42AB220 F51C193A 60619692 DB60492E
  93301D06 03551D0E 04160414 853668C4 2AB220F5 1C193A60 619692DB 60492E93
  300D0609 2A864886 F70D0101 05050003 82010100 124626C9 736ED569 1567E6EC
  605FA8A8 8D8B3E24 EDB33D61 98ED20D6 41F7CA1E 521264A4 93C41685 655170CE
  FB7438F2 5F54C52F CAB8FCFA A277D0E6 18D979EC 878D0FED 0EE26994 2F2BD442
  9A4CD04F A11E60A0 67A7F7C4 82841E9F E37153A8 FA6DBF19 82A9D18C B6331535
  D1D2116C 3AC2CF95 55999EC8 CFAA17E5 484B72B6 D41C62A4 770F224C D38E9763
  6E5B398C F0D58DCB 0C000BDD 36EC2AF1 06DD6028 A7CF0481 2D32902A A43B74E5
  4D3D7FFD AAE3FD3E 1DA9C414 A784A61A D31A6AA1 EFE727DC BB7FFE75 97AD9744
  62F5A78E 54519434 A5409D61 44E926E3 8D286F2F EECBF89B 046D1FBB 37FBDEE9
  427A2E7A 7991BE67 30760CD6 355077AE 648B6B4F
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0P5
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1.11
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
!
interface Serial0/1/1
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 stopbits 1
line aux 0
line vty 0 4
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@ci              sco.com
 ! the email address configured in Cisco Smart License Portal will be used as co              ntact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#
S2>show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S2>show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
10   Operations                       active
20   CarPark                          active
99   Management                       active
1000 Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
10   enet  100010     1500  -      -      -        -    -        0      0
20   enet  100020     1500  -      -      -        -    -        0      0
99   enet  100099     1500  -      -      -        -    -        0      0
1000 enet  101000     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S2> show run
          ^
% Invalid input detected at '^' marker.

S2>en
Password:
Password:
S2#show run
Building configuration...

Current configuration : 1788 bytes
!
! Last configuration change at 12:11:16 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$pzd0O/180u8du3$dxMRRra0XbFEa3mQu6va6zjVFhUdOoxTCbLGpPLv0tQ
!
username cisco privilege 15 secret 9 $9$D5Ekkp7rh3YhZp$ySV08xxQayocKcl/2X.uBwVDZ              W.fmy9Zsc2lDZl8llw
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
ip http server
ip http secure-server
!
!
!
!
line con 0
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login
 transport input none
!
end

S2#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S2#
S1#show up interface brief
         ^
% Invalid input detected at '^' marker.

S1#en
S1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
Vlan9                  192.168.10.2    YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down

S1#how vlan
    ^
% Invalid input detected at '^' marker.

S1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
7    London                           active
9    S1                               active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
7    enet  100007     1500  -      -      -        -    -        0      0
9    enet  100009     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S1#show run
Building configuration...

Current configuration : 1845 bytes
!
! Last configuration change at 12:18:17 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$oloVoa/2JTtu/Z$oVcepVxNAYa5FkCq5GLffIeFaiN9XbH.yf/.mhb03pU
enable password cisco123
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan9
 ip address 192.168.10.2 255.255.255.0
!
ip default-gateway 192.168.40.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password cisco123
 login
line vty 0 4
 login
 transport input none
line vty 5 15
 login
 transport input none
!
end

S1#
S1#show ip interface brief
Any interface listed with OK? value "NO" does not have a valid configuration

Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   unassigned      YES unset  administratively down down
Gi0/0/1.11             unassigned      YES unset  administratively down down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      NO  unset  down                  down
Serial0/1/1            unassigned      NO  unset  down                  down
R1#
R1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

R1#show run
Building configuration...

Current configuration : 5934 bytes
!
! Last configuration change at 11:51:22 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-2451180461
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2451180461
 revocation-check none
 rsakeypair TP-self-signed-2451180461
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-2451180461
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 32343531 31383034 3631301E 170D3234 30383231 30383033
  34315A17 0D333430 38323130 38303334 315A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 34353131
  38303436 31308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100D29E CFDDF758 6715DCB0 23420DDF 50CD1BED D8189DAA 1DCB1692
  40845BCA E2930B87 66A834A2 4DD7336F 24005B2C 58EB67A1 4E7FD174 926F5282
  AC4374F9 7BB68985 7FC61FD9 C08B65B5 2F9C3897 4BC3DC0C C7A8D7F3 06892CBE
  4AA9EB25 423E0C04 F9E53F18 ABA9183C 64D87242 CB860905 2F57B027 D2C4401C
  5D08FB0E 1A86BF72 1E51C5AD 6DB6ED7E 7F1C71B3 15E24658 9EAC4184 B0E4D2A2
  FA90B49A A564C63B 59E4E59A 917BEF2E B2DA3F42 57574598 78B84DC5 16D40161
  7725B4AA 2ACD3DA9 B449ECC6 307A87EE E7D1E096 11CC4458 AB9404AE EDFA2A75
  892C51B0 982590ED B61D5298 F3DDBDFA FD3E9C34 48D5EDAD 5D203725 F26668C5
  B77AEB43 D52B0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14853668 C42AB220 F51C193A 60619692 DB60492E
  93301D06 03551D0E 04160414 853668C4 2AB220F5 1C193A60 619692DB 60492E93
  300D0609 2A864886 F70D0101 05050003 82010100 124626C9 736ED569 1567E6EC
  605FA8A8 8D8B3E24 EDB33D61 98ED20D6 41F7CA1E 521264A4 93C41685 655170CE
  FB7438F2 5F54C52F CAB8FCFA A277D0E6 18D979EC 878D0FED 0EE26994 2F2BD442
  9A4CD04F A11E60A0 67A7F7C4 82841E9F E37153A8 FA6DBF19 82A9D18C B6331535
  D1D2116C 3AC2CF95 55999EC8 CFAA17E5 484B72B6 D41C62A4 770F224C D38E9763
  6E5B398C F0D58DCB 0C000BDD 36EC2AF1 06DD6028 A7CF0481 2D32902A A43B74E5
  4D3D7FFD AAE3FD3E 1DA9C414 A784A61A D31A6AA1 EFE727DC BB7FFE75 97AD9744
  62F5A78E 54519434 A5409D61 44E926E3 8D286F2F EECBF89B 046D1FBB 37FBDEE9
  427A2E7A 7991BE67 30760CD6 355077AE 648B6B4F
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0P5
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1.11
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
!
interface Serial0/1/1
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 stopbits 1
line aux 0
line vty 0 4
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@ci              sco.com
 ! the email address configured in Cisco Smart License Portal will be used as co              ntact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#
