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Lab 2: Design a Simple Network with 2 PC's connected to a Switch.
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Warm-up
Based on your acquired skills from previous lab works, complete the following.
Build a Simple Network as per the topology given below Configure the IP Address as per the addressing table Use Ping Utility to check if the connection is successful.
(Save the file as Lab2_ Student_ID) and submit it via Moodle Link ONLY
Topology:
[image: ]

Addressing Table

	Device
	Interface
	IP Address
	Subnet Mask

	PC-A
	NIC
	192.168.1.10
	255.255.255.0

	PC-B
	NIC
	192.168.1.11
	255.255.255.0



Record your outcome: Is the Ping between PC- A and PC- B Successful? The ping was successful.

[image: ]
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Objectives
Every computer on an Ethernet local network has a Media Access Control (MAC) address that is burned into the Network Interface Card (NIC). Computer MAC addresses are usually displayed as 6 sets of two hexadecimal numbers separated by dashes
 
or
 
colons
 
(exam
ple:
 
15-EF-A3-45-9B-57).
 
The
 
ipconfig
 
/all
 
command
 
displays the computer MAC
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Determine
 
the
 
MAC
 
address
 
of
 
a
 
Windows
 
computer
 
on
 
an
 
Ethernet
 
network
 
using the ipconfig /all
 
command.
Analyze
 
a
 
MAC
 
address
 
to
 
determine
 
the
 
manufacturer.
Analyze the Wired and Wireless Network
 
connection.
Analyze Address Resolution Protocol
 
(ARP).
)
Requirements
· PC running Windows 10 with at least one Ethernet network interface card (NIC) or the above created Topology in Packet Tracer.
· Connectivity to the Internet

Task 1: Determine the MAC address of a Windows computer on an Ethernet network using the ipconfig /all command.

(From the previous lab, you should know the step-by-step procedure to execute a “PING”/ “TRACERT” command in a Packet Tracer) – Execute those steps, if you work with Packet Tracer.
In your PC

[bookmark: Step_1:_Open_a_Windows_command_prompt_wi]Step 1: Open a Windows command prompt window
Right-click on the Start button and select Command Prompt.
[image: ]

[bookmark: Step_2:_Use_the_ipconfig_/all_command]Step 2: Use the ipconfig /all command
Enter the ipconfig /all command at the command prompt. Press Enter. (Typical results are shown in the following figure, but your computer will display different information.)


[image: ]

[bookmark: Step_3:_Locate_the_MAC_(physical)_addres]Step 3: Locate the MAC (physical) address(es) in the output from the ipconfig
/all command
Use the table below to fill in the description of the Ethernet adapter and the Physical (MAC) Address:

	Description
	Physical Address

	Intel(R) Ethernet Connection (2) I219-V
	A8-A1-59-29-88-E6

	Npcap Loopback Adapter
	02-00-4C-4F-4F-50

	
	


How many MAC addresses did you discover in your PC?  2	


Task 2: Analyzing the Parts of a MAC Address
Every Ethernet network interface has a physical address assigned to it when it is manufactured. These addresses are 48 bit (6 bytes) long and are written in hexadecimal notation.
MAC addresses are made up of two parts.
One part of the MAC address, the first 3 bytes, represents the vendor who manufactured the network interface. This part of the MAC is called the OUI (Organizationally Unique Identifier). Each vendor who wants to make and sell Ethernet network interfaces must register with the IEEE in order to be assigned an OUI.
The second part of the address, the remaining 3 bytes are the unique ID for the interface. All MAC addresses that begin with the same OUI must have unique values in the last 3 bytes.
In the example shown in the lab, the physical MAC address for the Ethernet LAN interface is D4-BE-D9-13-63-00.


	
Manufacturer OUI
	Unique Identifier for the Interface
	
Vendor Name

	D4-BE-D9
	13-63-00
	Dell Incorporated



[bookmark: Step_4:_List_MAC_addresses_discovered_by]Step 4: List MAC addresses discovered by you in Part 1.
List the 3-byte Manufacturer OUI and the 3-byte unique interface identifier. You will fill in the Vendor name in Step 2.

	
Manufacturer OUI
	Unique Identifier for the Interface
	
Vendor Name

	D4-BE-D9
	13-63-00
	Dell Incorporated

	A8-A1-59
	29-88-E6
	ASRock Incorporation

	02-00-4C
	4F-4F-50
	No Matches



[bookmark: Step_5:_Lookup_the_vendors_who_are_the_r]Step 5: Lookup the vendors who are the registered owners of the OUI that you listed in the table.
a. Wireshark.org provides an easy to use lookup tool at https://www.wireshark.org/tools/oui-lookup.html. Use this tool, or use the Internet to search for other ways to identify an OUI.
[image: ]
b. Use the information that you found to update the vendor column in the chart in Step 1. How many different vendors did you discover?   1	

Record your Reflection
1. Why might a computer have more than one MAC address?
MAC Addresses are based on the networks a device has, most computers nowadays have more networks they can connect to, which means they need a mac address for each network they can connect to. For example, my pc has only an ethernet cable so only has 1 mac address.




2. Try connecting and disconnecting the network cable(s) to your network adapter(s) and use the ipconfig /all again. What changes do you see? Does the MAC address still display? Will the MAC address ever change?
The display has changed, because there is no connection all information about the network is no longer being displayed, however there are still 2 MAC addresses being displayed. 




3. What are other names for the MAC address?
from what I have researched a MAC address has other names: burned-in address, Ethernet hardware address, hardware address, and physical address.


Task 3: Wired and Wireless Network Connection.

[bookmark: Step_6:_Open_the_Network_Connections_win]Step 6: Open the Network Connections window by right-clicking the Windows Start button > Network Connections.

[bookmark: Step_7:_The_Network_Connections_window_d]Step 7: The Network Connections window displays the list of NICs available on this PC. Look for your Local Area Connection and Wireless Network Connection adapters in this window.
[image: ]

Note: Other types of network adapters, such as Bluetooth Network connection and Virtual Private Network (VPN) adapter, may also be displayed in this window.
Verify the wireless network connection settings
Step 8: Select the Wireless Network Connection option. Right-click on it to display a drop-down list. The first option displays if your wireless NIC is enabled or disabled. Currently, this NIC is enabled which is why the Disable option is displayed. If your wireless NIC is disabled, you will have an option to Enable it.
[image: ]

[image: ]Step 9: Click Status to open the Wireless Network Connection Status window.
What is the Service Set Identifier (SSID) for the wireless router of your connection?
 Glide	_ 	
What is the speed of your wireless connection?
 173.3 mbps	_ 	

Step 10: Click Details to display the Network Connection Details window.
[image: ]

What is the MAC address of your wireless NIC?
 E4-5E-37-9D-C6-A0	_	_


Step 11: Open a command window prompt and type ipconfig /all.
C:\Users\Bob> ipconfig /all
[image: ]

Notice the information displayed is similar to the Network Connection Details window information. When you have reviewed the details, click Close to return to the Wireless Network Connection Status window.

[image: ]Step 12: Return to the Wireless Network Connection Status window. Click Wireless Properties to open the Wireless Network Properties window of the Home-Net network.
Step 13: You should always use wireless security whenever available. To verify (or configure) the wireless security options click on the Security tab.
[image: ]
The window displays the type of security and encryption method enabled. You can also enter (or change) the security key in this window. Close all windows.

Work with your wired NIC.
We will now verify the wired network connection settings.

Step 14: Open the Network Connections window by right-clicking Windows Start > Network Connections.
Step 15: Select and right-click the Local Area Connection option to display the drop-down list. If the NIC is disabled, enable it.
[image: ]

Step 16: Click the Status option to open the Local Area Connection Status window. This window displays information about your wired connection to the LAN.
[image: ]

Step 17: Click Details… to view the address information for your LAN connection.
[image: ]

Step 18: Open a command window prompt and type ipconfig /all. Find your Local Area Connection information and compare this with the information displayed in the Network Connection Details window.
[image: ]

Step 19: Close all windows on your desktop.

Identify and Use the System Tray Network Icons

Use the Wireless Network icon.
Step 20: The bottom right-hand corner of the Windows 10 screen contains the system tray. Move your mouse to display the system tray as shown.
[image: ]

Note: If your wired network is enabled, a different network icon ([image: ]) is displayed in the system tray.

[image: ]Step 21: In this example, the 3rd icon from the left is the wireless network icon. If you hover over it, it displays the currently connected networks.
Step 22: Click the wireless network icon, and it displays the wired and wireless network SSIDs that are in range of your wireless NIC.
[image: ]

[image: ]Step 23: Right-click the wireless network icon, and it displays a troubleshooting option and to open the Network and Sharing Center window.
Step 24: Click on the Open Network and Sharing Center option.
[image: ]

Step 25: The Network and Sharing Center is a central window that displays information about the active network or networks, the network type, the type of access.

Record your Reflection:
Why would you activate more than one NIC on a PC?
           You could activate more than one NIC for a couple reasons the main being that if a NIC fails it could break an important connection, with a second NIC you could continue as normal until repairs can take place, another reason could be to separate traffic to improve speeds.


Task 4: Address Resolution Protocol (ARP).
[bookmark: Use_your_PC/_Laptop_with_Internet_Connec][bookmark: Objectives]Use your PC/ Laptop with Internet Connection to execute this Task. Objectives
Download and Install Wireshark
Capture and Analyze ARP Data in Wireshark
· Start and stop data capture of ping traffic to remote hosts.
· Locate the IPv4 and MAC address information in captured PDUs.
· Analyze the content of the ARP messages exchanged between devices on the LAN.
View the ARP cache entries on the PC
· Access the Windows Command Prompt.
· Use the Windows arp command to view the local ARP table cache on the PC.

[bookmark: Background_/_Scenario]Background / Scenario
Address Resolution Protocol (ARP) is used by TCP/IP to map a Layer 3 IPv4 address to a Layer 2 MAC address. When an Ethernet frame is transmitted on the network, it must have a destination MAC address. To dynamically discover the MAC address of a known destination, the source device broadcasts an ARP request on the local network. The device that is configured with the destination IPv4 address responds to the request with an ARP reply and the MAC address is recorded in the ARP cache.
Every device on the LAN maintains its own ARP cache. The ARP cache is a small area in RAM that holds the ARP responses. Viewing an ARP cache on a PC displays the IPv4 address and the MAC address of each device on the LAN with which the PC has exchanged ARP messages.
Wireshark is a software protocol analyzer, or "packet sniffer" application, used for network troubleshooting, analysis, software and protocol development, and education. As data streams travel back and forth over the network, the sniffer "captures" each protocol data unit (PDU) and can decode and analyze its content according to the appropriate protocol specifications.
Wireshark is a useful tool for anyone working with networks and can be used with most labs in the Cisco courses for data analysis and troubleshooting. This lab provides instructions for downloading and installing Wireshark, although it may already be installed. In this lab, you will use Wireshark to capture ARP exchanges on the local network.

Required Resources
· 1 Windows 10 PC with Internet access

Download and Install Wireshark
Wireshark has become the industry standard packet-sniffer program used by network engineers. This open source software is available for many different operating systems, including Windows, Mac, and Linux.
If Wireshark is already installed on your PC, you can skip Part 1 and go directly to Part 2. If Wireshark is not installed on your PC, check with your instructor about your academy’s software download policy.

[bookmark: Step_26:_Download_Wireshark.]Step 26:  Download Wireshark.
a. Wireshark can be downloaded from www.wireshark.org.
b. Click Download.
[image: ]

c. Choose the software version you need based on your PC’s architecture and operating system. For instance, if you have a 64-bit PC running Windows, choose Windows Installer (64-bit).
[image: ]
d. After making a selection, the download should start. Click Save File if prompted. The location of the downloaded file depends on the browser and operating

system that you use. For Windows users, the default location is the Downloads
folder.

[bookmark: Step_27:_Install_Wireshark.]Step 27: Install Wireshark.
e. The downloaded file is named Wireshark-win64-x.x.x.exe, where x represents the version number. Double-click the file to start the installation process. It is version 2.0.5 in this example.
f. Respond to any security messages that may display on your screen. If you already have a copy of Wireshark on your PC, you will be prompted to uninstall the old version before installing the new version. It is recommended that you remove the old version of Wireshark prior to installing another version. Click Yes to uninstall the previous version of Wireshark.
[image: ]

g. If this is the first time to install Wireshark, or after you have completed the uninstall process, you will navigate to the Wireshark Setup wizard. Click Next.
[image: ]
h. Continue advancing through the installation process. Click I Agree when the License Agreement window displays.
i. Keep the default settings on the Choose Components window and click Next.

j. Choose your desired shortcut options and click Next.

.[image: ]
k. You can change the installation location of Wireshark, but unless you have limited disk space, it is recommended that you keep the default location.
[image: ]
l. To capture live network data, WinPcap must be installed on your PC. If WinPcap is already installed on your PC, the Install check box will be unchecked. If your installed version of WinPcap is older than the version that comes with Wireshark, it is recommend that you allow the newer version to be installed by clicking the Install WinPcap x.x.x (version number) check box.

Finish the WinPcap Setup Wizard if installing WinPcap.
[image: ]
Note: You maybe prompted to install USBPcap. The installation of USBPcap is optional.
m. Wireshark starts installing its files and a separate window displays with the status of the installation. Click Next when the installation is complete.
[image: ]

n. Click Finish to complete the Wireshark install process.
[image: ]


Capture and Analyze Local ARP Data in Wireshark

You will ping another PC on the LAN and capture ARP requests and replies in Wireshark. You will also look inside the frames captured for specific information. This analysis should help to clarify how packet headers are used to transport data to their destination.

Step 28: Retrieve your PC’s interface addresses.
For this lab, you will need to retrieve your PC’s IPv4 address and the MAC address.
o. Open a command window, type ipconfig /all, and then press Enter.

p. Note which network adapter that the PC is using to access the network. Record your PC interface’s IPv4 address and MAC address (Physical Address).
[image: ]
Step 29: Start Wireshark and begin capturing data.

q. On your PC, click Start and type Wireshark. Click  Wireshark Desktop App
when it appears in the search results window.
Note: Alternatively, your installation of Wireshark may also provide a Wireshark Legacy option. This displays Wireshark in the older but widely recognized GUI. The remainder of this lab was completed using the newer Desktop App GUI.
r. After Wireshark starts, select the network interface that you identified with  the
ipconfig command. Enter	arp  in  the  filter  box. This  selection  configures

Wireshark to only display packets that are part of the ARP exchanges between the devices on the local network.
[image: ]

s. After you have selected the correct interface and entered the filter information, click Start ([image: ]) to begin the data capture. Information will start scrolling down the top section in Wireshark. Each line represents a message being sent between a source and destination device on the network.
[image: ]

t. Open a command prompt window. Use the ping command to test connectivity to the default gateway address that you identified in Part 2, step 1c.
[image: ]

u. Stop capturing data by clicking Stop Capture ([image: ]) on the toolbar.
[bookmark: Step_30:_Examine_the_captured_data.]Step 30: Examine the captured data.
In Step 3, examine the data that was generated by the ping requests, Wireshark data is displayed in three sections:
1) The top section displays the list of PDU frames captured with a summary of the IPv4 packet information listed.
2) The middle section lists PDU information for the frame selected in the top part of the screen and separates a captured PDU frame by its protocol layers.
3) The bottom section displays the raw data of each layer. The raw data is displayed in both hexadecimal and decimal form.
[image: ]

a. Click one of the ARP frames in the top section that has your PC MAC address as the source address in the frame and “broadcast” as the destination of the frame.
b. With this PDU frame still selected in the top section, navigate to the middle section. Click the arrow to the left of the Ethernet II row to view the Destination and Source MAC addresses.
[image: ]

Does	the	Source	MAC	address	match	your	PC’s	interface?



c. Click the arrow to the left of the Address Resolution Protocol (request) row to view the content of the ARP request.
[image: ]

[bookmark: Step_31:_View_ARP_cache_entries_on_a_Win]Step 31: View ARP cache entries on a Windows PC.
a. Open a command prompt window on the PC. At the prompt, enter arp –a and press enter.
[image: ]

The output of the arp –a command displays the entries that are in the cache on the PC. In the example, the PC has entries for the default gateway (192.168.1.1) and for two PCs that are located on the same LAN (192.168.1.9 and 192.168.1.13).
What is the result of executing the arp –a command on your PC?


b. The arp command on the Windows PC has another functionality. Enter arp /? at the command prompt and press enter. The arp command options enable you to view, add and remove ARP table entries if necessary.
[image: ]

Which option deletes an entry from the ARP cache?
                                 Arp /d inetaddr
What would be the result of issuing the arp –d * command?
                                 Arp-d deletes the entire entries and cache


[bookmark: Record_your_Reflection]Record your Reflection
1. What is a benefit of keeping ARP cache entries in memory on the source computer?
The benefit of keeping the ARP cache entries in the memory of the source computer is that; it saves time on your pc trying to work out what IP address matches which MAC address due to it already knowing because its saved on the pc.



2. If the destination IPv4 address is not located on the same network as the source host, what MAC address will be used as the destination target MAC address in the frame?
the MAC address used will be the default gateway MAC address, due to the internet control message protocol (ICMP) using it automatically.










Learnings from this lab:

· Build a Simple Network
· Configure the IP Address
· Use Ping/ Trace route Utility to check the connection status
· Use ipconfig /all command to determine the MAC address of a Windows computer on an Ethernet network.
· Analyze a MAC address to determine the manufacturer.
· Analyze the Wired and Wireless Network connection.
· Analyze Address Resolution Protocol (ARP).
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More downloads and documentation can be found on the do ads
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Wireshark 20.5 (64-bit) Setup

Wireshark 20.2 (64-bit)is already installed.

Would you like to uninstall it first?

No Cancel
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Welcome to the Wireshark 2.0.5
(64-bit) Setup Wizard

This wizard wil quide you through the instalation of
Wiireshark.

Before starting the intallation, make sure Wreshark s not
runring.

Clck Next to continue.

> Cancel
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M Wireshark 2.0.5 (64-bit) Setup. -

Select Additional Tasks
Wihich additonsl tasks shouid be done?

Create Shorteuts
Sishark StarE Mien T

[ wireshark Desktop fcon
Viireshark Quick Launch Lcon
Viresherk Legacy Start Menu Ttem
[ wireshark Legacy Desktop Icon
Vireshark Legacy Quick Launch Icon

File Extensions.
(@ Associate trace file extensions to Wireshark

(O Associate trace fle extensions to Wireshark Legacy.
ONone

Extensions: 5vw, acp, 3pc, atc bfr, cap, enc, ef, fdc, out, peap,
peapng, pkt, rf5, snoop, SYc, tp, 1l trace, tr, v, wpc, wpz.

Wireshark Instalr (tm)

X
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Install WinPcap?
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X
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Wireshark 2.0.5 (64bt) has been installed on your
computer.

Clck Finsh to dose ths wizard.

[Run Wireshark 2.0.5 (645)
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Command Prompt

Connection-specific DNS Suffix

Wireless LAN adapter Wireless Network Connection:

Link-local IPv6 Address

Description Intel(R) Centrino(R) Advanced-N 6205
Physical Address. : A4-4E-31-AD-78-4C

"DHCP Enabled. i . T Yes

Autoconfiguration Enabled . : Yes

: fe80::f9e7:e41d:a772:f993%11(Preferred)

IPv4 Address.
Subnet Mask .
Lease Obtained.
Lease Expires
Default Gateway
DHCP Server

192.168.1.8(Preferred)

255.255.255.@

Thursday, August @4, 2016 5:35:35 PM
Friday, August @5, 2016 5:35:35 PM
192.168.1.1

192.168.1.1

DHCPv6 IAID . . .
DHCPv6 Client DUID
DNS Servers ..
NetBIOS over Tcplp

245648945

: ©0-01-00-01-1B-87-BF-52-A4-4E-31-AD-78-4C

192.168.1.1

: Disabled
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M The Wireshark Network Analyzer - o X
Ele Edt View Go Captue Analyze Statistics Telephony Wireless Tools Help

dmze nmpRERes=FsEEHaaas

Taey 2 dsplay fiter .. <Ciif> 3 -] oression...

Capture
-using s fter:

Wireless Network Connection SV SN Y N—
Bluetooth Network Connection 6

Learn
You are runring Wireshark 2.0.5 (v2.0.5-0-ga3be9c from master-2.0). You receive automatic updates.

P — || Nopackets || profie: Defat
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£ Capturing from Wireless Network Connection (arp) - o X
Ele Edit View Go Capture Analyze Statistics Telephony Wireless Tools Help

.6 RERe=s=FaEaaaH
(Mool 2 dislay fter_<cury> 3 ) Bpresson... +
o  Tme Protocol _Length_1nfo G
1 6.000000 e 60 Who has 192.168.1.17 Tell 192.168.1.3
21,2678 e 60 Who has 192.168.1.17 Tell 192.168.1.3
3 1ls76205 e 60 uho has 192.168.1.17 Tell 192.168.1.3 v

> Frame 1: 60 bytes on wire (480 bits), 60 bytes captured (480 bits) on interface @
> Ethernet II, Src: Microchi_32:b7:3d (00:04:23:32:b7:3d), Dst: Broadcast (Ff:ff:ff:ff:ff:ff)
> Address Resolution Protocol (request)

oo FF FF FF FF FF FF 00 04 a3 32 b7 3d 06 06 00 01
0010 @8 00 06 04 00 01 00 04 a3 32 b7 3d c a8 01 03
0020 FF FF FF FF FF FF co a8 01 01 00 00 00 00 00 00
0030 00 00 00 00 00 00 00 00 00 00 00 00

@ 7 Wireless Network Connection: <ive capture in progress> || Packets: 23 - Displayed: 23 (100.0%) || Profie: Default
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Command Prompt

\Users>ping 192.168.1.1

Pinging 192.165.1.1 with 32 bytes of data
Reply from 192.168.1.1: bytes=32 time=Ims
Reply from 192.168.1.1

Reply from 192.168.1.1
Reply from 192.168.1.1

Ping statistics for 192.168.1.1

Packets: Sent = 4, Received = 4, Lost = @ (0% loss),
ppproximate round trip times in milli-seconds

Minimum = Ins, Maximum = 4ns, Average = 2ms
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M "Wireless Network Connection (arp) - o x
File Edit View Go Capture Analyze Statistics Telephony Wireless Tools Help

dmceimmB Re==FssEaaan

(N Tacely a display fiter . <ctri/> 3 -] Expresson +

No.  Tme Source. Destration Protocl  Length  Info A

2 1.265714 Microchi_32:|

+3d Broadcast ARP 60 Who has 192.168.1.12 Tell 192.168.1.3

31.9%6225  Microchi_32 Eroadcast P 60 Who has 192.168.1.12 Tell 192.168.1.3 ivi
42.639866  Microchi_32: Broadcast are 60 Who has 192.168.1.12 Tell 192.165.1.3 individual PDUs )
~ Frame 1: 60 bytes on wire (480 bits), 60 bytes ceptured (480 bits) on interface @ ~

Interface id: @ (\Device\NPF_{4DD27686-1E37-4F0A-BOGA-ECBE22032990})
Encapsulation type: Ethernet (1)

Arrival Time: Aug 4, 2016 19:13:58.548592008 US Mountain Standard Time i + H

[Time shift for this packet: ©.000000060 seconds] Middle section displays
Epoch Time: 1476363238.648592000 seconds the detailsabout the
[Time delta from previous captured frame: ©.000000800 seconds] fe

[Tine delta from previous displayed frame: 0.866000008 seconds] highlighted PDU

[Tine since reference or first frame: ©.000000600 seconds]
Frame Number: 1

Frame Length: 60 bytes (488 bits)

Capture Length: 60 bytes (488 bits) v

oeon  ff FF £f £f ff £f 00 64 a3 32 b7 3d €8 06 00 €1 i i
0010 08 90 €6 04 Pe o1 84 a3 32 b7 3d c@ a8 @1 @3 Bonom SECtIDn dlsplays
the raw data

00
2020 ff FF £f £f £f £f cO a8 01 01 00 00 GO 00 20 GO
0030 00 00 €0 00 00 00 00 00 00 0O 00 00

@ 7 wireshark_pcepng_4DD27686-1E37-40A-B06AE6BE22032950_20160804191357_a14032 || Packets: 82 - Displayed: 82 (100.0%) | Profie: Default
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M “Wireless Network Connection (arp) - [m] x
File Edit View Go Capture Analze Statistics Telephony Wireless Tooks Help

A m 7 Qaaan

(N Tacey 2 deplay iter .. <cini> - - 3 -] Bpresson.. +

Source Destination Protocol  Length  Info
Microch: Broadcast

12 8.9303 IntelCor ad:78. 42 19.

> Frame 11: 82 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface @
~ Ethernet II, Src: IntelCor_ad:78:4c (ad:4e:31:ad:78:4c), Dst: Broadcast (Ff:ff:ff:ff:ff:ff)

> Destination: Broadcast (FF:ffiffiffiffiff) : . .
> Source: IntelCor_ad:78:4c (ad:de:31:ad:78:4c) : This section displays the
Tpel AP (ebne) information contained in

> Address Resolution Protocol (request) the Layer 2 framie hesder

@ 7 Frame (frame), 42bytes || Packets: 82 - Displayed: 82(100.0%) || Profie: Defauit
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M “Wireless Network Connection (arp) - a 5.3
File Edit View Go Capture Analyze Statistics Telephony Wireless Tools Help
A9 IRRB R=»=FssEaaan

Apply a display fiter ... <Ctrl-f> = -] Expression..

Time Source Destination Protocl  Length  Info

10 7.811031 Microchi_32:b7:3d Broadcast ARP 60 Who has 192.168.1.1? Tell 192.168.1.3

11 8.921443 IntelCor_ad:78:4c Broadcast ARP 42 Who has 192.168.1.9? Tell 192.168.1.8

12 8.930365 HonHaiPr be:15:63 IntelCor ad:78.. ARP 42 192.168.1.9 is at 90:4c:eS:be:15:63

Hardware type: Ethernet (1)

Protocol type: IPvé (@x0300)

Hardware size: 6

Protocol size: 4

Opcode: request (1)

Sender MAC address: IntelCor_ad:78:4c (a4:4e:31:ad:78:4c)
Sender IP address: 192.168.1.5

Target MAC address: 00:00:00_00:00:00 (00:00:00:00:00:00)
Target IP address: 192.168.1.9

> Frame 11: 42 bytes on wire (336 bits), 42 bytes captured (336 bits) on interface 0
> Ethernet II, Src: IntelCor ad:78:4c (ad:de:31:ad:78:4c), Dst: Broadcast (ff:ff:ff:ff:ff:ff)
v Address Resolution Protocol (request)

This ARP request is looking for
the MAC address associated
with the IP address 192.168.1.9.

@

7 Frame (frame), 42 bytes

|| Packets: 82 - Displayed: 82(100.0%) || Profle: Defauit
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Command Prompt

\arp -

Interface: 192.165.1.5 -
Internet Address
192.168.1.1
192.165.1.9
192.165.1.13
224.0.0.5
224.0.0.6
224.0.0.22
224.0.0.252
224.0.0.253
239.255.255.250
255.255.255.255

>

oxb
Physical Address
80-37-73-ca-b1-7a
90-4c-25-be-15-63
e
01-00-52-00-00-05
01-00-52-00-00-06
01-00-52-00-00-15
01-00-52-00-00-Fc
01-00-52-00-00-7d
01-00-52-7¢-FF-Fa
P

Type
dynamic
dynamic
dynamic
static
static
static
static
static
static
static
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Command Prompt

\sarp /2

eth_addr
if_addr

Example

> arp -a

> arp -s 157.55.85.212  00-3a-00-62-C6-09 .

isplays and modifies the IP-to-Physical address translation tables used by
address resolution protocol (ARP).

RP -5 inet_addr eth_addr [if_addr]
RP -d inet_addr [if addr]
RP -a [inet_addr] [-N if_addr] [-v]

Displays current ARP entries by interrogating the current
protocol data. If inet_addr is specified, the IP and Physical
addresses for only the specified computer are displayed. If
more than one network interface uses ARP, entries for each ARP
table are displayed.

Same as -a.

Displays current ARP entries in verbose mode. All invalid
entries and entries on the loop-back interface will be shown.
Specifies an internet address.

Displays the ARP entries for the network interface specified
by if_addr.

Deletes the host specified by inet_addr. inet_addr may be
wildcarded with * to delete all hosts.

Adds the host and associates the Internet address inet_addr
with the Physical address eth_addr. The Physical address is
given as 6 hexadecimal bytes separated by hyphens. The entry
is permanent.

Specifies a physical address.

If present, this specifies the Internet address of the
interface whose address translation table should be modified.
If not present, the first applicable interface will be used.

Adds a static entry.
Displays the arp table.
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