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Activity Results

You did not complete the activity. Please close this window and try again.

Overall Feedback Assessment ltems Connectivity Tests
N

Time Elapsed: 02:36:51

Expand/Collapse All ' Show Incorrect Items Score :61/100
Item Count :61/96
Assessment ltems Status Points Component(s) Feedback -
—}- Network Component Items/Total Score
—|- Ha1: DHCP 0 Other Ip 22/29 22/29
- PonIs:astEthernetO g 8:22; Other 10721 10721
@ DHCP client enable Correct 1 Ip Physl|cal 10/14 10/14
Z|. Ha2: DHCP 0 Other Routing 16/21 16/21
—]. Ports 0 Other Switching 3/5 3/5
—|- FastEthernet0 0 Other fr
& DHCP client enable Correct 1 Ip
-]+ He1: 192.168.1.11/24 0 Other
—|- Ports 0 Other
—|- FastEthernet0 0 Other
& |P Address Correct 1 Ip
—J- Hc2: DHCP 0 Other
—|- Ports 0 Other
—|- FastEthernet0 0 Other
& DHCP client enable Correct 1 Ip
- Ra1
X Banner MOTD Incorrect 1 Other
—|- Console Line 0 Other
& Logging Synch Correct 1 Physical
—|- DHCP Server
—|- Excluded Addresses
X 10.67.1.110.67.1.10 Incorrect 1 Ip
X 192.168.10.1 192.168.10.10 Incorrect 1 Ip
—|- Pools
—|- Pool C2
X Default Gateway Incorrect 1 Ip
X Name Incorrect 1 Ip
—|- Pool Mid
X DNS server IP Incorrect 1 Ip
X Subnet mask Incorrect 1 Ip
—}- Pool Top 0 Ip
X Network Address Incorrect 1 Ip
X IP Domain Name Incorrect 1 Other
—|- Ports
—}- GigabitEthernet0/0/0 0 Other j
W  Dnrt Qtahie Inrarrant 1 Dhuciral
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(B2 PT Activity: 02:38:25

e Router Id for Rcl with 1.1.1.1 and Rc2 with 5.5.5.5

¢ Configure appropriate interfaces as passive.

¢ Configure the reference bandwidth to 1Gigabit.

¢ Configure the network statement for each locally attached networks using a wild card mask
matching the network’s subnet mask.

16. Configure DHCP relay (IP - Helper address) at the appropriate Interface enabling Hc2 for DHCP
Configuration.

17. Configure Hcl with appropriate IP address, subnet mask and default gateway as per the
addressing table.

18. Test your configuration (Before ACL) Answer this question in a Word Document with a screenshot
of Evidence.

Time Elapsed: 02:38:25
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