	Activity to be Assessed
	Assessment Number

	Working under overhead power cables.
	0021

	Persons undertaking or affected by the activity

	

	
	x
	Employees
	x
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Going to close to the live wire and a Site operative being electrocuted. 
	3
	5
	15

	2
	Heavy Machinery and plant encountering the overhead power line.
	3
	5
	15

	3
	The overhead power line collapsing on the site.
	2
	4
	8

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	Existing Control Measures / Additional Control Measures Required

	1
	Maintaining the minimum distance required from the lines, this includes all operatives and plant. If unavoidable request temporary diversion of power. A competent person should measure the distance to ensure it is safe. Onsite training given to all operatives who require it.

	2
	All machinery coming onto site must be suitable to this specific site. It must always comply with the overhead distances. If machinery that doesn’t comply with the minimum height requirements must be used onsite, it is the duty of the Site Manager to ensure the overhead power line is switched off whilst the machinery is in use. If a driver makes contact with a power line they are to stay in the seat until an expert has deemed it safe for him to get out.

	3
	All excavations are to ensure they do not affect and structure already in place. The Site Manager is to liaise with the Network Operator, confirming all plans coincide with the work happening on the ground.
Health and Safety officer on site will receive extra training on electrical burns. All higher risk activity will require the Site Manager to inform the local Accident and Emergency for standby.

	4
	

	5
	

	6
	

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Going to close to the live wire and a Site operative being electrocuted.
	1
	5
	5

	2
	Heavy Machinery and plant encountering the overhead power line.
	2
	5
	10R

	3
	The overhead power line collapsing on the site.
	1
	4
	4

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	Name  Sean Leach
Position  
	Signed
S.Leach

	   Date of Completion: 
22/10/2020

	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury

	Reviewed by:
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk



