Assignment Task 2 – Virtualisation & Networking (Screenshot Guide)
2.2.1 Evidence of Download and Installation
- Creation of Virtual Machine Windows 1 
- Creation of Virtual Machine Debian 1 
- Installation of Windows OS – Screenshot of Desktop.
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2.2.2 Deploy Network as per the Given Topology
- Creation of NAT Network 1 for Windows 
- Evidence Windows PC 1 Connected to NAT Network 1 
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2.2.3 IP Addressing
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- Windows Machine 1 – ipconfig Output 
- Windows Machine 2 – ipconfig Output 
- Network Address for NAT Network 1 (Windows)
2.4 Test and Troubleshoot
- Successful Ping: Windows → Windows (Ping 192.168.100.10 and 192.168.100.20)
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