
Building configuration...
[OK]
S1#
S1#
S1#
S1#
S1#
S1#show run
Building configuration...

Current configuration : 1802 bytes
!
! Last configuration change at 12:02:43 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
interface Vlan7
 description London
 ip address 192.168.20.1 255.255.255.0
!
interface Vlan8
 description Swansea
 ip address 192.168.30.1 255.255.255.0
!
interface Vlan9
 description Management
 ip address 192.168.40.3 255.255.255.0
!
ip http server
ip http secure-server
!
!
!
banner motd ^Cswre-lab.com^C
!
line con 0
line vty 5 15
!
end

S1#show ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan7                  192.168.20.1    YES manual down                  down
Vlan8                  192.168.30.1    YES manual down                  down
Vlan9                  192.168.40.3    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S1#





Building configuration...
[OK]
S1#
S1#
S1#
S1#
S1#
S1#show run
Building configuration...

Current configuration : 1802 bytes
!
! Last configuration change at 12:02:43 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
interface Vlan7
 description London
 ip address 192.168.20.1 255.255.255.0
!
interface Vlan8
 description Swansea
 ip address 192.168.30.1 255.255.255.0
!
interface Vlan9
 description Management
 ip address 192.168.40.3 255.255.255.0
!
ip http server
ip http secure-server
!
!
!
banner motd ^Cswre-lab.com^C
!
line con 0
line vty 5 15
!
end

S1#show ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan7                  192.168.20.1    YES manual down                  down
Vlan8                  192.168.30.1    YES manual down                  down
Vlan9                  192.168.40.3    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S1#swre-lab.com
R1>
R1>
R1>show run
         ^
% Invalid input detected at '^' marker.

R1>en
R1#show run
Building configuration...

Current configuration : 6303 bytes
!
! Last configuration change at 11:57:05 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
no ip domain lookup
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-3237628287
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3237628287
 revocation-check none
 rsakeypair TP-self-signed-3237628287
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-3237628287
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33323337 36323832 3837301E 170D3234 30383231 30373335
  32375A17 0D333430 38323130 37333532 375A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 32333736
  32383238 37308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100AADF CF36CEE4 896B0230 16CDC623 C6AF8D4B 9944BCD0 F0236EE3
  2C305BAF EB658F3D 61FE19B2 2D9282AE AF459535 0F4A1381 92456074 714EC7A6
  E2EEE476 9BED6F1F F7FC735D F8D33367 DDEA315F 0D9CCB82 9C1FC12D 23FDE9CE
  839C3FC0 47278C36 7C49E25B 38D49F39 1D360321 B359E016 32765E3C 55EB8ACF
  FD34C29C AE6441DF 6D898C18 26DEC731 E3688764 3064CD32 B5F6C983 3BA82D0B
  568463CF 4D3410F8 E15462C7 BB4E0144 984EDCB7 2CA05BAB D4C121C2 84343C24
  45189B05 379BC37A AB012584 9C20E0AC 4594B3BD 28645D73 81F64817 A4EF1506
  91086342 B76C68F0 69B7D5D1 199AEE40 FD158564 E0C7CE34 D2AC9347 AF0066DB
  8F41518E 26590203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 143E93A1 594864CC B487B66C B014C7D7 A4AB71AB
  4B301D06 03551D0E 04160414 3E93A159 4864CCB4 87B66CB0 14C7D7A4 AB71AB4B
  300D0609 2A864886 F70D0101 05050003 82010100 5A93F94F 84643AE7 704FE25A
  31D15220 83E08E50 E9FA0E94 5C204094 DA6B03CA 3329183C DC6D240B C52A6A28
  6B9DD5DF 1B8A1985 14137F3A 02974C7C DFA8B0E6 EC7254A0 D11D99FD 9FC67CA7
  3E23938B 50509E6F 909BACE3 0AAEA0FB 4E662D5D E2329C3B FBC7F4B7 3FE1A4E2
  487957B2 09338F92 63FE2E19 DDD3AECB AE776F10 F84DDAD8 623023CA 3936537A
  AED6459E D556B830 D8BF247B 208DA5E3 F6E9A5B6 50529AC3 E49BEDA4 8A84FAD6
  23105E3F 75418EC2 71D47CD9 AEB11DBD 972F3EE7 2D66CEDD F8C0D898 2C1CF0C4
  536F2315 B5FF7CC8 2BE08F75 850FFD43 181188DD 9E0770DF C54C2491 5206CA1D
  C4BC472D 58498B8F FEFF49BF 86249EB0 9FF829CD
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0PF
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1.7
 encapsulation dot1Q 7
 ip address 192.168.20.1 255.255.255.0
!
interface GigabitEthernet0/0/1.8
 encapsulation dot1Q 8
 ip address 192.168.30.1 255.255.255.0
!
interface GigabitEthernet0/0/1.9
 encapsulation dot1Q 9
 ip address 192.168.40.1 255.255.255.0
!
interface GigabitEthernet0/0/1.11
 encapsulation dot1Q 11
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
banner motd ^Cswre-lab.com^C
!
line con 0
 stopbits 1
line aux 0
line vty 0 4
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

R1#show ip config
             ^
% Invalid input detected at '^' marker.

R1#show ip interface bri
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/1   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/1.7 192.168.20.1    YES manual administratively down down
GigabitEthernet0/0/1.8 192.168.30.1    YES manual administratively down down
GigabitEthernet0/0/1.9 192.168.40.1    YES manual administratively down down
Gi0/0/1.11             unassigned      YES unset  administratively down down
GigabitEthernet0/0/2   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/3   unassigned      YES NVRAM  administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
R1#








Building configuration...
[OK]
S1#
S1#
S1#
S1#
S1#
S1#show run
Building configuration...

Current configuration : 1802 bytes
!
! Last configuration change at 12:02:43 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
interface Vlan7
 description London
 ip address 192.168.20.1 255.255.255.0
!
interface Vlan8
 description Swansea
 ip address 192.168.30.1 255.255.255.0
!
interface Vlan9
 description Management
 ip address 192.168.40.3 255.255.255.0
!
ip http server
ip http secure-server
!
!
!
banner motd ^Cswre-lab.com^C
!
line con 0
line vty 5 15
!
end

S1#show ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan7                  192.168.20.1    YES manual down                  down
Vlan8                  192.168.30.1    YES manual down                  down
Vlan9                  192.168.40.3    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S1#swre-lab.com
R1>
R1>
R1>show run
         ^
% Invalid input detected at '^' marker.

R1>en
R1#show run
Building configuration...

Current configuration : 6303 bytes
!
! Last configuration change at 11:57:05 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
no ip domain lookup
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-3237628287
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3237628287
 revocation-check none
 rsakeypair TP-self-signed-3237628287
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-3237628287
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33323337 36323832 3837301E 170D3234 30383231 30373335
  32375A17 0D333430 38323130 37333532 375A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 32333736
  32383238 37308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100AADF CF36CEE4 896B0230 16CDC623 C6AF8D4B 9944BCD0 F0236EE3
  2C305BAF EB658F3D 61FE19B2 2D9282AE AF459535 0F4A1381 92456074 714EC7A6
  E2EEE476 9BED6F1F F7FC735D F8D33367 DDEA315F 0D9CCB82 9C1FC12D 23FDE9CE
  839C3FC0 47278C36 7C49E25B 38D49F39 1D360321 B359E016 32765E3C 55EB8ACF
  FD34C29C AE6441DF 6D898C18 26DEC731 E3688764 3064CD32 B5F6C983 3BA82D0B
  568463CF 4D3410F8 E15462C7 BB4E0144 984EDCB7 2CA05BAB D4C121C2 84343C24
  45189B05 379BC37A AB012584 9C20E0AC 4594B3BD 28645D73 81F64817 A4EF1506
  91086342 B76C68F0 69B7D5D1 199AEE40 FD158564 E0C7CE34 D2AC9347 AF0066DB
  8F41518E 26590203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 143E93A1 594864CC B487B66C B014C7D7 A4AB71AB
  4B301D06 03551D0E 04160414 3E93A159 4864CCB4 87B66CB0 14C7D7A4 AB71AB4B
  300D0609 2A864886 F70D0101 05050003 82010100 5A93F94F 84643AE7 704FE25A
  31D15220 83E08E50 E9FA0E94 5C204094 DA6B03CA 3329183C DC6D240B C52A6A28
  6B9DD5DF 1B8A1985 14137F3A 02974C7C DFA8B0E6 EC7254A0 D11D99FD 9FC67CA7
  3E23938B 50509E6F 909BACE3 0AAEA0FB 4E662D5D E2329C3B FBC7F4B7 3FE1A4E2
  487957B2 09338F92 63FE2E19 DDD3AECB AE776F10 F84DDAD8 623023CA 3936537A
  AED6459E D556B830 D8BF247B 208DA5E3 F6E9A5B6 50529AC3 E49BEDA4 8A84FAD6
  23105E3F 75418EC2 71D47CD9 AEB11DBD 972F3EE7 2D66CEDD F8C0D898 2C1CF0C4
  536F2315 B5FF7CC8 2BE08F75 850FFD43 181188DD 9E0770DF C54C2491 5206CA1D
  C4BC472D 58498B8F FEFF49BF 86249EB0 9FF829CD
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0PF
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1.7
 encapsulation dot1Q 7
 ip address 192.168.20.1 255.255.255.0
!
interface GigabitEthernet0/0/1.8
 encapsulation dot1Q 8
 ip address 192.168.30.1 255.255.255.0
!
interface GigabitEthernet0/0/1.9
 encapsulation dot1Q 9
 ip address 192.168.40.1 255.255.255.0
!
interface GigabitEthernet0/0/1.11
 encapsulation dot1Q 11
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
banner motd ^Cswre-lab.com^C
!
line con 0
 stopbits 1
line aux 0
line vty 0 4
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

R1#show ip config
             ^
% Invalid input detected at '^' marker.

R1#show ip interface bri
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/1   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/1.7 192.168.20.1    YES manual administratively down down
GigabitEthernet0/0/1.8 192.168.30.1    YES manual administratively down down
GigabitEthernet0/0/1.9 192.168.40.1    YES manual administratively down down
Gi0/0/1.11             unassigned      YES unset  administratively down down
GigabitEthernet0/0/2   unassigned      YES NVRAM  administratively down down
GigabitEthernet0/0/3   unassigned      YES NVRAM  administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
R1#
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>
S2>en
S2#show ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan9                  192.168.40.3    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S2#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
2    VLAN0002                         active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
2    enet  100002     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

S2#show login
     No login delay has been applied.
     No Quiet-Mode access list has been configured.

     Router NOT enabled to watch for login Attacks

S2#show run
Building configuration...

Current configuration : 1618 bytes
!
! Last configuration change at 14:36:46 UTC Wed Apr 4 2035
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
interface Vlan9
 description Management
 ip address 192.168.40.3 255.255.255.0
!
ip http server
ip http secure-server
!
!
!
!
line con 0
line vty 5 15
!
end

S2#show ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan9                  192.168.40.3    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S2#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
2    VLAN0002                         active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
2    enet  100002     1500  -      -      -        -    -        0      0
 --More—


