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Figure 1: Network Routing and IP Address configuration
(Source: Self-created)
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Figure 2: Active Directory Domain Services Configuration
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Figure 3: DNS Configuration
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Figure 4: DHCP Configuration
(Source: Self-created)
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Figure 5: RRAS Configuration
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Figure 6: User Account Management
(Source: Self-created)
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Figure 7: Shared Storage
(Source: Self-created)
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Figure 8: Web Services
(Source: Self-created)
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Figure 9: Remote Desktop Services
(Source: Self-created)
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Jroot@localadmin:™# ip addr
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Link/ether 08:00:27:29:49:b6 brd ff:f:ff:ff:ffiff
inet 192.168.20.10/24 scope global enposs
valid_lft forever preferred_lft forever
ineté feso::a00:27ff:fe29:43b6/64 scope link
valid_lft forever preferred_lft forever





image4.png
ip addr
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc nogueue state UNKNOWN group default qlen 1000
Link/loopback 00:00:00:00:00:00 brd 00: :00:00:00
inet 127.0.9.1/8 scope host lo
valid_Lft forever preferred_Lft forever
inet6 ::1/128 scope host noprefixroute
valid_1ft forever preferred_Lft forever
ethd: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default glen 1000
Link/ether 08:00:27:5a:! brd fF:Ff:FF:FFFFFF
inet 10.0.2.15/24 brd 10.0.2.255 scope global dynamic noprefixroute etho
valid_1ft 86020sec preferred_lft 86020sec
inet6 fd17:625¢c:£037:2:f13:19dd:48d8:c535/64 scope global dynamic noprefixroute
valid_lft 86322sec preferred_lft 14322sec
inet6 fed0::2f00:7e1d:73cf:lebe/64 scope link noprefixroute
valid_lft forever preferred_Lft forever
3: ethl: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1
link/ether 08:00:27:d7:70:d2 brd ff:ff:ff:ff:Ff:ff
20/24 scope global ethl
valid_1ft forever preferred_Lft forever
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